-*- text -*-
***************************
CDMA2000 V5.20
***************************

Date:	November 2, 2010

Base:	V5.20
MMI:	2.99T
LH:	V2.88L	V12
	X3.26d	V22

General Remarks
===============

	This release of CDMA2000 software is based on the CMU base system V5.20 and
	can be installed together with other V5.20 compatible function groups.

	This version is the same as version 5x20.I06, but with a new base


Known Issues:
============

	None



***************************
CDMA2000 5x08.B02
***************************

Date:	October 29, 2010

Base:	V5.08
MMI:	2.99T
LH:	V2.88j	V12
	X3.26b	V22

General Remarks
===============

	This release of CDMA2000 software is based on the CMU base system V5.08 and
	can be installed together with other V5.08 compatible function groups.

Enhancements since last official version V5.08 (10aug2010):
===========================================================

	Repaired bug that causes a LH crash when establishing a call
	This base is *NOT* compatible with base V5.05.


Known Issues:
============

	None



***************************
CDMA2000 5x20.I06
***************************

Date:	October 20, 2010

Base:	5x20.I05
MMI:	2.99T
LH:	V2.88L	V12
	X3.26d	V22

General Remarks
===============

	This release of CDMA2000 software is based on the CMU base system 5x20.I05 and
	can be installed together with other 5x20.I05 compatible function groups.

Enhancements since last official version V5.10 (05june2009):
============================================================

	Incorporated PCB Puncture Adjustment during FCH Gain update
	Repair bug that causes a LH crash when establishing a call
	Repaired problem in HW signal off state (MESSAGE_HWL_CHANGE_LEVEL handling)
	Handled the race condition involving the Protocol Revision parameter 
	Made Inactivity Control hidden parameters visible again (Bugzilla # 507)
	Fixed broken remote command (Bugzilla # 509)
	Fixed preregistration paging problem with Class 1 IMSI
	Base 5x20 integrated to allow for some hardware changes.
	This base is *NOT* compatible with base V5.10.


Known Issues:
============

	None



***************************
CDMA2000 5x10.A05
***************************

Date:	October 1, 2010

Base:	V5.10
MMI:	2.99T
LH:	V2.88i	V12
	X3.26b	V22

General Remarks
===============

	This release of CDMA2000 software is based on the CMU base system V5.10 and
	can be installed together with other V5.10 compatible function groups.

Enhancements since last official version V5.10 (05june2009):
==============================================

	Repair bug that causes a LH crash when establishing a call
	Repaired problem in HW signal off state (MESSAGE_HWL_CHANGE_LEVEL handling)
	Handled the race condition involving the Protocol Revision parameter 
	Made Inactivity Control hidden parameters visible again (Bugzilla # 507)
	Fixed broken remote command (Bugzilla # 509)
	Fixed preregistration paging problem with Class 1 IMSI


Known Issues:
============

	None



***************************
CDMA2000 5x10.A04
***************************

Date:	August 31, 2010

Base:	V5.10
MMI:	2.99T
LH:	V2.88i	V12
	X3.26a	V22

General Remarks
===============

	This release of CDMA2000 software is based on the CMU base system V5.10 and
	can be installed together with other V5.10 compatible function groups.

Enhancements since last official version V5.10 (05june2009):
==============================================

	Repaired problem in HW signal off state (MESSAGE_HWL_CHANGE_LEVEL handling)
	Handled the race condition involving the Protocol Revision parameter 
	Made Inactivity Control hidden parameters visible again (Bugzilla # 507)
	Fixed broken remote command (Bugzilla # 509)
	Fixed preregistration paging problem with Class 1 IMSI


Known Issues:
============

	None



***************************
CDMA2000 5x20.I05
***************************

Date:	August 24, 2010

Base:	5x20.I05
MMI:	2.99T
LH:	V2.88i	V12
	X3.26a	V22

General Remarks
===============

	This release of CDMA2000 software is based on the CMU base system 5x20.I05 and
	can be installed together with other 5x20.I05 compatible function groups.

Enhancements since last official version V5.10 (05june2009):
==============================================

	Base 5x20 integrated to allow for some hardware changes.
	Repaired problem in HW signal off state (MESSAGE_HWL_CHANGE_LEVEL handling)
	Handled the race condition involving the Protocol Revision parameter 
	Made Inactivity Control hidden parameters visible again (Bugzilla # 507)
	Fixed broken remote command (Bugzilla # 509)
	Fixed preregistration paging problem with Class 1 IMSI
	This base is *NOT* compatible with base V5.10.


Known Issues:
============

	None



***************************
CDMA2000 5x08.B01
***************************

Date:	August 4, 2010

Base:	5x08.B01
MMI:	2.99T
LH:	V2.88i	V12
	X3.25u	V22

General Remarks
===============

	This release of CDMA2000 software is based on the CMU base system 5x08.B01 and
	can be installed together with other V5.08 compatible function groups.

Enhancements since last official version V5.05 (07may2009):
===========================================================

	New base integrated to allow for some hardware changes.
	No functional difference between this version and the 5x05.A03 version.
	This base is *NOT* compatible with base V5.05.


Known Issues:
============

	None



***************************
CDMA2000 5x20.A01
***************************

Date:	August 2, 2010

Base:	5x20.A01
MMI:	2.99T
LH:	V2.88i	V12
	X3.25u	V22

General Remarks
===============

	This release of CDMA2000 software is based on the CMU base system 5x20.A30 and
	can be installed together with other 5x20.A30 compatible function groups.

Enhancements since last official version V5.10 (05june2009):
==============================================

	New base integrated to allow for some hardware changes.
	No functional difference between this version and the 5x10.A03 version.
	This base is *NOT* compatible with base V5.10.


Known Issues:
============

	None



***************************
CDMA2000 5x08.A01
***************************

Date:	July 30, 2010

Base:	5x08.A01
MMI:	2.99T
LH:	V2.88i	V12
	X3.25u	V22

General Remarks
===============

	This release of CDMA2000 software is based on the CMU base system 5x08.A01 and
	can be installed together with other V5.08 compatible function groups.

Enhancements since last official version V5.05 (07may2009):
==============================================

	New base integrated to allow for some hardware changes.
	No functional difference between this version and the 5x05.A03 version.
	This base is *NOT* compatible with base V5.05.


Known Issues:
============

	None



***************************
CDMA2000 5x05.A03
***************************

Date:	July 2, 2010

Base:	V5.05
MMI:	2.99T
LH:	V2.88i	V12
	X3.25u	V22

General Remarks
===============

	This release of CDMA2000 software is based on the CMU base system V5.05 and
	can be installed together with other V5.05 compatible function groups.

Enhancements since last official version V5.05 (07may2009):
===========================================================

	LH:  Prevented the L2_DschArqMgr from being used after it has been deleted due to a handoff.


Known Issues:
============

	None



***************************
CDMA2000 5x10.A03
***************************

Date:	March 9, 2010

Base:	V5.10
MMI:	2.99T
LH:	V2.88h	V12
	X3.25t	V22

General Remarks
===============

	This release of CDMA2000 software is based on the CMU base system V5.10 and
	can be installed together with other V5.10 compatible function groups.

Enhancements since last official version V5.10 (05june2009):
==============================================

	Repaired problem in HW signal off state (MESSAGE_HWL_CHANGE_LEVEL handling)
	Handled the race condition involving the Protocol Revision parameter 
	Made Inactivity Control hidden parameters visible again (Bugzilla # 507)
	Fixed broken remote command (Bugzilla # 509)
	Fixed preregistration paging problem with Class 1 IMSI


Known Issues:
============

	None



***************************
CDMA2000 5x05.A02
***************************

Date:	March 5, 2010

Base:	V5.05
MMI:	2.99T
LH:	V2.88h	V12
	X3.25t	V22

General Remarks
===============

	This release of CDMA2000 software is based on the CMU base system V5.05 and
	can be installed together with other V5.05 compatible function groups.

Enhancements since last official version V5.05 (07may2009):
==============================================

	Repaired problem in HW signal off state (MESSAGE_HWL_CHANGE_LEVEL handling)
	Handled the race condition involving the Protocol Revision parameter 
	Made Inactivity Control hidden parameters visible again (Bugzilla # 507)
	Fixed broken remote command (Bugzilla # 509)
	Fixed preregistration paging problem with Class 1 IMSI


Known Issues:
============

	None



***************************
CDMA2000 5x05.A01
***************************

Date:	January 8, 2010

Base:	V5.05
MMI:	2.99S
LH:	V2.88h	V12
	X3.25t	V22

General Remarks
===============

	This release of CDMA2000 software is based on the CMU base system V5.05 and
	can be installed together with other V5.05 compatible function groups.

Enhancements since last official version V5.05 (07may2009):
==============================================

	Fixed preregistration paging problem with Class 1 IMSI

Known Issues:
============

	None



***************************
CDMA2000 5x10.A02
***************************

Date:	May 29, 2009

Base:	5x10.A01
MMI:	2.99S
LH:	V2.88f	V12
	X3.25q	V22

General Remarks
===============

	This release of CDMA2000 software is based on the CMU base system 5x10.A01 and
	can be installed together with other 5x10.Axx (*not* V5.00) compatible function groups.

Enhancements since last official version V5.05 (07may2009):
==============================================

	Handled two messages arriving in incorrect state (in ip_par & sigl4tsk)

Known Issues:
============

	None



***************************
CDMA2000 5x10.A01
***************************

Date:	May 20, 2009

Base:	5x10.A01
MMI:	2.99S
LH:	V2.88f	V12
	X3.25q	V22

General Remarks
===============

	This release of CDMA2000 software is based on the CMU base system 5x00.B15
	and can be installed together with other 5x00.B15 (*not* V5.00) compatible function groups.

Enhancements since last official version V5.05 (07may2009):
==============================================

	None

Known Issues:
============

	None



***************************
CDMA2000 5x00.A78
***************************

Date:	May 3, 2009

Base:	5x00.B15
MMI:	2.99S
LH:	V2.88f	V12
	X3.25q	V22

General Remarks
===============

	This release of CDMA2000 software is based on the CMU base system 5x00.B15
	and can be installed together with other 5x00.B15 (*not* V5.00) compatible function groups.

Enhancements since last official version V5.01 (10oct2008):
==============================================

	5x00.A74: FSW: Trying new base for compatibility with new MMI
	5x00.A74: LH: Fixed PPP Authentication issue related to CHAP/PAP
	5x00.A73: MMI: Corrected DBM parameter problem
	5x00.A72: FSW: Corrected looping method of copying DBM binary data block
	5x00.A72: LH:  Changed DBM cdma2k time source
	5x00.A71: FSW: Corrected pending event flag usage in call to send_lh_message
	5x00.A70: FSW: Corrected DBM binary block access
	5x00.A69: FSW: Implemented DBM bit count / byte count conversions
	5x00.A68: FSW: Implemented Data Burst Message handling
	5x00.A68: FSW: Allow new band classes 18 and 19
	5x00.A68: LH:  Implemented Data Burst Message handling
	5x00.A68: LH:  Fixed PREV_7 paging bug
	5x00.A68: LH:  Allow new band classes 18 and 19
	5x00.A66: FSW: change state direction when receiving msg SIG_MESSAGE_CMND_OFF in Signal Off state
	5x00.A66: FSW: resend msg MESSAGE_HWL_CHANGE_LEVEL when received in Wait For Signal Off state
	5x00.A64: FSW: Corrected bug in unicode char qty calculation
	5x00.A64: FSW: Allow uppercase keyword Data on SMS line as well as lowercase keyword data
	5x00.A64: FSW: Added handling of CoPro message COR_MESSAGE_COMMAND when it is received in the wrong state
	5x00.A64: FSW: Added function group version check to disallow loading mismatched function groups
	5x00.A64: LH:  Fixed P_REV 7 paging issue
	5x00.A64: LH:  Added A_GPS Support ( Ethernet Based )
	5x00.A63: LH:  Fixed red box that occurs while running FER meas
	5x00.A62: LH:  Paging issue in P_REV 7 mode

Known Issues:
============

	None



***************************
CDMA2000 5x00.A77
***************************

Date:	April 30, 2009

Base:	5x00.B15
MMI:	2.99S
LH:	V2.88f	V12
	X3.25p	V22

General Remarks
===============

	This release of CDMA2000 software is based on the CMU base system 5x00.B15
	and can be installed together with other 5x00.B15 (*not* V5.00) compatible function groups.

Enhancements since last official version V5.01 (10oct2008):
==============================================

	5x00.A74: FSW: Trying new base for compatibility with new MMI
	5x00.A74: LH: Fixed PPP Authentication issue related to CHAP/PAP
	5x00.A73: MMI: Corrected DBM parameter problem
	5x00.A72: FSW: Corrected looping method of copying DBM binary data block
	5x00.A72: LH:  Changed DBM cdma2k time source
	5x00.A71: FSW: Corrected pending event flag usage in call to send_lh_message
	5x00.A70: FSW: Corrected DBM binary block access
	5x00.A69: FSW: Implemented DBM bit count / byte count conversions
	5x00.A68: FSW: Implemented Data Burst Message handling
	5x00.A68: FSW: Allow new band classes 18 and 19
	5x00.A68: LH:  Implemented Data Burst Message handling
	5x00.A68: LH:  Fixed PREV_7 paging bug
	5x00.A68: LH:  Allow new band classes 18 and 19
	5x00.A66: FSW: change state direction when receiving msg SIG_MESSAGE_CMND_OFF in Signal Off state
	5x00.A66: FSW: resend msg MESSAGE_HWL_CHANGE_LEVEL when received in Wait For Signal Off state
	5x00.A64: FSW: Corrected bug in unicode char qty calculation
	5x00.A64: FSW: Allow uppercase keyword Data on SMS line as well as lowercase keyword data
	5x00.A64: FSW: Added handling of CoPro message COR_MESSAGE_COMMAND when it is received in the wrong state
	5x00.A64: FSW: Added function group version check to disallow loading mismatched function groups
	5x00.A64: LH:  Fixed P_REV 7 paging issue
	5x00.A64: LH:  Added A_GPS Support ( Ethernet Based )
	5x00.A63: LH:  Fixed red box that occurs while running FER meas
	5x00.A62: LH:  Paging issue in P_REV 7 mode

Known Issues:
============

	None



***************************
CDMA2000 5x00.A76
***************************

Date:	April 28, 2009

Base:	5x00.B15
MMI:	2.99S
LH:	V2.88f	V12
	X3.25p	V22

General Remarks
===============

	This release of CDMA2000 software is based on the CMU base system 5x00.B15
	and can be installed together with other 5x00.B15 (*not* V5.00) compatible function groups.

Enhancements since last official version V5.01 (10oct2008):
==============================================

	5x00.A74: FSW: Trying new base for compatibility with new MMI
	5x00.A74: LH: Fixed PPP Authentication issue related to CHAP/PAP
	5x00.A73: MMI: Corrected DBM parameter problem
	5x00.A72: FSW: Corrected looping method of copying DBM binary data block
	5x00.A72: LH:  Changed DBM cdma2k time source
	5x00.A71: FSW: Corrected pending event flag usage in call to send_lh_message
	5x00.A70: FSW: Corrected DBM binary block access
	5x00.A69: FSW: Implemented DBM bit count / byte count conversions
	5x00.A68: FSW: Implemented Data Burst Message handling
	5x00.A68: FSW: Allow new band classes 18 and 19
	5x00.A68: LH:  Implemented Data Burst Message handling
	5x00.A68: LH:  Fixed PREV_7 paging bug
	5x00.A68: LH:  Allow new band classes 18 and 19
	5x00.A66: FSW: change state direction when receiving msg SIG_MESSAGE_CMND_OFF in Signal Off state
	5x00.A66: FSW: resend msg MESSAGE_HWL_CHANGE_LEVEL when received in Wait For Signal Off state
	5x00.A64: FSW: Corrected bug in unicode char qty calculation
	5x00.A64: FSW: Allow uppercase keyword Data on SMS line as well as lowercase keyword data
	5x00.A64: FSW: Added handling of CoPro message COR_MESSAGE_COMMAND when it is received in the wrong state
	5x00.A64: FSW: Added function group version check to disallow loading mismatched function groups
	5x00.A64: LH:  Fixed P_REV 7 paging issue
	5x00.A64: LH:  Added A_GPS Support ( Ethernet Based )
	5x00.A63: LH:  Fixed red box that occurs while running FER meas
	5x00.A62: LH:  Paging issue in P_REV 7 mode

Known Issues:
============

	None



***************************
CDMA2000 5x00.A75
***************************

Date:	April 23, 2009

Base:	5x00.B15
MMI:	2.99S
LH:	V2.88e	V12
	X3.25o	V22

General Remarks
===============

	This release of CDMA2000 software is based on the CMU base system 5x00.B15
	and can be installed together with other 5x00.B15 (*not* V5.00) compatible function groups.

Enhancements since last official version V5.01 (10oct2008):
==============================================

	5x00.A74: FSW: Trying new base for compatibility with new MMI
	5x00.A74: LH: Fixed PPP Authentication issue related to CHAP/PAP
	5x00.A73: MMI: Corrected DBM parameter problem
	5x00.A72: FSW: Corrected looping method of copying DBM binary data block
	5x00.A72: LH:  Changed DBM cdma2k time source (5x00.A72)
	5x00.A71: FSW: Corrected pending event flag usage in call to send_lh_message
	5x00.A70: FSW: Corrected DBM binary block access
	5x00.A69: FSW: Implemented DBM bit count / byte count conversions
	5x00.A68: FSW: Implemented Data Burst Message handling
	5x00.A68: FSW: Allow new band classes 18 and 19
	5x00.A68: LH:  Implemented Data Burst Message handling
	5x00.A68: LH:  Fixed PREV_7 paging bug
	5x00.A68: LH:  Allow new band classes 18 and 19
	5x00.A66: FSW: change state direction when receiving msg SIG_MESSAGE_CMND_OFF in Signal Off state
	5x00.A66: FSW: resend msg MESSAGE_HWL_CHANGE_LEVEL when received in Wait For Signal Off state
	5x00.A64: FSW: Corrected bug in unicode char qty calculation
	5x00.A64: FSW: Allow uppercase keyword Data on SMS line as well as lowercase keyword data
	5x00.A64: FSW: Added handling of CoPro message COR_MESSAGE_COMMAND when it is received in the wrong state
	5x00.A64: FSW: Added function group version check to disallow loading mismatched function groups
	5x00.A64: LH:  Fixed P_REV 7 paging issue
	5x00.A64: LH:  Added A_GPS Support ( Ethernet Based )
	5x00.A63: LH:  Fixed red box that occurs while running FER meas
	5x00.A62: LH:  Paging issue in P_REV 7 mode

Known Issues:
============

	None



***************************
CDMA2000 5x00.A74
***************************

Date:	April 10, 2009

Base:	5x00.B15
MMI:	2.99S
LH:	V2.88d	V12
	X3.25n	V22

General Remarks
===============

	This release of CDMA2000 software is based on the CMU base system 5x00.B15
	and can be installed together with other 5x00.B15 (*not* V5.00) compatible function groups.

Enhancements:
=============

	FSW: Trying new base for compatibility with new MMI
	LH: Fixed PPP Authentication issue related to CHAP/PAP

Known Issues:
============

	None



***************************
CDMA2000 5x00.A73
***************************

Date:	April 9, 2009

Base:	V5.03
MMI:	2.99S
LH:	V2.88c	V12
	X3.25m	V22

General Remarks
===============

	This release of CDMA2000 software is based on the CMU base system V5.03
	and can be installed together with other V5.03 (*not* V5.00) compatible function groups.

Enhancements:
=============

	MMI: Corrected DBM parameter problem

Known Issues:
============

	None



***************************
CDMA2000 5x00.A72
***************************

Date:	April 2, 2009

Base:	V5.03
MMI:	2.99P
LH:	V2.88c	V12
	X3.25m	V22

General Remarks
===============

	This release of CDMA2000 software is based on the CMU base system V5.03
	and can be installed together with other V5.03 (*not* V5.00) compatible function groups.

Enhancements:
=============

	FSW: Corrected looping method of copying DBM binary data block 
	LH:  Changed DBM cdma2k time source

Known Issues:
============

	None



***************************
CDMA2000 5x00.A71
***************************

Date:	April 1, 2009

Base:	V5.03
MMI:	2.99P
LH:	V2.88b	V12
	X3.25L	V22

General Remarks
===============

	This release of CDMA2000 software is based on the CMU base system V5.03
	and can be installed together with other V5.03 (*not* V5.00) compatible function groups.

Enhancements:
=============

	FSW: Corrected pending event flag usage in call to send_lh_message

Known Issues:
============

	None



***************************
CDMA2000 5x00.A70
***************************

Date:	April 1, 2009

Base:	V5.03
MMI:	2.99P
LH:	V2.88b	V12
	X3.25L	V22

General Remarks
===============

	This release of CDMA2000 software is based on the CMU base system V5.03
	and can be installed together with other V5.03 (*not* V5.00) compatible function groups.

Enhancements:
=============

	FSW: Corrected DBM binary block access

Known Issues:
============

	None



***************************
CDMA2000 5x00.A69
***************************

Date:	March 30, 2009

Base:	V5.03
MMI:	2.99P
LH:	V2.88a	V12
	X3.25k	V22

General Remarks
===============

	This release of CDMA2000 software is based on the CMU base system V5.03
	and can be installed together with other V5.03 (*not* V5.00) compatible function groups.

Enhancements:
=============

	FSW: Implemented DBM bit count / byte count conversions

Known Issues:
============

	None



***************************
CDMA2000 5x00.A68
***************************

Date:	March 18, 2009

Base:	V5.03
MMI:	2.99P
LH:	V2.87w	V12
	X3.25j	V22

General Remarks
===============

	This release of CDMA2000 software is based on the CMU base system V5.03
	and can be installed together with other V5.03 (*not* V5.00) compatible function groups.

Enhancements:
=============

	FSW: Implemented Data Burst Message handling
	FSW: Allow new band classes 18 and 19
	LH:  Implemented Data Burst Message handling
	LH:  Fixed PREV_7 paging bug
	LH:  Allow new band classes 18 and 19

Known Issues:
============

	None



***************************
CDMA2000 5x00.A67
***************************

Date:	March 5, 2009

Base:	V5.00
MMI:	2.99M
LH:	V2.87u	V12
	X3.25i	V22

General Remarks
===============

	This release of CDMA2000 software is based on the CMU base system V5.00
	and can be installed together with other V5.00 compatible function groups.

Enhancements:
=============

	None

Known Issues:
============

	None



***************************
CDMA2000 5x00.A66
***************************

Date:	March 4, 2009

Base:	V5.00
MMI:	2.99M
LH:	V2.87u	V12
	X3.25h	V22

General Remarks
===============

	This release of CDMA2000 software is based on the CMU base system V5.00
	and can be installed together with other V5.00 compatible function groups.

Enhancements:
=============

	FSW: change state direction when receiving msg SIG_MESSAGE_CMND_OFF in Signal Off state
	FSW: resend msg MESSAGE_HWL_CHANGE_LEVEL when received in Wait For Signal Off state

Known Issues:
============

	None



***************************
CDMA2000 5x00.A65
***************************

Date:	February 15, 2009

Base:	V5.00
MMI:	2.99L
LH:	V2.87u	V12
	X3.25h	V22

General Remarks
===============

	This release of CDMA2000 software is based on the CMU base system V5.00
	and can be installed together with other V5.00 compatible function groups.

Enhancements:
=============

	None


Known Issues:
============

	None



***************************
CDMA2000 5x00.A64
***************************

Date:	February 10, 2009

Base:	V5.00
MMI:	2.99L
LH:	V2.87s	V12
	X3.25e	V22

General Remarks
===============

	This release of CDMA2000 software is based on the CMU base system V5.00
	and can be installed together with other V5.00 compatible function groups.

Enhancements:
=============

	FSW: Corrected bug in unicode char qty calculation
	FSW: Allow uppercase keyword Data on SMS line as well as lowercase keyword data
	FSW: Added handling of CoPro message COR_MESSAGE_COMMAND when it is received in the wrong state
	FSW: Added function group version check to disallow loading mismatched function groups
	LH:  Fixed P_REV 7 paging issue
	LH:  Added A_GPS Support ( Ethernet Based )


Known Issues:
============

	None



***************************
CDMA2000 5x00.A63
***************************

Date:	December 19, 2008

Base:	V5.00
MMI:	2.99K
LH:	V2.87m	V12
	X3.25b	V22

General Remarks
===============

	This release of CDMA2000 software is based on the CMU base system V5.00
	and can be installed together with other V5.00 compatible function groups.

Enhancements:
=============

	LH: Fixed red box that occurs while running FER meas

Known Issues:
============

	None



***************************
CDMA2000 5x00.A62
***************************

Date:	November 21, 2008

Base:	V5.00
MMI:	2.99J
LH:	V2.87l	V12
	X3.24t	V22

General Remarks
===============

	This release of CDMA2000 software is based on the CMU base system V5.00
	and can be installed together with other V5.00 compatible function groups.

Enhancements:
=============

	LH: Paging issue in P_REV 7 mode

Known Issues:
============

	None





***************************
CDMA2000 4x50.B10
***************************

Date:	October 17, 2008

Base:	V4.51
MMI:	2.99J
LH:	V2.87F	V12
	X3.24O	V22

General Remarks
===============

	This release of CDMA2000 software is based on the CMU base system V4.51
	and can be installed together with other V4.51 compatible function groups.

Enhancements:
=============

	None

Known Issues:
===========

	None



***************************
CDMA2000 4x50.B09
***************************

Date:	October 14, 2008

Base:	V4.51
MMI:	2.99J
LH:	V2.87e	V12
	X3.24n	V22

General Remarks
===============

	This release of CDMA2000 software is based on the CMU base system V4.51
	and can be installed together with other V4.51 compatible function groups.

Enhancements:
=============

	LH:  Increased size of SMS text area in structure LH_C2K_SMS_MESSAGE_DATA to 512 chars.
	FSW: Changed LH load design to retry when self test is running, otherwise fail (red box) if two loads fail sequentially.

Known Issues:
===========

	None



***************************
CDMA2000 5x00.A61
***************************

Date:	October 6, 2008

Base:	V5.00
MMI:	2.99J
LH:	V2.87d	V12
	X3.24m	V22

General Remarks
===============

	This release of CDMA2000 software is based on the CMU base system V5.00
	and can be installed together with other V5.00 or 5x00.A56 compatible function groups.

Enhancements:
=============

	General:
	FSW: Changed LH load design to retry when self test is running, otherwise fail (red box) if two loads fail sequentially.

Known Issues:
===========

	None



***************************
CDMA2000 4x50.B08
***************************

Date:	October 2, 2008

Base:	V4.51
MMI:	2.99J
LH:	V2.87e	V12
	X3.24n	V22

General Remarks
===============

	This release of CDMA2000 software is based on the CMU base system V4.51
	and can be installed together with other V4.51 compatible function groups.

Enhancements:
=============

	LH:  Special build for QualComm containing increased SMS message length

Known Issues:
===========

	None



***************************
CDMA2000 4x50.B07
***************************

Date:	October 1, 2008

Base:	V4.51
MMI:	2.99J
LH:	V2.87d	V12
	X3.24m	V22

General Remarks
===============

	This release of CDMA2000 software is based on the CMU base system V4.51
	and can be installed together with other V4.51 compatible function groups.

Enhancements:
=============

	General:
	LH:  Additional fix to support fall back to SimpleIP call after the Failure of MobileIP call.
	FSW: Redesigned lh interface code to make it more robust

Known Issues:
===========

	None



***************************
CDMA2000 5x00.A60
***************************

Date:	September 30, 2008

Base:	V5.00
MMI:	2.99J
LH:	V2.87d	V12
	X3.24m	V22

General Remarks
===============

	This release of CDMA2000 software is based on the CMU base system V5.00
	and can be installed together with other V5.00 or 5x00.A56 compatible function groups.

Enhancements:
=============

	General:
	LH:  Additional fix to support fall back to SimpleIP call after the Failure of MobileIP call.
	FSW: Redesigned lh interface code to make it more robust

Known Issues:
===========

	None



***************************
CDMA2000 4x50.B06
***************************

Date:   September 24, 2008

Base:	V4.51
MMI:	2.99J
LH:	V2.87c	V12
	X3.24L	V22

General Remarks
===============

	This release of CDMA2000 software is based on the CMU base system V4.51
	and can be installed together with other V4.51 compatible function groups.

Enhancements:
=============

	LH:  Bug fix for the redbox seen in CCF
	LH:  Changes to correct the file creation time stamp

	General:
	LH:  Boot loader update: new soft boot ROM version is 1.55. Only print "Exception MSG:" when a prior exception has been detected.
	LH:  Do not print out task names for previous and current task ID at system start.  This fix addresses the H300 data exception at system start.
	LH:  Exceptions no longer produce a Red Box. Instead, one yellow box will be generated along with one or more warning messages which are sent to the CMU. The warning messages can be found in the c2kfault.log file.

Known Issues:
===========

	None



***************************
CDMA2000 5x00.A59
***************************

Date:	September 22, 2008

Base:	V5.00
MMI:	2.99J
LH:	V2.87c	V12
	X3.24L	V22

General Remarks
===============

	This release of CDMA2000 software is based on the CMU base system V5.00
	and can be installed together with other V5.00 or 5x00.A56 compatible function groups.

Enhancements:
=============

	None


Known Issues:
===========

	None



***************************
CDMA2000 5x00.A58
***************************

Date:	September 18, 2008

Base:	V5.00
MMI:	2.99J
LH:	V2.87a	V12
	X3.24k	V22

General Remarks
===============

	This release of CDMA2000 software is based on the CMU base system V5.00
	and can be installed together with other V5.00 or 5x00.A56 compatible function groups.

Enhancements:
=============

	LH:  Bug fix for the redbox seen in CCF
	LH:  Changes to correct the file creation time stamp

	General:
	LH:  Boot loader update: new soft boot ROM version is 1.55. Only print "Exception MSG:" when a prior exception has been detected.
	LH:  Do not print out task names for previous and current task ID at system start.  This fix addresses the h300 data exception at system start.
	LH:  Exceptions no longer produce a Red Box. Instead, one yellow box will be generated along with one or more warning messages which are sent to the CMU. The warning messages can be found in the c2kfault.log file if using the latest FSW software or in the k83p.log file (must enable k83p logging in the cmu.ini file) if using earlier FSW software.
	FSW: Warning messages from the LH will be logged in the c2kfault.log file.


Known Issues:
===========

	None



***************************
CDMA2000 4x50.B05
***************************

Date:   September 16, 2008

Base:	V4.51
MMI:	2.99J
LH:	V2.87a	V12
	X3.24i	V22

General Remarks
===============

	This release of CDMA2000 software is based on the CMU base system V4.51
	and can be installed together with other V4.51 compatible function groups.

Enhancements:
=============

	General:
	FSW:	Warning messages from the LH will be logged in the c2kfault.log file.

Known Issues:
===========

	None



***************************
CDMA2000 4x50.B04
***************************

Date:   September 15, 2008

Base:	V4.51
MMI:	2.99J
LH:     V2.87a  V12
        X3.24h  V22

General Remarks
===============

	This release of CDMA2000 software is based on the CMU base system V4.51
	and can be installed together with other V4.51 compatible function groups.

Enhancements:
=============

	LH:  Bug fix for the redbox seen in CCF
	LH:  Changes to correct the file creation time stamp

	General enhancements in this version:
	LH:  Boot loader update: new soft boot ROM version is 1.55. Only print "Exception MSG:" when a prior exception has been detected.
	LH:  Do not print out task names for previous and current task ID at system start.  This fix addresses the h300 data exception at system start.
	LH:  Exceptions no longer produce a Red Box. Instead, one yellow box will be generated along with one or more warning messages which are sent to the CMU. The warning messages can be found in the c2kfault.log file if using the latest FSW software or in the k83p.log file (must enable k83p logging in the cmu.ini file) if using earlier FSW software.


Known Issues:
===========

	None



***************************
CDMA2000 4x50.B03
***************************

Date:	Aug 28, 2008

Base:	V4.51
MMI:	2.99J
LH:	V2.86u	V12
	X3.24e	V22

General Remarks
===============

	This release of CDMA2000 software is based on the CMU base system V4.51
	and can be installed together with other V4.51 compatible function groups.

Enhancements:
=============

	LH: Fixed LH crash during SMS file ftp transfer


Known Issues:
===========

	None



***************************
CDMA2000 4x50.B02
***************************

Date:	Aug 22, 2008

Base:	V4.51
MMI:	2.99J
LH:	V2.86r	V12
	X3.24c	V22

General Remarks
===============

	This release of CDMA2000 software is based on the CMU base system V4.51
	and can be installed together with other V4.51 compatible function groups.

Enhancements:
=============

	FSW: Corrected RF connector limits for U99 option after reset
	FSW: Fixed RF connector limits conflict if U99 is present and AWGN is enabled


Known Issues:
===========

	None



***************************
CDMA2000 5x00.A57
***************************

Date:	August 4, 2008

Base:	V5.00
MMI:	2.99J
LH:	V2.86q	V12
	X3.24b	V22

General Remarks
===============

	This release of CDMA2000 software is based on the CMU base system V5.00
	and can be installed together with other V5.00 or 5x00.A56 compatible function groups.

Enhancements:
=============

	None


Known Issues:
===========

	BR #458: LH:  Power Control PATTERN mode is not doing what it is supposed to be doing
	BR #470: LH:  FETAP Send-Queue Algorithm Needs Refinement
	BR #472: LH:  C2K Access Ch preamble length needs to be configurable
	BR #479: FSW: SO33 PPP Authentication Shared by IMT2K FGroups
	BR #482: FSW: U99 not recognized in non signaling after front panel reset



Note: Official version V5.00 was based on the 5x00.A56 and released on July 30, 2008.


***************************
CDMA2000 5x00.A56
***************************

Date:	July 17, 2008

Base:	5x00.A56
MMI:	2.99J
LH:	V2.86m	V12
	X3.23o	V22

General Remarks
===============

	This release of CDMA2000 software is based on the CMU base system 5x00.A56
	and can be installed together with other 5x00.A55 or 5x00.A56 compatible function groups.

Enhancements:
=============

	LH:  Enabled IEI handling for B83 without B89 to support data call
	FSW: Increased Protocol Revision parameter upper limit value from 6 to 7
	FSW: Added time stamp option for SMS text message from file


Known Issues:
===========

	None



***************************
CDMA2000 4x50.B01
***************************

Date:	July 17, 2008

Base:	V4.51
MMI:	2.99J
LH:	V2.86m	V12
	X3.23o	V22

General Remarks
===============

	This release of CDMA2000 software is based on the CMU base system V4.51
	and can be installed together with other V4.51 compatible function groups.

Enhancements:
=============

	LH:  Enabled IEI handling for B83 without B89 to support data call
	FSW: Increased Protocol Revision parameter upper limit value from 6 to 7
	FSW: Added time stamp option for SMS text message from file


Known Issues:
===========

	None



***************************
CDMA2000 5x00.A55
***************************

Date:	July 08, 2008

Base:	5x00.A55
MMI:	2.99J
LH:	V2.86m	V12
	X3.23m	V22

General Remarks
===============

	This release of CDMA2000 software is based on the CMU base system 5x00.A55
	and can be installed together with other 5x00.A55 compatible function groups.

Enhancements:
=============

	FSW: clarified mapping of access probe parameters
	FSW: fixed early "retain netclock" adjust during startup


Known Issues:
===========

	FSW: SMS sent from from file has no time stamp option



Note: Official version V4.53 was based on the 4x50.A93 and released on July 10, 2008.


***************************
CDMA2000 4x50.A93
***************************

Date:	July 02, 2008

Base:	V4.51
MMI:	2.99J
LH:	V2.86m	V12
	X3.23m	V22

General Remarks
===============

	This release of CDMA2000 software is based on the CMU base system V4.51
	and can be installed together with other V4.51 compatible function groups.

Enhancements:
=============

	FSW: clarified mapping of access probe parameters
	FSW: fixed early "retain netclock" adjust during startup


Known Issues:
===========

	FSW: SMS sent from from file has no time stamp option



***************************
CDMA2000 4x50.A92
***************************

Date:	July 01, 2008

Base:	V4.51
MMI:	2.99J
LH:	V2.86m	V12
	X3.23m	V22

General Remarks
===============

	This release of CDMA2000 software is based on the CMU base system V4.51
	and can be installed together with other V4.51 compatible function groups.

Enhancements:
=============

	FSW: fixed netclock related yellow boxes during interband handoff


Known Issues:
===========

	None



***************************
CDMA2000 5x00.A50
***************************

Date:	June 28, 2008

Base:	5x00.A50
MMI:	2.99J
LH:	V2.86m	V12
	X3.23m	V22

General Remarks
===============

	This release of CDMA2000 software is based on the CMU base system 5x00.A50
	and can be installed together with other 5x00.A50 compatible function groups.

Enhancements:
=============

	FSW: incorporated all the scattered netclock fixes from other clearcase views
	FSW: fixed LH Sync reboot problem (when RequestInProgress is NULL)


Known Issues:
===========

	Netclock yellow boxes from file pmgr.cpp and pmgr_pi2.cpp



***************************
CDMA2000 4x50.A90
***************************

Date:	June 26, 2008

Base:	V4.51
MMI:	2.99J
LH:	V2.86m	V12
	X3.23m	V22

General Remarks
===============

	This release of CDMA2000 software is based on the CMU base system V4.51
	and can be installed together with other V4.51 compatible function groups.

Enhancements:
=============

	FSW: installed remaining netclock fixes from other clearcase views


Known Issues:
===========

	None



***************************
CDMA2000 4x50.A88
***************************

Date:	June 24, 2008

Base:	V4.51
MMI:	2.99J
LH:	V2.86m	V12
	X3.23m	V22

General Remarks
===============

	This release of CDMA2000 software is based on the CMU base system V4.51
	and can be installed together with other V4.51 compatible function groups.

Enhancements:
=============

	FSW: repaired filename creation for incoming SMS text & unicode messages


Known Bugs:
===========

	None



***************************
CDMA2000 4x50.A87
***************************

Date:	June 24, 2008

Base:	V4.51
MMI:	2.99J
LH:	V2.86m	V12
	X3.23m	V22

General Remarks
===============

	This release of CDMA2000 software is based on the CMU base system V4.51
	and can be installed together with other V4.51 compatible function groups.

Enhancements:
=============

	None


Known Bugs:
===========

	None



***************************
CDMA2000 4x50.A86
***************************

Date:	June 23, 2008

Base:	V4.51
MMI:	2.99J
LH:	V2.86m	V12
	X3.23m	V22

General Remarks
===============

	This release of CDMA2000 software is based on the CMU base system V4.51
	and can be installed together with other V4.51 compatible function groups.

Enhancements:
=============

	None


Known Bugs:
===========

	None



***************************
CDMA2000 4x50.A85
***************************

Date:	June 19, 2008

Base:	V4.51
MMI:	2.99J
LH:	V2.86m	V12
	X3.23m	V22

General Remarks
===============

	This release of CDMA2000 software is based on the CMU base system V4.51
	and can be installed together with other V4.51 compatible function groups.

Enhancements:
=============

	FSW: Repaired problem with changing hardware settings while in Signal Off


Known Bugs:
===========

	None



***************************
CDMA2000 4x50.A84
***************************

Date:	June 18, 2008

Base:	V4.51
MMI:	2.99J
LH:	V2.86m	V12
	X3.23k	V22

General Remarks
===============

	This release of CDMA2000 software is based on the CMU base system V4.51
	and can be installed together with other V4.51 compatible function groups.

Enhancements:
=============

	FSW: Fixed a CMU hang state for power level changes in Signal Off


Known Bugs:
===========

	If you change hardware settings while in Signal Off, then the first value within a measurement will be incorrect



***************************
CDMA2000 4x50.A83
***************************

Date:	June 18, 2008

Base:	V4.51
MMI:	2.99J
LH:	V2.86m	V12
	X3.23k	V22

General Remarks
===============

	This release of CDMA2000 software is based on the CMU base system V4.51
	and can be installed together with other V4.51 compatible function groups.

Enhancements:
=============

	FSW: reworked class DELAYED_MESSAGE_TO_LH to keep data pointer intact


Known Bugs:
===========

	None



***************************
CDMA2000 4x50.A82
***************************

Date:	June 18, 2008

Base:	V4.51
MMI:	2.99J
LH:	V2.86m	V12
	X3.23k	V22

General Remarks
===============

	This release of CDMA2000 software is based on the CMU base system V4.51
	and can be installed together with other V4.51 compatible function groups.

Enhancements:
=============

	None


Known Bugs:
===========

	None



***************************
CDMA2000 5x00.A42
***************************

Date:	June 18, 2008

Base:	5x00.A40
MMI:	2.99J
LH:	V2.86m	V12
	X3.23j	V22

General Remarks
===============

	This release of CDMA2000 software is based on the CMU base system 5x00.A40
	and can be installed together with other 5x00.A40 compatible function groups.


Enhancements:
=============

	Corrected sasflash version


Known Bugs:
===========

	DSP-Crash when call has been up for several hours



***************************
CDMA2000 5x00.A41
***************************

Date:	June 14, 2008

Base:	5x00.A40
MMI:	2.99J
LH:	V2.86j	V12
	X3.23j	V22

General Remarks
===============

	This release of CDMA2000 software is based on the CMU base system 5x00.A40
	and can be installed together with other 5x00.A40 compatible function groups.


Enhancements:
=============

	FSW: Param Connect_Gbl_SignallingInfo_Used_ProtocolRevision instantiated


Known Bugs:
===========

	DSP-Crash when call has been up for several hours



***************************
CDMA2000 4x50.A81
***************************

Date:	June 11, 2008

Base:	V4.51
MMI:	2.99J
LH:	V2.86m  V12
	X3.23j  V22

General Remarks
===============

	This release of CDMA2000 software is based on the CMU base system V4.51
	and can be installed together with other V4.51 compatible function groups.

Enhancements:
=============

	FSW: Fixed Vocoder Failure


Known Bugs:
===========

	None




***************************
CDMA2000 5x00.A40
***************************

Date:	June 6, 2008

Base:	5x00.A40
MMI:	2.99J
LH:	V2.86j  V12
	X3.23h  V22

General Remarks
===============

	This release of CDMA2000 software is based on the CMU base system 5x00.A40
	and can be installed together with other 5x00.A40 compatible function groups.


Enhancements:
=============

	FSW: Fixed teleserviceId from file format for SMS messages
	FSW: MO binary SMS does not get truncated [PR #465]
	FSW: Fix for "custom generator failed" in B96 selftest



Known Bugs:
===========

	DSP-Crash when call has been up for several hours



***************************
CDMA2000 4x50.A80
***************************

Date:	June 6, 2008

Base:	V4.51
MMI:	2.99J
LH:	V2.86m  V12
	X3.23h  V22

General Remarks
===============

	This release of CDMA2000 software is based on the CMU base system V4.51
	and can be installed together with other V4.51 compatible function groups.
	Note: there is no version 4x50.A79

Enhancements:
=============

	FSW: Fixed teleserviceId from file format for SMS messages
	FSW: MO binary SMS does not get truncated [PR #465]
	FSW: Fix for "custom generator failed" in B96 selftest


Known Bugs:
===========

	None



***************************
CDMA2000 4x50.A78
***************************

Date:	June 5, 2008

Base:	V4.51
MMI:	2.99J
LH:	V2.86m  V12
	X3.23h  V22

General Remarks
===============

	This release of CDMA2000 software is based on the CMU base system V4.51
	and can be installed together with other V4.51 compatible function groups.


Enhancements:
=============

	These fixes were brought over from the 5x00 branch and now exist in the 4x50 branch:

	FSW: Fixed update of CDMA2000 Signalling Output Power when Frequency Dependent Attenuation is enabled
	FSW: Implemented multiple data lines for SMS messages
	FSW: Corrected calculation of quantity of bytes sent to LH for Unicode SMS message
	FSW: Implemented teleserviceId from file format for SMS messages
	FSW: Implemented Event Register bits AMES and RMES for SMS messaging
	LH:  Removed pop-up message box displayed to indicate MMS sent notification
	LH:  Increased Caller ID string size from 11 (10 chars) to 33 (32 chars) [PR #460]
	MMI: Increased Caller ID string size from 11 (10 chars) to 33 (32 chars) [PR #460]
	Fixed Audio File Names

Known Bugs:
===========

	Bug 465: MO Binary SMS message is being truncated



***************************
CDMA2000 4x50.A77
***************************

Date:	June 4, 2008

Base:	V4.51
MMI:	2.99G
LH:	V2.86k  V12
	X3.23g  V22

General Remarks
===============

	This release of CDMA2000 software is based on the CMU base system V4.51
	and can be installed together with other V4.51 compatible function groups.


Enhancements:
=============

	LH:  Added support to send all 8 teleservice IDs to the mobile using the sendSMS.exe application
	LH:  Fixed PREV 4 problem (phone was not establishing a call on a PREV 4 base station)
	LH:  Added functionality to ignore ALL access probe messages from the mobile (previously the LH just rejected the Registration msg)


Known Bugs:
===========

	None



***************************
CDMA2000 5x00.A35
***************************

Date:	May 15, 2008

Base:	5x00.A35
MMI:	2.99H
LH:	V2.86j  V12
	X3.23d  V22

General Remarks
===============

	This release of CDMA2000 software is based on the CMU base system 5x00.A35
	and can be installed together with other 5x00.A35 compatible function groups.


Enhancements:
=============

	FSW: Implemented Event Register bits AMES and RMES for SMS messaging


Known Bugs:
===========

	These three bugs will be fixed in the next MMI release (2.99I)
		Bug 408: cdma2k SMS File selection text is incorrect
		Bug 460: Caller ID string Entry Field too short
		Bug 465: MO Binary SMS message is being truncated
	DSP-Crash when call has been up for several hours



***************************
CDMA2000 4x50.A76
***************************

Date:	May 13, 2008

Base:	V4.51
MMI:	2.99G
LH:	V2.86h  V12
	X3.23d  V22

General Remarks
===============

	This release of CDMA2000 software is based on the CMU base system V4.51
	and can be installed together with other V4.51 compatible function groups.


Enhancements:
=============

	Removes the MMS message sent notification pop up on CMU.


Known Bugs:
===========

	None



***************************
CDMA2000 4x30.B03
***************************

Date:	May 7, 2008

Base:	V4.35
MMI:	2.99A
LH:	V2.84q  V12
	V3.18x  V22

General Remarks
===============

	This release of CDMA2000 software is based on the CMU base system V4.35
	and can be installed together with other V4.35 compatible function groups.


Enhancements:
=============

        FSW: Redesigned path transfer in linkhandler interface to fix netclock issues
	     when coming from any other function group


Known Bugs:
===========

	None



***************************
CDMA2000 4x30.B02
***************************

Date:	April 29, 2008

Base:	V4.35
MMI:	2.99A
LH:	V2.84q  V12
	V3.18x  V22

General Remarks
===============

	This release of CDMA2000 software is based on the CMU base system V4.35
	and can be installed together with other V4.35 compatible function groups.


Enhancements:
=============

        FSW: corrected OLTR lower limit line calculation
        FSW: implemented bandclass handoff fix


Known Bugs:
===========

	None



***************************
CDMA2000 5x00.A28
***************************

Date:	April 25, 2008

Base:	5x00.A25
MMI:	2.99H
LH:	V2.86j  V12
	X3.23d  V22

General Remarks
===============

	This release of CDMA2000 software is based on the CMU base system 5x00.A25
	and can be installed together with other 5x00 compatible function groups.

	Version 5x00.A27 was corrupt and was deleted!!!


Enhancements:
=============

	LH:  Removed pop-up message box displayed to indicate MMS sent notification
	FSW: Corrected calculation of quantity of bytes sent to LH for Unicode SMS message


Known Bugs:
===========

	DSP-Crash when call has been up for several hours



***************************
CDMA2000 4x30.B01
***************************

Date:	April 24, 2008

Base:	V4.35
MMI:	2.99A
LH:	V2.84q  V12
	V3.18x  V22

General Remarks
===============

	This release of CDMA2000 software is based on the CMU base system V4.35
	and can be installed together with other V4.35 compatible function groups.


Enhancements:
=============

	Redesigned path transfer in linkhandler interface to fix netclock
	issues when coming from alien function groups.


Known Bugs:
===========

	None



***************************
CDMA2000 4x30.A99
***************************

Date:	April 22, 2008

Base:	V4.35
MMI:	2.99A
LH:	V2.84q  V12
	V3.18x  V22

General Remarks
===============

	This release of CDMA2000 software is based on the CMU base system V4.35
	and can be installed together with other V4.35 compatible function groups.


Enhancements:
=============

	Fixes a Bandclass handoff problem discovered at Samsung


Known Bugs:
===========

	None



***************************
CDMA2000 5x00.A26
***************************

Date:	April 17, 2008

Base:	5x00.A25
MMI:	2.99H
LH:	V2.86j  V12
	X3.23c  V22

General Remarks
===============

	This release of CDMA2000 software is based on the CMU base system 5x00.A25
	and can be installed together with other 5x00 compatible function groups.


Enhancements:
=============

	Fixed Audio File Names

Known Bugs:
===========

	DSP-Crash when call has been up for several hours



***************************
CDMA2000 4x50.A75
***************************

Date:	April 14, 2008

Base:	V4.51
MMI:	2.99G
LH:	V2.86h  V12
	X3.22h  V22

General Remarks
===============

	This release of CDMA2000 software is based on the CMU base system V4.51
	and can be installed together with other V4.51 compatible function groups.


Enhancements:
=============

	Redesigned path transfer in linkhandler interface to fix netclock
	issues when coming from alien function groups.

Known Bugs:
===========

	None





***************************
CDMA2000 5x00.A21
***************************

Date:	April 10, 2008

Base:	5x00.A20
MMI:	2.99H
LH:	V2.86h  V12
	X3.23a  V22

General Remarks
===============

	This release of CDMA2000 software is based on the CMU base system 5x00.A20
	and can be installed together with other 5x00 compatible function groups.


Enhancements:
=============

	LH: Increased Caller ID string size from 11 (10 chars) to 33 (32 chars)


Known Bugs:
===========

	None



***************************
CDMA2000 4x30.A98
***************************

Date:	April 9, 2008

Base:	V4.35
MMI:	2.99A
LH:	V2.84d  V12
	V3.18W  V22

General Remarks
===============

	This release of CDMA2000 software is based on the CMU base system V4.35
	and can be installed together with other V4.35 compatible function groups.

	Engineering build only.


Enhancements:
=============

	Fixes a linkhandler crash that occurs when the netclock hasn't had time to settle
	yet during the change of function groups.

Known Bugs:
===========

	Access Probes meas must be restarted after SigOff/SigOn Cycle



***************************
CDMA2000 5x00.A20
***************************

Date:	April 9, 2008

Base:	5x00.A20
MMI:	2.99H
LH:	V2.86h  V12
	X3.22h  V22

General Remarks
===============

	This release of CDMA2000 software is based on the CMU base system 5x00.A20
	and can be installed together with other 5x00 compatible function groups.


Enhancements:
=============

	MMI: Increased Caller ID string size from 11 (10 chars) to 33 (32 chars)


Known Bugs:
===========

	None



***************************
CDMA2000 4x30.A97
***************************

Date:	April 7, 2008

Base:	V4.35
MMI:	2.99A
LH:	V2.84d  V12
	V3.18W  V22

General Remarks
===============

	This release of CDMA2000 software is based on the CMU base system V4.35
	and can be installed together with other V4.35 compatible function groups.

	Engineering build only.


Enhancements:
=============

	Hopefully a bug fix for a rare error (path manager error in linkhandler
 	interface) at Samsung,

Known Bugs:
===========

	Access Probes meas must be restarted after SigOff/SigOn Cycle



***************************
CDMA2000 5x00.A15
***************************

Date:	March 20, 2008

Base:	5x00.A15
MMI:	2.99G
LH:	V2.86h  V12
	X3.22h  V22

General Remarks
===============

	This release of CDMA2000 software is based on the CMU base system 5x00.A15
	and can be installed together with other 5x00 compatible function groups.


Enhancements:
=============

	FSW: Implemented multiple data lines for SMS messages
	FSW: Implemented size checks for binary and unicode SMS messages


Known Bugs:
===========

	None



***************************
CDMA2000 4x50.A74
***************************

Date:	March 4, 2008

Base:	V4.51
MMI:	2.99G
LH:	V2.86a  V12
	X3.22c  V22

General Remarks
===============

	This release of CDMA2000 software is based on the CMU base system V4.51
	and can be installed together with other V4.51 compatible function groups.


Enhancements:
=============

	FSW: Fixed Interband Handoffs
	LH: Fixed TCP/IP timeout for remote CMU connection
	LH: boot ROM changes in Yetifsh.fw to fix B83 boot failures during continous self test
             1. Finalized MPC8540 Errata DDR11
             2. Disabled the DDR SDRAM interface logic prior to configuring the memory controller.


Known Bugs:
===========

	None





***************************
CDMA2000 5x00.A01
***************************

Date:	February 27, 2008

Base:	5x00.A01
MMI:	2.99G
LH:	V2.86a  V12
	X3.22a  V22

General Remarks
===============

	This release of CDMA2000 software is based on the CMU base system 5x00.A01
	and can be installed together with other 5x00 compatible function groups.


Enhancements:
=============

	FSW: Fixed update of CDMA2000 Signalling Output Power when Frequency Dependent Attenuation is enabled


Known Bugs:
===========

	None



***************************
CDMA2000 4x50.A73
***************************

Date:	February 25, 2008

Base:	V4.51
MMI:	2.99G
LH:	V2.86a  V12
	X3.22a  V22

General Remarks
===============

	This release of CDMA2000 software is based on the CMU base system V4.51
	and can be installed together with other V4.51 compatible function groups.


Enhancements:
=============

	FSW: fixed B88 Netclock race condition
	FSW: added capability to bypass version mismatch check


Known Bugs:
===========

	None



***************************
CDMA2000 4x50.A72
***************************

Date:	February 21, 2008

Base:	V4.51
MMI:	2.99G
LH:	V2.86a  V12
	X3.22a  V22

General Remarks
===============

	This release of CDMA2000 software is based on the CMU base system V4.51
	and can be installed together with other V4.51 compatible function groups.


Enhancements:
=============

	LH:  Fix to prevent the Link Handler crash during function group change
	FSW: PDSN configuration parameters for PDSN mode, ports and addresses are now common to all CDMA and EVDO function groups
	FSW: Bandclass handoff within a function group is now supported


Known Bugs:
===========

	None



***************************
CDMA2000 4x50.A70
***************************

Date:	February 11, 2008

Base:	V4.51
MMI:	2.99G
LH:	V2.85p  V12
	X3.20q  V22

General Remarks
===============

	This release of CDMA2000 software is based on the CMU base system V4.51
	and can be installed together with other V4.51 compatible function groups.


Enhancements:
=============

	LH:  Fixed PDSN parameter initialization problem
	FSW: Added teleservice ID handling for SMS messaging


Known Bugs:
===========

	None



***************************
CDMA2000 4x50.A64
***************************

Date:	January 24, 2008

Base:	V4.51
MMI:	2.99G
LH:	V2.85L  V12
	X3.20L  V22

General Remarks
===============

	This release of CDMA2000 software is based on the CMU base system V4.51
	and can be installed together with other V4.51 compatible function groups.


Enhancements:
=============

	LH:  Fix to properly initialize a CMU configured with a B83V22 board without the B89 module
	LH:  Fix to prevent an unnecessary LH initiated dropped call when the user changing the call lost detect timer while in a connection with active RL traffic
	FSW: Fixed crash on reboot after use of Frequency Dependent Attenuation
	FSW: Optimized power level changes to improve response time
	FSW: Optimized power level changes when Power Control Bits are All Up or All Down and signalling is OFF


Known Bugs:
===========

	None



***************************
CDMA2000 4x50.A63
***************************

Date:	January 18, 2008

Base:	V4.51
MMI:	2.99F
LH:	V2.85j  V12
	X3.20j  V22

General Remarks
===============

	This release of CDMA2000 software is based on the CMU base system V4.51
	and can be installed together with other V4.51 compatible function groups.


Enhancements:
=============

	FSW: removed CHECK from method clear_resource_notifier_drain in file sigctl.cpp


Known Bugs:
===========

	None



***************************
CDMA2000 4x50.A62
***************************

Date:	January 17, 2008

Base:	V4.51
MMI:	2.99F
LH:	V2.85j  V12
	X3.20j  V22

General Remarks
===============

	This release of CDMA2000 software is based on the CMU base system V4.51
	and can be installed together with other V4.51 compatible function groups.


Enhancements:
=============

	corrected binary SMS message problem with value 0x00
	enabled SMS message file copy into CMU cdma2k directory
	created default mobile max power limit when maxEIRP report is disabled



Known Bugs:
===========

	None



***************************
CDMA2000 4x50.A61
***************************

Date:	January 11, 2008

Base:	V4.51
MMI:	2.99F
LH:	V2.85i  V12
	X3.20i  V22

General Remarks
===============

	This release of CDMA2000 software is based on the CMU base system V4.51
	and can be installed together with other V4.51 compatible function groups.


Enhancements:
=============

	Bug# 449 - Crash when creating SO33 service option
	Fix bootup problem when CMU is configured for Dynamic mode addressing and no DHCP server is connected to the CMU
	Fix for path manager crash when switching function groups in remote mode due to path allocation request timeout


Known Bugs:
===========

	None



***************************
CDMA2000 4x50.A60
***************************

Date:	January 4, 2008

Base:	V4.51
MMI:	2.99F
LH:	V2.85f  V12
	X3.20d  V22

General Remarks
===============

	This release of CDMA2000 software is based on the CMU base system V4.51
	and can be installed together with other V4.51 compatible function groups.


Enhancements:
=============

	Implemented "MEID pending" message for certain phones


Known Bugs:
===========

	None



***************************
CDMA2000 4x50.A59
***************************

Date:	January 1, 2008

Base:	V4.51
MMI:	2.99E
LH:	V2.85f  V12
	X3.20d  V22

General Remarks
===============

	This release of CDMA2000 software is based on the CMU base system V4.51
	and can be installed together with other V4.51 compatible function groups.

	This is another feature complete build checking that we are ready for a release candidate

Enhancements:
=============

	None

Known Bugs:
===========

	None



***************************
CDMA2000 4x50.A58
***************************

Date:	December 20, 2007

Base:	V4.51
MMI:	2.99C
LH:	V2.85f  V12
	X3.20d  V22

General Remarks
===============

	This release of CDMA2000 software is based on the CMU base system V4.51
	and can be installed together with other V4.51 compatible function groups.

	This is another feature complete build checking that we are ready for a release candidate

Enhancements:
=============

	None

Known Bugs:
===========

	None



***************************
CDMA2000 4x50.A57
***************************

Date:	December 18, 2007

Base:	V4.51
MMI:	2.99C
LH:	V2.85e  V12
	X3.20b  V22

General Remarks
===============

	This release of CDMA2000 software is based on the CMU base system V4.51
	and can be installed together with other V4.51 compatible function groups.

	This is another feature complete build checking that we are ready for a release candidate

Enhancements:
=============

    LH:  Web Server up and running on V22
    Undo alert state call release
    Add disconnect / abort to registered state


Known Bugs:
===========

	None



***************************
CDMA2000 4x50.A56
***************************

Date:	December 14, 2007

Base:	V4.51
MMI:	2.99C
LH:	V2.84p  V12
	X3.19t  V22

General Remarks
===============

	This release of CDMA2000 software is based on the CMU base system V4.51
	and can be installed together with other V4.51 compatible function groups.

	This is another feature complete build checking that we are ready for a release candidate

Enhancements:
=============

	Bug# 444: replace suspended "Connect MS" while paging (MMI change)


Known Bugs:
===========

	None



***************************
CDMA2000 4x50.A54
***************************

Date:	December 12, 2007

Base:	V4.51
MMI:	2.99B
LH:	V2.84p  V12
	X3.19r  V22

General Remarks
===============

	This release of CDMA2000 software is based on the CMU base system V4.51
	and can be installed together with other V4.51 compatible function groups.

	This is another feature complete build checking that we are ready for a release candidate

Enhancements:
=============

	None (EVDO changes only)


Known Bugs:
===========

	None



***************************
CDMA2000 4x30.A96
***************************

Date:	December 11, 2007

Base:	4x30.A95
MMI:	2.99A
LH:	V2.84d  V12
	V3.18W  V22

General Remarks
===============

	This release of CDMA2000 software is based on the CMU base system 4x30.A95
	and can be installed together with other 4x30.95 compatible function groups.

	Engineering build only.


Enhancements:
=============

	Improvements to the Yeti flash for V22:
	1. Wrong LongCodeMask being generated on SCH channel when PLCM Derivation set to MEID preferred.
	2. Ignore incoming Page at mobile which caused LH to block and FSW to hang in call setup state.


Known Bugs:
===========

	Access Probes meas must be restarted after SigOff/SigOn Cycle



***************************
CDMA2000 4x50.A49
***************************

Date:	December 5, 2007

Base:	V4.51
MMI:	2.99B
LH:	V2.84p  V12
	X3.19q  V22

General Remarks
===============

	This release of CDMA2000 software is based on the CMU base system V4.51
	and can be installed together with other V4.51 compatible function groups.

	This is another feature complete build checking that we are ready for a release candidate

Enhancements:
=============

	Removed erroneous local environment message in OLTR measurement
	Increased FER report interval rate (Motorola problem)


Known Bugs:
===========

	None



***************************
CDMA2000 4x50.A48
***************************

Date:	November 29, 2007

Base:	V4.51
MMI:	2.99B
LH:	V2.84p  V12
	X3.19q  V22

General Remarks
===============

	This release of CDMA2000 software is based on the CMU base system V4.51
	and can be installed together with other V4.51 compatible function groups.

	This is another feature complete build checking that we are ready for a release candidate

Enhancements:
=============

	None (LH and FSW changes for EVDO)

Known Bugs:
===========

	None



***************************
CDMA2000 4x50.A47
***************************

Date:	November 28, 2007

Base:	V4.51
MMI:	2.99B
LH:	V2.84p  V12
	V3.19L  V22

General Remarks
===============

	This release of CDMA2000 software is based on the CMU base system V4.51
	and can be installed together with other V4.51 compatible function groups.

	This is another feature complete build checking that we are ready for a release candidate

Enhancements:
=============

	None (LH and FSW changes for EVDO)

Known Bugs:
===========

	None



***************************
CDMA2000 4x50.A46
***************************

Date:	November 16, 2007

Base:	V4.51
MMI:	2.99B
LH:	V2.84p  V12
	V3.19g  V22

General Remarks
===============

	This release of CDMA2000 software is based on the CMU base system V4.51
	and can be installed together with other V4.51 compatible function groups.

	This is another feature complete build checking that we are ready for a release candidate

Enhancements:
=============

	None (LH changes for EVDO)

Known Bugs:
===========

	None



***************************
CDMA2000 4x50.A45
***************************

Date:	November 15, 2007

Base:	V4.51
MMI:	2.99B
LH:	V2.84o  V12
	V3.19f  V22

General Remarks
===============

	This release of CDMA2000 software is based on the CMU base system V4.51
	and can be installed together with other V4.51 compatible function groups.

	This is another feature complete build checking that we are ready for a release candidate

Enhancements:
=============

	Fixed Remote mode timeout for Access Probe Meas

Known Bugs:
===========

	None



***************************
CDMA2000 4x50.A44
***************************

Date:	November 13, 2007

Base:	V4.51
MMI:	2.99B
LH:	V2.84n  V12
	V3.19e  V22

General Remarks
===============

	This release of CDMA2000 software is based on the CMU base system V4.51
	and can be installed together with other V4.51 compatible function groups.

	This is a feature complete build checking that we are ready for a release candidate

Enhancements:
=============

	Remove support for PDSN mode on B83 V12 boards
	Fix for PPP state display
	Fix establishment of SO33 connections on the B83V12
	Fix a problem with the interface to the SMS Windows application (requested by OnStar)
	Band Class 15 handoffs now work

Known Bugs:
===========

	None





***************************
CDMA2000 4x50.A43
***************************

Date:	November 12, 2007

Base:	V4.51
MMI:	2.99B
LH:	X2.84L  V12
	X3.19c  V22

General Remarks
===============

	This release of CDMA2000 software is based on the CMU base system V4.51
	and can be installed together with other V4.51 compatible function groups.

	Engineering build for debugging purposes only.


Enhancements:
=============

	Added Select_SoftwareOptions_Enable_Feature_PDSNModes to V22_Only_Options table


Known Bugs:
===========

	None




***************************
CDMA2000 4x50.A42
***************************

Date:	November 6, 2007

Base:	4x50.A40
MMI:	2.99B
LH:	X2.84l  V12
	X3.19c  V22

General Remarks
===============

	This release of CDMA2000 software is based on the CMU base system 4x50.A40
	and can be installed together with other 4x50.A40 compatible function groups.

	Engineering build for debugging purposes only.


Enhancements:
=============

	Access Probe Standby Level response for high power BS settings improved.


Known Bugs:
===========

	None





***************************
CDMA2000 4x50.A41
***************************

Date:	October 30, 2007

Base:	4x50.A40
MMI:	2.99B
LH:	V2.84f  V12
	V3.18b  V22

General Remarks
===============

	This release of CDMA2000 software is based on the CMU base system 4x50.A40
	and can be installed together with other 4x50.A40 compatible function groups.

	Engineering build only.


Enhancements:
=============

	Access Probe meas has been enhanced
	Fix for address problem with SMS windows application
	Changed how the LH reports MS Band Class 7-15  ( support to the FSW )
	Sig Off/On problem ASP meas restart is fixed (LH corrected trigger routing failure at re-initialization)


Known Bugs:
===========

	None



***************************
CDMA2000 4x30.A95
***************************

Date:	October 2, 2007

Base:	4x30.A95
MMI:	2.99A
LH:	V2.84d  V12
	X3.18u  V22

General Remarks
===============

	This release of CDMA2000 software is based on the CMU base system 4x30.A95
	and can be installed together with other 4x30.95 compatible function groups.

	Engineering build only.


Enhancements:
=============

	Access Probes changes backed out of LH build


Known Bugs:
===========

	Access Probes meas must be restarted after SigOff/SigOn Cycle



***************************
CDMA2000 4x30.A94
***************************

Date:	October 1, 2007

Base:	4x30.A90
MMI:	2.99A
LH:	V2.84d  V12
	X3.18t  V22

General Remarks
===============

	This release of CDMA2000 software is based on the CMU base system 4x30.A90
	and can be installed together with other 4x30.90 compatible function groups.

	Engineering build only.


Enhancements:
=============

	Speech Activity Display fixed after Handoffs


Known Bugs:
===========

	Access Probes meas must be restarted after SigOff/SigOn Cycle





***************************
CDMA2000 4x30.A93
***************************

Date:	September 28, 2007

Base:	4x30.A90
MMI:	2.99A
LH:	V2.84d  V12
	X3.18s  V22

General Remarks
===============

	This release of CDMA2000 software is based on the CMU base system 4x30.A90
	and can be installed together with other 4x30.90 compatible function groups.

	Engineering build only.


Enhancements:
=============

	unicode char qty corrected for SMS messages
	B88 NSig generator (recently broken) is functional again


Known Bugs:
===========

	Access Probes meas must be restarted after SigOff/SigOn Cycle





***************************
CDMA2000 4x30.A91
***************************

Date:	September 27, 2007

Base:	4x30.A90
MMI:	2.99A
LH:	V2.84d  V12
	X3.18r  V22

General Remarks
===============

	This release of CDMA2000 software is based on the CMU base system 4x30.A90
	and can be installed together with other 4x30.90 compatible function groups.

	Engineering build only.


Enhancements:
=============

	LH fix for erroroneous Calibration message due to loss of I2C bus

Known Bugs:
===========

	Access Probes meas must be restarted after SigOff/SigOn Cycle





***************************
CDMA2000 4x30.A90
***************************

Date:	September 26, 2007

Base:	4x30.A90
MMI:	2.99A
LH:	V2.84d  V12
	X3.18p  V22

General Remarks
===============

	This release of CDMA2000 software is based on the CMU base system 4x30.A90
	and can be installed together with other 4x30.90 compatible function groups.

	Engineering build only.


Enhancements:
=============

	LH fix for erroroneous Calibration message due to loss of I2C bus
	Ping Measurement working properly

Known Bugs:
===========

	None



***************************
CDMA2000 4x30.A86
***************************

Date:	September 21, 2007

Base:	4x30.A85
MMI:	2.99A
LH:	V2.84d  V12
	X3.18o  V22

General Remarks
===============

	This release of CDMA2000 software is based on the CMU base system 4x30.A85
	and can be installed together with other 4x30.85 compatible function groups.

	It is a release candidate for the V4.35

Enhancements:
=============

	Same as 4x30.B85

Known Bugs:
===========

	None



***************************
CDMA2000 4x30.A85
***************************

Date:	September 20, 2007

Base:	4x30.A85
MMI:	2.99A
LH:	V2.84d  V12
	X3.18o  V22

General Remarks
===============

	This release of CDMA2000 software is based on the CMU base system 4x30.A85
	and can be installed together with other 4x30.85 compatible function groups.


Enhancements:
=============

	Introduced the new external PDSN feature which allows the CMU to be configured as a PDSN server or client
	New remote commands for "Retain_B83_timing_reference"
	PR 402 : Unicode data in SMS msg not being passed to mobile properly
	PR 407 : Mobile's In Use Protocol Revision not updated after handoff
	PR 410 : Changing SO68 Encode Rate drops SO2 Call
	PR 412 : SMS call ID not being sent properly


Known Bugs:
===========

	None



***************************
CDMA2000 4X40.D05
***************************

Date:	August 22, 2007

Base:	4x40.D05
MMI:	2.98R
LH:	V2.84b  V12
	X3.18L  V22

General Remarks
===============

	This 4x40 release of CDMA2000 software is based on the CMU base system 4x40.D05
	and can be installed together with other 4x40.D05 compatible function groups.


Enhancements:
=============

	SMS copy feature implemented with unique function group directories
	RFL registration moved for Smart Align meas


Known Bugs:
===========

	None



***************************
CDMA2000 4X30.A60
***************************

Date:	July 20, 2007

Base:	V4.30
MMI:	2.98R
LH:	V2.84b  V12
	X3.18L  V22

General Remarks
===============

	This release of CDMA2000 software is based on the CMU base system V4.30
	and can be installed together with other V4.30 compatible function groups.

	This is an engineering release candidate for the V4.32

Enhancements:
=============

	Same as 4x30.A56 except with versions.cnf file update correctly
	PDSN params instanciated, but not implemented at this time


Known Bugs:
===========

	None



***************************
CDMA2000 4X30.A56
***************************

Date:	July 19, 2007

Base:	V4.30
MMI:	2.98R
LH:	V2.84b  V12
	X3.18L  V22

General Remarks
===============

	This release of CDMA2000 software is based on the CMU base system V4.30
	and can be installed together with other V4.30 compatible function groups.

	This is an engineering release candidate for the V4.32

Enhancements:
=============

	SMS changes implemented:
	- new directories for out_msg files
	- reload button implemented correctly
	- Unicode and Binary SMS messages are now being sent correctly to mobile
	B85V22 vocoder properly being detected


Known Bugs:
===========

	None



***************************
CDMA2000 4X30.A55
***************************

Date:   July 11, 2007

Base:   V4.30
MMI:    2.98R
LH:     V2.83t  V12
	X3.18g  V22

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system V4.30
        and can be installed together with other V4.30 compatible function groups.

	This is an engineering release

Enhancements:
=============

	changed Check to Check_Repair for SigFer unknown message handling
	ensure generator is ON before setting or resetting the Low Spur Mode


Known Bugs:
===========

	None



***************************
CDMA2000 4X30.A54
***************************

Date:   July 9, 2007

Base:   V4.30
MMI:    2.98R
LH:     V2.83t  V12
	X3.18g  V22

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system V4.30
        and can be installed together with other V4.30 compatible function groups.

	This is an engineering release

Enhancements:
=============

	Speech Activity Display bugs (Bug #397)
	- reset counters when starting the Speech Activity Measurement
	- count blanked frames in the FL
	- prevent the measurement from running if not in a speech call
	SMS outgoing files included in version install directories

Known Bugs:
===========

	None



***************************
CDMA2000 4X30.A53
***************************

Date:   July 2, 2007

Base:   V4.30
MMI:    2.98R
LH:     V2.83r  V12
	X3.18e  V22

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system V4.30
        and can be installed together with other V4.30 compatible function groups.

	This is an engineering release

Enhancements:
=============

	Low Spur mode implemented (Caution: Not thoroughly tested yet. An RxTx board of Rev 13 or higher is needed.)


Known Bugs:
===========

	None



***************************
CDMA2000 4X30.A52
***************************

Date:   June 26, 2007

Base:   V4.30
MMI:    2.98Q
LH:     V2.83o  V12
	X3.18b  V22

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system V4.30
        and can be installed together with other V4.30 compatible function groups.

	This is an engineering release

Enhancements:
=============

	Smart Align - FDA block in SA mode fixed


Known Bugs:
===========

	IP_PAR Null Pointer Red Box results from interrupted hybrid synch process



***************************
CDMA2000 4X30.A51
***************************

Date:   June 20, 2007

Base:   V4.30
MMI:    2.98Q
LH:     V2.83N  V12
	X3.18A  V22

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system V4.30
        and can be installed together with other V4.30 compatible function groups.

	This is an engineering release

Enhancements:
=============

	Speech Activity Display enabled.
	Speech Activity Display throughput statistics correction
	PLCM Memory Leak fixed
	MEID update for Signal Off/On


Known Bugs:
===========

	IP_PAR Null Poiner Red Box results from interrupted hybrid synch process



***************************
CDMA2000 4X30.A50
***************************

Date:   June 19, 2007

Base:   V4.30
MMI:    2.98Q
LH:     V2.83K  V12
	X3.17V  V22

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system V4.30
        and can be installed together with other V4.30 compatible function groups.

	This is an engineering release

Enhancements:
=============

	Fix of freezing interband handoff

Known Bugs:
===========

	IP_PAR Null Poiner Red Box results from interrupted hybrid synch process



***************************
CDMA2000 4X30.A49
***************************

Date:   June 19, 2007

Base:   V4.30
MMI:    2.98Q
LH:     V2.83K  V12
	X3.17V  V22

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system V4.30
        and can be installed together with other V4.30 compatible function groups.

	This is an engineering release

Enhancements:
=============

	Fix of Samsung paging issues

Known Bugs:
===========

	IP_PAR Null Poiner Red Box results from interrupted hybrid synch process



***************************
CDMA2000 4X30.A48
***************************

Date:   June 12, 2007

Base:   V4.30
MMI:    2.98P
LH:     V2.83k  V12
	X3.17t  V22

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system V4.30
        and can be installed together with other V4.30 compatible function groups.

	This is an engineering release

Enhancements:
=============

	Speech Activity meas enhanced
	K87 problems have been fixed


Known Bugs:
===========

	Speech Activity meas:  MMI fields not complete for Reverse Thruput
	IP_PAR Null Poiner Red Box results from interrupted hybrid synch process



***************************
CDMA2000 4X30.A47
***************************

Date:   June 8, 2007

Base:   V4.30
MMI:    2.98o
LH:     V2.83e  V12
	X3.17n  V22

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        V4.30 and can be installed together with other V4.30 compatible
	function groups.

	This is an engineering release

Enhancements:
=============

	GPIB script was enhanced for MEID problem
	Speech Activity meas enabled


Known Bugs:
===========

	in Speech Activity meas:
		(1) MMI fields not complete
		(2) the data will not reset when the meas is turned off
		(3) the meas does not go to HALT when the call is not established




***************************
CDMA2000 4X30.A46
***************************

Date:   June 4, 2007

Base:   V4.30
MMI:    2.98N
LH:     V2.82v  V12
	X3.17a  V22

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        V4.30 and can be installed together with other V4.30 compatible
	function groups.

	This is an engineering release

Enhancements:
=============

	SMS unicode bug fix
	DHCP bug fix for failure scenario


Known Bugs:
===========

	None



***************************
CDMA2000 4X30.A45
***************************

Date:   May 25, 2007

Base:   V4.30
MMI:    2.98M
LH:     V2.82r  V12
	X3.16s  V22

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        V4.30 and can be installed together with other V4.30 compatible
	function groups.

	This is an engineering release

Enhancements:
=============

	Bug #381:  cdma2k system time GPIB commands added
	Bug #380:  Booting up in dynamic IP addressing mode fails

Known Bugs:
===========

	Binary SMS known problems:
	-a- binary SMS Reload switch causes File selection to go gray (need to reset to turn black again)
	-b- outgoing unicode msg from file does not convert the data correctly

	Service cfg --> Service Option 68 --> Average Encoding Rate is not being sent to the vocoder
	    before the call is established. It is only being sent when the Avg Encoding Rate is changes,
	    so there is a possibility that the MMI and vocoder can get out of sync. The problem may not
	    be noticable, as the vocoder should continue to sound normal.
	Without a new LH build the SO68 settings cannot be changed while in another service option
		or the LH will crash.



***************************
CDMA2000 4X30.A44
***************************

Date:   May 24, 2007

Base:   V4.30
MMI:    2.98M
LH:     V2.82r  V12
	X3.16s  V22

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        V4.30 and can be installed together with other V4.30 compatible
	function groups.

	This is an engineering release

Enhancements:
=============

	Bug #373  cdma2k system time GPIB commands added
	Bug #378  changes/enhancement for binary SMS
	redesign for binary SMS complete
	SO68/EVRC-B/4GV included in this release


Known Bugs:
===========

	Binary SMS known problems:
	-a- binary SMS Reload switch causes File selection to go gray (need to reset to turn black again)
	-b- outgoing unicode msg from file does not convert the data correctly

	Service cfg --> Service Option 68 --> Average Encoding Rate is not being sent to the vocoder
	    before the call is established. It is only being sent when the Avg Encoding Rate is changes,
	    so there is a possibility that the MMI and vocoder can get out of sync. The problem may not
	    be noticable, as the vocoder should continue to sound normal.
	Can *NOT* bring up CMU in Dynamic IP Mode (will cause red box)



***************************
CDMA2000 4X30.A43
***************************

Date:   May 15, 2007

Base:   V4.30
MMI:    2.98L
LH:     V2.82q  V12
	X3.16r  V22

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        V4.30 and can be installed together with other V4.30 compatible
	function groups.

	This is an engineering release

Enhancements:
=============

        Binary SMS code implemented for incoming & outgoing messages
	New vocoder DLD files used that modified DMA/ESSI sync sequence on B85v22 vocoder


Known Bugs:
===========

	Binary SMS known problems:
	- Preview of outgoing file info not implemented
	- Formatting of input message does not match that of outgoing message
	- Reload function does not work correctly
	- Outgoing SMS buffer is not cleared before writing
	- Load Error comes up as the default for outgoing message From File (believed to be an MMI problem)



***************************
CDMA2000 4X30.A42
***************************

Date:   May 7, 2007

Base:   V4.30
MMI:    2.98K
LH:     V2.82p  V12
	X3.16q  V22

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        V4.30 and can be installed together with other V4.30 compatible
	function groups.

	This is an engineering release

Enhancements:
=============

        New In-Traffic System Parameters message for passing SID/NID information after a handoff
        Fix for avoiding FATAL when receive invalid Band Subclass information from the MS
        Fix for Status Response memory leak


Known Bugs:
===========

	None



***************************
CDMA2000 4X40.C01
***************************

Date:   May 7, 2007

Base:   4x40.C01
MMI:    2.98K
LH:     V2.82L  V12
	X3.16I  V22

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        4x40.C01 and can be installed together with other 4x40.C01 compatible
	function groups.

	This is an engineering release

Enhancements:
=============

	None

Known Bugs:
===========

	None



***************************
CDMA2000 4X30.A41
***************************

Date:   April 25, 2007

Base:   V4.30
MMI:    2.98E
LH:     V2.82J  V12
	V3.15P  V22

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        V4.30 and can be installed together with other V4.30 compatible
	function groups.

	The version has been built directly on the CDMA2000 V4.31 with Smart Alignment changes added.

	!!! This is a ONLY test build for Clark Conrad and the Motorola folks.

Enhancements:
=============

	Modified Smart Align commands to the CoPro in drpv_tsk.cpp

Known Bugs:
===========

	None



***************************
CDMA2000 4X30.A40
***************************

Date:   April 24, 2007

Base:   V4.30
MMI:    2.98J
LH:     V2.82L  V12
	X3.16L  V22

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        V4.30 and can be installed together with other V4.30 compatible
	function groups.

	The version has been built directly on the CDMA2000 V4.30 with some bug fixes.

	!!! This is a ONLY test build for Rolf Lorenzen and the new EVDO power measurement !!!

Enhancements:
=============

	None

Known Bugs:
===========

	None



***************************
CDMA2000 4X30.A39
***************************

Date:   April 17, 2007

Base:   V4.30
MMI:    2.98E
LH:     V2.82J  V12
	V3.15P  V22

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        V4.30 and can be installed together with other V4.30 compatible
	function groups.

	The version has been built directly on the CDMA2000 V4.30 with some bug fixes.

	This is a release candidate for the V4.31

Enhancements:
=============

	Fixes of some memory leaks

	Vocoder fix

Known Bugs:
===========

	None



***************************
CDMA2000 4X40.B35
***************************

Date:   April 17, 2007

Base:   4x40.B35
MMI:    2.98J
LH:     V2.82L  V12
	X3.16L  V22

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        4x40.B35 and can be installed together with other 4x40.B35 compatible
	function groups.

	This is an engineering release

Enhancements:
=============

	Sync now checks for external reference frequency.

	Else, identical to 4x30.A38

Known Bugs:
===========

	None



***************************
CDMA2000 4X30.A38
***************************

Date:   April 16, 2007

Base:   V4.30
MMI:    2.98J
LH:     V2.82L  V12
	X3.16L  V22

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        V4.30 and can be installed together with other V4.30 compatible
	function groups.

	This is an engineering release

Enhancements:
=============

	Bug 333: Enumerated values for Preamble Length message to LH
	Bug 347: Changing CDMA System Time causes red box
	Binary & Unicode SMS works for outgoing messages; source can be internal or file


Known Bugs:
===========

	None



***************************
CDMA2000 4X30.A37
***************************

Date:   April 12, 2007

Base:   V4.30
MMI:    2.98E
LH:     V2.82J  V12
	V3.15P  V22

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        V4.30 and can be installed together with other V4.30 compatible
	function groups.

	The version has been built directly on the CDMA2000 V4.30 with some bug fixes.

	This is a release candidate for the V4.31

Enhancements:
=============

	Improvements for the continuous self test and compensation for LH boot problems

	Bug fixes for sigping

Known Bugs:
===========

	None



***************************
CDMA2000 4X30.A36
***************************

Date:   April 9, 2007

Base:   V4.30
MMI:    2.98I
LH:     V2.82L  V12
	X3.16j  V22

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        V4.30 and can be installed together with other V4.30 compatible
	function groups.

	This is an engineering release

Enhancements:
=============

	Fixed crashes of B96 self test when B83 reboot freezes.
	Repair attempts in the linkhandler interface when B83 reboot freezes.
	SigPing now sends only one Echo request to the linkhandler (BSC/CNTL), instead of one for each possible sector/channel combination.


Known Bugs:
===========

	None



***************************
CDMA2000 4X30.A35
***************************

Date:   April 3, 2007

Base:   V4.30
MMI:    2.98I
LH:     V2.82L  V12
	X3.16j  V22

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        V4.30 and can be installed together with other V4.30 compatible
	function groups.

	This is an engineering release

Enhancements:
=============

	Bug 337: GPIB command for MEID inquiry has been added
	CONFigure:NETWork:CINDicator:CID GPIB command now works


Known Bugs:
===========

	None



***************************
CDMA2000 4X30.A34
***************************

Date:   March 30, 2007

Base:   V4.30
MMI:    2.98H
LH:     V2.82L  V12
	X3.16j  V22

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        V4.30 and can be installed together with other V4.30 compatible
	function groups.

	This is an engineering release

Enhancements:
=============

	None


Known Bugs:
===========

	None



***************************
CDMA2000 4X30.A33
***************************

Date:   March 28, 2007

Base:   V4.30
MMI:    2.98H
LH:     V2.82L  V12
	X3.16j  V22

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        V4.30 and can be installed together with other V4.30 compatible
	function groups.

	This is an engineering release

Enhancements:
=============

	Fixed B96 self test code problems


Known Bugs:
===========

	None



***************************
CDMA2000 4X30.A32
***************************

Date:   March 27, 2007

Base:   V4.30
MMI:    2.98H
LH:     V2.82L  V12
	X3.16j  V22

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        V4.30 and can be installed together with other V4.30 compatible
	function groups.

	This is an engineering release

Enhancements:
=============

	Trigger debounce added for PvF as well as Smart Align meas
	Added new params for binary SMS: code only partially implemented


Known Bugs:
===========

	None



***************************
CDMA2000 4X30.A31
***************************

Date:   March 22, 2007

Base:   V4.30
MMI:    2.98H
LH:     V2.82L  V12
	X3.16j  V22

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        V4.30 and can be installed together with other V4.30 compatible
	function groups.

	This is an engineering release

Enhancements:
=============

	Bug 311: despreading in IQRF Analyzer meas responds to data rate changes
	Bug 332: Tx measurements (and trigger) now working


Known Bugs:
===========

	None



***************************
CDMA2000 4X30.A30
***************************

Date:   March 21, 2007

Base:   V4.30
MMI:    2.98H
LH:     V2.82L  V12
	X3.16j  V22

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        V4.30 and can be installed together with other V4.30 compatible
	function groups.

	This is an engineering release

Enhancements:
=============

	CR# 324: Binary SMS: params and enums added in MMI


Known Bugs:
===========

	None



***************************
CDMA2000 4X30.A29
***************************

Date:   March 14, 2007

Base:   V4.30
MMI:    2.98G
LH:     V2.82L  V12
	X3.16g  V22

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        V4.30 and can be installed together with other V4.30 compatible
	function groups.

	This is an engineering release

Enhancements:
=============

	Ping Config Menu showed small "CDMA2000" in the header



Known Bugs:
===========

	None


***************************
CDMA2000 4X30.A28
***************************

Date:   March 9, 2007

Base:   V4.30
MMI:    2.98G
LH:     V2.82L  V12
	X3.16f  V22

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        V4.30 and can be installed together with other V4.30 compatible
	function groups.

	This is an engineering release

Enhancements:
=============

	Fixed some memory leaks

	Changed NSig AWGN to limit Connectors


Known Bugs:
===========

	None


***************************
CDMA2000 4X30.A27
***************************

Date:   March 6, 2007

Base:   V4.30
MMI:    2.98G
LH:     V2.82L  V12
	X3.16e  V22

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        V4.30 and can be installed together with other V4.30 compatible
	function groups.

	This is an engineering release

Enhancements:
=============

	SO68 Vocoder selection activated  (CR #306)


Known Bugs:
===========

	None



***************************
CDMA2000 4X30.A26
***************************

Date:   February 27, 2007

Base:   V4.30
MMI:    2.98F
LH:     V2.82k V12
	X3.16c  V22

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        V4.30 and can be installed together with other V4.30 compatible
	function groups.

	This is an engineering release

Enhancements:
=============

	Origination address for SMS
	Unicode / Hindi SMS support

Known Bugs:
===========

	None



***************************
CDMA2000 4X30.A25
***************************

Date:   February 23, 2007

Base:   4x30.A20
MMI:    2.98F
LH:     V2.82k V12
	X3.16b  V22

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        4x30.A20 and can be installed together with V4.30 or other 4x30.A20
        function groups.

	This is an engineering release

Enhancements:
=============

	Origination address for SMS
	Unicode / Hindi SMS support

Known Bugs:
===========

	None



***************************
CDMA2000 4X30.A24
***************************

Date:   February 14, 2007

Base:   V4.30
MMI:    2.98E
LH:     V2.82j V12
	V3.15p V22

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        V4.30 and can be installed together with other V4.30 function
        groups.

	This is an engineering release

Enhancements:
=============

	None

Known Bugs:
===========

	None



***************************
CDMA2000 4X30.A23
***************************

Date:   February 5, 2007

Base:   V4.30
MMI:    2.98E
LH:     V2.82j V12
	V3.15p V22

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        V4.30 and can be installed together with other V4.30 function
        groups.

	This is a release candidate for the V4.30

Enhancements:
=============

	None

Known Bugs:
===========

	None



***************************
CDMA2000 4X30.A22
***************************

Date:   February 2, 2007

Base:   4x30.A16
MMI:    2.98E
LH:     V2.82j V12
	V3.15p V22

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        4x30.A16 and can be installed together with other 4x30.A16 function
        groups.

	This is a release candidate for the V4.30

Enhancements:
=============

	None

Known Bugs:
===========

	None



***************************
CDMA2000 4X30.A21
***************************

Date:   February 2, 2007

Base:   4x30.A16
MMI:    2.98E
LH:     V2.82i V12
	V3.15o V22

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        4x30.A16 and can be installed together with other 4x30.A16 function
        groups.

	This is an engineering version for internal use only.

Enhancements:
=============

	None

Known Bugs:
===========

	None



***************************
CDMA2000 4X30.A20
***************************

Date:   February 1, 2007

Base:   4x30.A16
MMI:    2.98E
LH:     V2.82i V12
	V3.15o V22

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        4x30.A16 and can be installed together with other 4x30.A16 function
        groups.

	This is an engineering version for internal use only.

Enhancements:
=============

	None

Known Bugs:
===========

	None



***************************
CDMA2000 4X30.A19
***************************

Date:   January 29, 2007

Base:   4x30.A16
MMI:    2.98E
LH:     V2.82i V12
	V3.15n V22

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        4x30.A15 and can be installed together with other 4x30.A15 function
        groups.

	This is an engineering version for internal use only.

Enhancements:
=============

	Final bug fixes for the Qualcomm Smart Alignment issues.



Known Bugs:
===========

	None



***************************
CDMA2000 4X30.A18
***************************

Date:   January 26, 2007

Base:   4x30.A15
MMI:    2.98E
LH:     V2.82G V12
	V3.15L V22

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        4x30.A15 and can be installed together with other 4x30.A15 function
        groups.

	This is an engineering version for internal use only.

Enhancements:
=============

	Hopefully bug fixes for the Qualcomm Smart Alignment issues

	Fix of the CMUgo error

Known Bugs:
===========

	None


***************************
CDMA2000 4X30.A17
***************************

Date:   January 26, 2007

Base:   4x30.A15
MMI:    2.98E
LH:     V2.82G V12
	V3.15L V22

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        4x30.A15 and can be installed together with other 4x30.A15 function
        groups.

	This is an engineering version for internal use only.

Enhancements:
=============

	Hopefully bug fixes for the Qualcomm Smart Alignment issues

	Fix of the CMUgo error

Known Bugs:
===========

	None



***************************
CDMA2000 4X20.B9B
***************************

Date:   January 25, 2007

Base:   V4.24
MMI:    2.95G
LH:     V2.83  V12
	V3.05h V22

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        V4.24 and can be installed together with other V4.24 function groups.


Enhancements:
=============

	Fix in large MS originated SMS

	Fix in smart alignment measurement

Known Bugs:
===========

	None



***************************
CDMA2000 4X30.A16
***************************

Date:   January 23, 2007

Base:   4x30.A15
MMI:    2.98E
LH:     V2.82G V12
	V3.15L V22

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        4x30.A15 and can be installed together with other 4x30.A15 function
        groups.

	This is an engineering version for internal use only.

Enhancements:
=============

	Some improvements in SO68

Known Bugs:
===========

	A rare system hang in signaling, when changing band classes
	A Qualcomm script makes the system react sluggish in non-sig
	A CMUgo script leads to a 100% reproduceable crash



***************************
CDMA2000 4X30.A15
***************************

Date:   January 22, 2007

Base:   4x30.A15
MMI:    2.98E
LH:     V2.82f V12
	V3.15k V22

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        4x30.A15 and can be installed together with other 4x30.A15 function
        groups.

	This is an engineering version for internal use only.

Enhancements:
=============

	SO68 works now

	Long received SMS won't crash anymore

Known Bugs:
===========

    	Message hangs in LH when So68 encoder rate or execute buttons are used.
		- Workaround is to end the call at the phone.




***************************
CDMA2000 4X30.A10
***************************

Date:   January 18, 2007

Base:   4x30.A05
MMI:    2.98E
LH:     V2.82d V12
	V3.15h V22

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        4x30.A10 and can be installed together with other 4x30.A10 function
        groups.

	This is an engineering version for internal use only.

Enhancements:
=============

	SO68 improvements

	Fix in Smart Alignment remote mode

Known Bugs:
===========

    	Message hangs in LH when So68 encoder rate or execute buttons are used.
		- Workaround is to end the call at the phone.




***************************
CDMA2000 4X30.A08
***************************

Date:   January 15, 2007

Base:   4x30.A05
MMI:    2.98D
LH:     V2.82d V12
	V3.15h V22

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        4x30.A05 and can be installed together with other 4x30.A05 function
        groups.

	This is an engineering version for internal use only.

Enhancements:
=============

	So68 initial implementation

Known Bugs:
===========

    	Message hangs in LH when So68 encoder rate or execute buttons are used.
		- Workaround is to end the call at the phone.




***************************
CDMA2000 4X30.A07
***************************

Date:   January 10, 2007

Base:   4x30.A05
MMI:    2.98C
LH:     V2.82C V12
	V3.15e V22

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        4x30.A05 and can be installed together with other 4x30.A05 function
        groups.

	This is an engineering version for internal use only.

Enhancements:
=============

	More logging and debugging code for Smart Alignment Measurement

Known Bugs:
===========

    	Bugs according to current state of product support database




***************************
CDMA2000 4X30.A06
***************************

Date:   January 9, 2007

Base:   4x30.A05
MMI:    2.98C
LH:     V2.82C V12
	V3.15e V22

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        4x30.A05 and can be installed together with other 4x30.A05 function
        groups.

	This is an engineering version for internal use only.

Enhancements:
=============

	Bug fix for Smart Alignment Measurement

Known Bugs:
===========

    	Bugs according to current state of product support database






***************************
CDMA2000 4X30.A05
***************************

Date:   January 8, 2007

Base:   4x30.A05
MMI:    2.98C
LH:     V2.82C V12
	V3.15e V22

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        4x30.A05 and can be installed together with other 4x30.A05 function
        groups.

	This is an engineering version for internal use only.

Enhancements:
=============

	B85 V22 vocoder for B89 is now being identified

Known Bugs:
===========

    	Bugs according to current state of product support database






***************************
CDMA2000 4X30.A01
***************************

Date:   January 5, 2007

Base:   4x30.A01
MMI:    2.98C
LH:     V2.82C V12
	V3.15e V22

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        4x30.A01 and can be installed together with other 4x30.A01 function
        groups.

	This is an engineering version for internal use only.

Enhancements:
=============

	SO68 MMI, not yet supported by FSW

Known Bugs:
===========

    	Bugs according to current state of product support database






***************************
CDMA2000 4X20.C20
***************************

Date:   January 3, 2007

Base:   V4.24
MMI:    2.98B
LH:     V2.82C V12
	V3.15e V22

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        V4.24 and can be installed together with other V4.24 function
        groups.

	This is an engineering version for internal use only.

Enhancements:
=============

	Correction for improper firmware in 4x20.C19 build

Known Bugs:
===========

    	Bugs according to current state of product support database






***************************
CDMA2000 4X20.C19
***************************

Date:   December 21, 2006

Base:   V4.24
MMI:    2.98B
LH:     V2.82C V12
	V3.15e V22

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        V4.24 and can be installed together with other V4.24 function
        groups.

	This is an engineering version for internal use only.

Enhancements:
=============

	None

Known Bugs:
===========

    	Bugs according to current state of product support database






***************************
CDMA2000 4X20.C18
***************************

Date:   December 20, 2006

Base:   V4.24
MMI:    2.98B
LH:     V2.82C V12
	V3.15e V22

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        V4.24 and can be installed together with other V4.24 function
        groups.

	This is an engineering version for internal use only.

Enhancements:
=============

	None

Known Bugs:
===========

    	Bugs according to current state of product support database





***************************
CDMA2000 4X20.C17
***************************

Date:   December 19, 2006

Base:   V4.24
MMI:    2.98B
LH:     V2.82C V12
	V3.15c V22

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        V4.24 and can be installed together with other V4.24 function
        groups.

	This is an engineering version for internal use only.

Enhancements:
=============

	Bug fixes for hybrid mode.

	MMI enhancements for smart alignment measurement

Known Bugs:
===========

    	Bugs according to current state of product support database





***************************
CDMA2000 4X20.C16
***************************

Date:   December 14, 2006

Base:   4x20.C15
MMI:    2.98A
LH:     V2.82C V12
	V3.15b V22

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        4x20.C15 and can be installed together with other 4x20.C15 function
        groups.

	This is an engineering version for presentation purposes only.

Enhancements:
=============

	None

Known Bugs:
===========

    	Bugs according to current state of product support database





***************************
CDMA2000 4X20.C15
***************************

Date:   December 13, 2006

Base:   4x20.C15
MMI:    2.98A
LH:     V2.82C V12
	V3.15W V22

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        4x20.C15 and can be installed together with other 4x20.C15 function
        groups.

	This is an engineering version for presentation purposes only.

Enhancements:
=============

	Some time sync improvements

Known Bugs:
===========

    	Bugs according to current state of product support database





***************************
CDMA2000 4X20.C12
***************************

Date:   December 4, 2006

Base:   4x20.C10
MMI:    2.98A
LH:     V2.82A V12
	V3.05W V22

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        4x20.C10 and can be installed together with other 4x20.C10 function
        groups.

	This is an engineering version for presentation purposes only.

Enhancements:
=============

	Improvements in CDMA2000 system time setting

Known Bugs:
===========

    	Bugs according to current state of product support database





***************************
CDMA2000 4X20.B9A
***************************

Date:   November 30, 2006

Base:   V4.20
MMI:    2.95G
LH:     V2.82c V12
	V3.05f V22

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        V4.20 and can be installed together with other V4.20 function groups.
	It is a release candidate for the V4.22 release.


Enhancements:
=============

	New drc2kmod.dld file for Min Power enhancements.  This version will ignore
	any vocoder attached to it.


Known Bugs:
===========

    	Bugs according to current state of Bugzilla database.




***************************
CDMA2000 4X20.C11
***************************

Date:   November 30, 2006

Base:   4x20.C10
MMI:    2.95G
LH:     V2.82A V12
	V3.05W V22

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        4x20.C10 and can be installed together with other 4x20.C10 function
        groups.

	This is an engineering version for presentation purposes only.

Enhancements:
=============

	None

Known Bugs:
===========

    	Bugs according to current state of product support database





***************************
CDMA2000 4X20.C10
***************************

Date:   November 29, 2006

Base:   4x20.C10
MMI:    2.95G
LH:     V2.82A V12
	V3.05W V22

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        4x20.C10 and can be installed together with other 4x20.C10 function
        groups.

	This is an engineering version for presentation purposes only.

Enhancements:
=============

	None

Known Bugs:
===========

    	Bugs according to current state of product support database





***************************
CDMA2000 4X20.C09
***************************

Date:   November 28, 2006

Base:   4x20.C05
MMI:    2.95G
LH:     V2.82A V12
	V3.05B V22

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        4x20.C05 and can be installed together with other 4x20.C05 function
        groups.


Enhancements:
=============

	This is a special release for testing the new V22 version of the B85 option (Vocoder)
        It is not a release candidate.

Known Bugs:
===========

    	Bugs according to current state of product support database





***************************
CDMA2000 4X20.C08
***************************

Date:   November 22, 2006

Base:   V4.20
MMI:    2.95G
LH:     V2.82c V12
	V3.05d V22

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        V4.20 and can be installed together with other V4.20 function groups.
	It is a release candidate for the V4.22 release.


Enhancements:
=============

	New LH firmware fixes Event Triggers and Slot Trigger

Known Bugs:
===========

    	Bugs according to current state of Bugzilla database.



***************************
CDMA2000 4X20.C07
***************************

Date:   November 21, 2006

Base:   V4.20
MMI:    2.95G
LH:     V2.82B V12
	V3.05C V22

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        V4.20 and can be installed together with other V4.20 function groups.
	It is a release candidate for the V4.22 release.


Enhancements:
=============

	Max Power MMI screen fixed.  New sasflash file needed due to different code base.

Known Bugs:
===========

    	Bugs according to current state of Bugzilla database.




***************************
CDMA2000 4X20.C05
***************************

Date:   November 20, 2006

Base:   4x20.C05
MMI:    2.95G
LH:     V2.82A V12
	V3.05B V22

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        4x20.C05 and can be installed together with other 4x20.C05 function
        groups.


Enhancements:
=============

	Bug fixes

Known Bugs:
===========

    	Bugs according to current state of product support database




***************************
CDMA2000 4X20.C03
***************************

Date:   November 10, 2006

Base:   4x20.C01
MMI:    2.95E
LH:     V2.82A V12
	V3.05A V22

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        4x20.C01 and can be installed together with other 4x20.C01 function
        groups.


Enhancements:
=============

	Switched on Rev A option

Known Bugs:
===========

    	Bugs according to current state of product support database




***************************
CDMA2000 4X20.C02
***************************

Date:   November 6, 2006

Base:   4x20.C01
MMI:    2.95E
LH:     V2.82A V12
	V3.05A V22

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        4x20.C01 and can be installed together with other 4x20.C01 function
        groups.

	This is a release candidate for the V4.22

Enhancements:
=============

	Switched off engineering options

Known Bugs:
===========

    	Bugs according to current state of product support database.





***************************
CDMA2000 4X20.C01
***************************

Date:   November 6, 2006

Base:   4x20.C01
MMI:    2.95E
LH:     V2.82A V12
	V3.05A V22

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        4x20.C01 and can be installed together with other 4x20.C01 function
        groups.


Enhancements:
=============

	Media Flow Time moved and renamed

	Partial B88 Rev. A support

	Bug fixes

Known Bugs:
===========

    	Bugs according to current state of product support database.





***************************
CDMA2000 4X20.B99
***************************

Date:   November 1, 2006

Base:   4x20.B97
MMI:    2.95C
LH:     X2.81K V12
	X3.04G V22

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        4x20.B97 and can be installed together with other 4x20.B97 function
        groups.


Enhancements:
=============

	Several bug fixes

	Improvements in Synchornization

Known Bugs:
===========

    	Bugs according to current state of product support database.





***************************
CDMA2000 4X20.B98
***************************

Date:   October 26, 2006

Base:   4x20.B97
MMI:    2.95C
LH:     X2.81J V12
	X3.04F V22

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        4x20.B97 and can be installed together with other 4x20.B97 function
        groups.


Enhancements:
=============

	GPIB command and bug fixes for external sync parameters

Known Bugs:
===========

    	Bugs according to current state of product support database.





***************************
CDMA2000 4X20.B97
***************************

Date:   October 25, 2006

Base:   4x20.B97
MMI:    2.95B
LH:     X2.81J V12
	X3.04F V22

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        4x20.B97 and can be installed together with other 4x20.B97 function
        groups.


Enhancements:
=============

	External B83 synchronization. Attention: doesn't work with Base 4x20.B97

Known Bugs:
===========

    	Bugs according to current state of product support database.





***************************
CDMA2000 4X20.B95
***************************

Date:   October 19, 2006

Base:   4x20.B95
MMI:    2.95A
LH:     X2.81i V12
	X3.04e V22

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        4x20.B95 and can be installed together with other 4x20.B95 function
        groups.


Enhancements:
=============

	None

Known Bugs:
===========

    	Bugs according to current state of product support database.





***************************
CDMA2000 4X20.B92
***************************

Date:   October 13, 2006

Base:   4x20.B90
MMI:    2.95A
LH:     X2.81G V12
	X3.04C V22

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        4x20.B90 and can be installed together with other 4x20.B90 function
        groups.


Enhancements:
=============

	None

Known Bugs:
===========

    	Bugs according to current state of product support database.




***************************
CDMA2000 4X20.B91
***************************

Date:   October 12, 2006

Base:   4x20.B90
MMI:    2.95A
LH:     V2.81G V12
	V3.04C V22

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        4x20.B90 and can be installed together with other 4x20.B90 function
        groups.


Enhancements:
=============

	Included in the cdma2k MMI:

	MEID support & new parameters
	LH dependent DNS support & new parameters
	Bug fixes


Known Bugs:
===========

    	Bugs according to current state of product support database.




***************************
CDMA2000 4X20.B90
***************************

Date:   October 3, 2006

Base:   4x20.B90
MMI:    2.95A
LH:     V2.81D V12
	V3.04A V22

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        4x20.B90 and can be installed together with other 4x20.B90 function
        groups.


Enhancements:
=============

	Included in the cdma2k MMI:

	MEID support & new parameters
	LH dependent DNS support & new parameters

	Included in the 3.04a Yetiflsh:

	Ability to change system time in EVDO
	Access Channel MAC parameters now configurable
	Access Parameters Overhead message fields configurable
	RLP/IP Throughput measurement
	Mobile IP functionality
	Ping measurement


Known Bugs:
===========

    	Bugs according to current state of product support database.




***************************
CDMA2000 4X20.B83
***************************

Date:   September 26, 2006

Base:   V4.21
MMI:    2.90Q
LH:     V2.81D V12
	V3.03H V22

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        V4.21 and can be installed together with other V4.21 function
        groups.

        This version is a release candidate for V4.21

Enhancements:
=============

	The B83 reboot function was removed from the Continuous Self Test.

Known Bugs:
===========

    	Bugs according to current state of product support database.




***************************
CDMA2000 4X20.B82
***************************

Date:   September 21, 2006

Base:   V4.21
MMI:    2.90Q
LH:     V2.81D V12
	V3.03H V22

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        V4.21 and can be installed together with other V4.21 function
        groups.

        This version is a release candidate for V4.21

Enhancements:
=============

	None since version 4x20.B81

Known Bugs:
===========

    	Bugs according to current state of product support database.




***************************
CDMA2000 4X20.B81
***************************

Date:   September 13, 2006

Base:   V4.20
MMI:    2.90Q
LH:     V2.81C V12
	V3.03G V22

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        V4.20 and can be installed together with other V4.20 function
        groups.

        This version is a release candidate for V4.21

Enhancements:
=============

	Fixed Linkhandler Crash when B83V22 came up in GSM

Known Bugs:
===========

    	Bugs according to current state of product support database.




***************************
CDMA2000 4X20.B79
***************************

Date:   September 1, 2006

Base:   V4.20
MMI:    2.90Q
LH:     V2.81C V12
	V3.03F V22

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        V4.20 and can be installed together with other V4.20 function
        groups.

        This version is a release candidate for V4.20

Enhancements:
=============

	None

Known Bugs:
===========

    	Bugs according to current state of product support database.




***************************
CDMA2000 4X20.B78
***************************

Date:   August 31, 2006

Base:   V4.20
MMI:    2.90Q
LH:     V2.81C V12
	V3.03E V22

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        V4.20 and can be installed together with other V4.20 function
        groups.

        This version is a release candidate for V4.20

Enhancements:
=============

	Fixed a rare linkhandler boot crash

Known Bugs:
===========

    	Bugs according to current state of product support database.




***************************
CDMA2000 4X20.B77
***************************

Date:   August 30, 2006

Base:   V4.20
MMI:    2.90Q
LH:     V2.81B V12
	V3.03D V22

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        V4.20 and can be installed together with other V4.20 function
        groups.

        This version is a release candidate for V4.20

Enhancements:
=============

	Removed red box for uncalibrated linkhandler

Known Bugs:
===========

    	Bugs according to current state of product support database.




***************************
CDMA2000 4X20.B76
***************************

Date:   August 23, 2006

Base:   4x20.B75
MMI:    2.90Q
LH:     V2.81  V12
	V3.03C V22

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        4x20.B75 and can be installed together with other 4x20.B75 function
        groups.

        This version is a release candidate for V4.20

Enhancements:
=============

	One minor bug fix

Known Bugs:
===========

    	Bugs according to current state of product support database.




***************************
CDMA2000 4X20.B75
***************************

Date:   August 22, 2006

Base:   4x20.B75
MMI:    2.90P
LH:     V2.81  V12
	V3.03A V22

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        4x20.B75 and can be installed together with other 4x20.B75 function
        groups.

        This version is a release candidate for V4.20

Enhancements:
=============

	Bug fixes for non-signaling

Known Bugs:
===========

    	Bugs according to current state of product support database.




***************************
CDMA2000 4X20.B72
***************************

Date:   August 18, 2006

Base:   4x20.B70
MMI:    2.90P
LH:     V2.81  V12
	V3.03  V22

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        4x20.B70 and can be installed together with other 4x20.B70 function
        groups.

        This version is a release candidate for V4.20

Enhancements:
=============

        No changes since 4x20.B71 for cdma2000

Known Bugs:
===========

    	Bugs according to current state of product support database.




***************************
CDMA2000 4X20.B71
***************************

Date:   August 17, 2006

Base:   4x20.B70
MMI:    2.90P
LH:     V2.81  V12
	V3.03  V22

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        4x20.B70 and can be installed together with other 4x20.B70 function
        groups.

        This version is a release candidate for V4.20

Enhancements:
=============

	Time Setting for Media Flow improved

	AWGN resolution

Known Bugs:
===========

    	Bugs according to current state of product support database.




***************************
CDMA2000 4X20.B70
***************************

Date:   August 11, 2006

Base:   4x20.B70
MMI:    2.90O
LH:     V2.81  V12
	X3.02I V22

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        4x20.B70 and can be installed together with other 4x20.B70 function
        groups.

        This version is a release candidate for V4.20

Enhancements:
=============

	Time Setting for Media Flow

Known Bugs:
===========

    	Bugs according to current state of product support database.




***************************
CDMA2000 4X20.B66
***************************

Date:   August 3, 2006

Base:   4x20.B65
MMI:    2.90M
LH:     X2.80F V12
	X3.02H V22

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        4x20.B65 and can be installed together with other 4x20.B65 function
        groups.

        This version is an engineering version

Enhancements:
=============

	NSig analyzer frequencies now correct after reboot

Known Bugs:
===========

    	Bugs according to current state of product support database.




***************************
CDMA2000 4X20.B65
***************************

Date:   August 2, 2006

Base:   4x20.B65
MMI:    2.90M
LH:     X2.80F V12
	X3.02H V22

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        4x20.B65 and can be installed together with other 4x20.B65 function
        groups.

        This version is an engineering version

Enhancements:
=============

	None

Known Bugs:
===========

    	Bugs according to current state of product support database.




***************************
CDMA2000 4X15.B71
***************************

Date:   July 26, 2006

Base:   4x15.B70
MMI:    2.71E
LH:     V2.59

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        4x15.B70 and can be installed together with other 4x15.B70 function
	groups.


Enhancements:
=============

	Fixes Bug #94 (genrator crash when waiting for the path)

Known Bugs:
===========

	-/-




***************************
CDMA2000 4X15.B70
***************************

Date:   July 26, 2006

Base:   4x15.B70
MMI:    2.71E
LH:     V2.59

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        4x15.B70 and can be installed together with other 4x15.B70 function
	groups.


Enhancements:
=============

	Support of U99 in Non-signaling

Known Bugs:
===========

	-/-




***************************
CDMA2000 4X20.B56
***************************

Date:   July 25, 2006

Base:   4x20.B55
MMI:    2.90L
LH:     X2.80D V12
	X3.02B V22

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        4x20.B55 and can be installed together with other 4x20.B55 function
        groups.

        This version is an engineering version

Enhancements:
=============

	NonSig Connector limits now support U99 option

Known Bugs:
===========

    	Bugs according to current state of product support database.




***************************
CDMA2000 4X20.B55
***************************

Date:   July 19, 2006

Base:   4x20.B55
MMI:    2.90L
LH:     X2.80D V12
	X3.02A V22

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        4x20.B55 and can be installed together with other 4x20.B55 function
        groups.

        This version is an engineering version

Enhancements:
=============

	None

Known Bugs:
===========

    	Bugs according to current state of product support database.




***************************
CDMA2000 4X20.B50
***************************

Date:   July 13, 2006

Base:   4x20.B50
MMI:    2.90L
LH:     X2.80D V12
	X3.01W V22

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        4x20.B50 and can be installed together with other 4x20.B50 function
        groups.

        This version is an engineering version

Enhancements:
=============

	None

Known Bugs:
===========

    	Bugs according to current state of product support database.




***************************
CDMA2000 4X15.B55
***************************

Date:   July 11, 2006

Base:   4x15.B55
MMI:    2.71E
LH:     V2.59

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        4x15.B55 and can be installed together with other 4x15.B55 function
	groups.


Enhancements:
=============

	-/-

Known Bugs:
===========

	-/-




***************************
CDMA2000 4X20.B46
***************************

Date:   July 7, 2006

Base:   4x20.B45
MMI:    2.90L
LH:     X2.80D V12
	X3.01V V22

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        4x20.B45 and can be installed together with other 4x20.B45 function
        groups.

        This version is an engineering version

Enhancements:
=============

	H-PSK measurements are working again

Known Bugs:
===========

    	Bugs according to current state of product support database.




***************************
CDMA2000 4X20.B45
***************************

Date:   June 30, 2006

Base:   4x20.B45
MMI:    2.90L
LH:     X2.80D V12
	X3.01S V22

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        4x20.B45 and can be installed together with other 4x20.B45 function
        groups.

        This version is an engineering version

Enhancements:
=============

	No new enhancements for this version


Known Bugs:
===========

    	Bugs according to current state of product support database.




***************************
CDMA2000 4X20.B40
***************************

Date:   June 27, 2006

Base:   4x20.B40
MMI:    2.90L
LH:     X2.80D V12
	X3.01R V22

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        4x20.B40 and can be installed together with other 4x20.B40 function
        groups.

        This version is an engineering version

Enhancements:
=============

	Forward Packet Activity param added


Known Bugs:
===========

    	Bugs according to current state of product support database.




***************************
CDMA2000 4X20.B36
***************************

Date:   June 16, 2006

Base:   4x20.B35
MMI:    2.90L
LH:     X2.80D V12
	X3.01Q V22

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        4x20.B35 and can be installed together with other 4x20.B35 function
        groups.

        This version is an engineering version

Enhancements:
=============

	CHAPInterval data type changed
	GPIB channel issue with BC 5

Known Bugs:
===========

    	Bugs according to current state of product support database.




***************************
CDMA2000 4X20.B35
***************************

Date:   June 12, 2006

Base:   4x20.B35
MMI:    2.90K
LH:     X2.80D V12
	X3.01Q V22

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        4x20.B35 and can be installed together with other 4x20.B35 function
        groups.

        This version is an engineering version

Enhancements:
=============

	Output trigger routing fixed

Known Bugs:
===========

    	Bugs according to current state of product support database.




***************************
CDMA2000 4X10.B40
***************************

Date:   June 8, 2006

Base:   4x10.B40
MMI:    2.71E
LH:     V2.59

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        4x10.B40 and can be installed together with other 4x10.B40 function
	groups.


Enhancements:
=============

	Timeouts for system self test delayed in order to support slower CMUs

	Rare invalid memory access for linkhandler error messages fixed


Known Bugs:
===========

	-/-




***************************
CDMA2000 4X20.B30
***************************

Date:   June 05, 2006

Base:   4x20.B30
MMI:    2.90K
LH:     X2.80B V12
	X3.01L V22

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        4x20.B30 and can be installed together with other 4x20.B30 function
        groups.

        This version is an engineering version

Enhancements:
=============

	None

Known Bugs:
===========

	Output trigger routing doesn't work anymore.

    	Bugs according to current state of product support database.




***************************
CDMA2000 4X20.B26
***************************

Date:   May 22, 2006

Base:   4x20.B25
MMI:    2.90J
LH:     X2.80A V12
	X3.01I V22

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        4x20.B25 and can be installed together with other 4x20.B25 function
        groups.

        This version is an engineering version

Enhancements:
=============

	Sasflash (B83V12) now built with old VxWorks. Will hopefully be more stable.

Known Bugs:
===========

    Loading a 4x20 version from a version < 4x20 and vice versa will lead to a crash
	on the first startup.

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.




***************************
CDMA2000 4X10.B25
***************************

Date:   May 15, 2006

Base:   4x10.B25
MMI:    2.71E
LH:     V2.59

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        4x10.B25 and can be installed together with other 4x10.B25 function
	groups.


Enhancements:
=============

	Bugfix for spikes in modulation measurements (new drc2kmod.dld)


Known Bugs:
===========

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.



***************************
CDMA2000 4X20.B25
***************************

Date:   May 12, 2006

Base:   4x20.B25
MMI:    2.90J
LH:     X3.00A V12
	X3.01H V22

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        4x20.B20 and can be installed together with other 4x20.B20 function
        groups.

        This version is an engineering version

Enhancements:
=============

	"Flying" Limit Lines in Channel Power measurement

Known Bugs:
===========

    Even with the new sasflash file, we can still observe occasional linkhandler
	crashes, especially when the B88 is present.

    Loading a 4x20 version from a version < 4x20 and vice versa will lead to a crash
	on the first startup.

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.




***************************
CDMA2000 4X20.B20
***************************

Date:   May 9, 2006

Base:   4x20.B20
MMI:    2.90I
LH:     X3.00A V12
	X3.01G V22

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        4x20.B20 and can be installed together with other 4x20.B20 function
        groups.

        This version is an engineering version

Enhancements:
=============

	"Flying" Limit Lines in Channel Power measurement

Known Bugs:
===========

    Even with the new sasflash file, we can still observe occasional linkhandler
	crashes, especially when the B88 is present.

    Loading a 4x20 version from a version < 4x20 and vice versa will lead to a crash
	on the first startup.

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.




***************************
CDMA2000 4X20.B15
***************************

Date:   April 26, 2006

Base:   4x20.B15
MMI:    2.90G
LH:     X3.00A V12
	X3.01F V22

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        4x20.B15 and can be installed together with other 4x20.B15 function
        groups.

        This version is an engineering version

Enhancements:
=============

	Support of self test with B83v22

Known Bugs:
===========

    Even with the new sasflash file, we can still observe occasional linkhandler
	crashes, especially when the B88 is present.

    Loading a 4x20 version from a version < 4x20 and vice versa will lead to a crash
	on the first startup.

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.




***************************
CDMA2000 4X20.B13
***************************

Date:   April 21, 2006

Base:   4x20.B11
MMI:    2.90G
LH:     X3.00A V12
	X3.01F V22

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        4x20.B11 and can be installed together with other 4x20.B11 function
        groups.

        This version is an engineering version

Enhancements:
=============

	None

Known Bugs:
===========

    Even with the new sasflash file, we can still observe occasional linkhandler
	crashes, especially when the B88 is present.

    Loading a 4x20 version from a version < 4x20 and vice versa will lead to a crash
	on the first startup.

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.




***************************
CDMA2000 4X20.B12
***************************

Date:   April 14, 2006

Base:   4x20.B11
MMI:    2.90G
LH:     X3.00A V12
	X3.01D V22

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        4x20.B11 and can be installed together with other 4x20.B11 function
        groups.

        This version is an engineering version

Enhancements:
=============

	None

Known Bugs:
===========

    Even with the new sasflash file, we can still observe occasional linkhandler
	crashes, especially when the B88 is present.

    Loading a 4x20 version from a version < 4x20 and vice versa will lead to a crash
	on the first startup.

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.




***************************
CDMA2000 4X20.B11
***************************

Date:   April 13, 2006

Base:   4x20.B11
MMI:    2.90G
LH:     X3.00A V12
	X3.01C V22

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        4x20.B11 and can be installed together with other 4x20.B11 function
        groups.

        This version is an engineering version

Enhancements:
=============

	ChannelPower vs. Pilot

Known Bugs:
===========

    Even with the new sasflash file, we can still observe occasional linkhandler
	crashes, especially when the B88 is present.

    Loading a 4x20 version from a version < 4x20 and vice versa will lead to a crash
	on the first startup.

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.




***************************
CDMA2000 4X20.B10
***************************

Date:   April 12, 2006

Base:   4x20.B10
MMI:    2.90F
LH:     X3.00A V12
	X3.01B V22

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        4x20.B10 and can be installed together with other 4x20.B10 function
        groups.

        This version is an engineering version

Enhancements:
=============

	None

Known Bugs:
===========

    Even with the new sasflash file, we can still observe occasional linkhandler
	crashes, especially when the B88 is present.

    Loading a 4x20 version from a version < 4x20 and vice versa will lead to a crash
	on the first startup.

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.




***************************
CDMA2000 4X10.B02
***************************

Date:   April 6, 2006

Base:   4x10.B01
MMI:    2.71E
LH:     V2.59

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        4x10.B01 and can be installed together with other 4x10.B01 function
	groups.

	Release Candidate V4.10

Enhancements:
=============

	No crash if mobile uses ESN as IMSI

	Bugfix for running Power vs. Frame in SON mode


Known Bugs:
===========

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.



***************************
CDMA2000 4X20.B07
***************************

Date:   April 5, 2006

Base:   4x20.B05
MMI:    2.90F
LH:     X3.00A V12
	X3.00F V22

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        4x20.B05 and can be installed together with other 4x20.B05 function
        groups.

        This version is an engineering version

Enhancements:
=============

	None

Known Bugs:
===========

    Even with the new sasflash file, we can still observe occasional linkhandler
	crashes, especially when the B88 is present.

    Loading a 4x20 version from a version < 4x20 and vice versa will lead to a crash
	on the first startup.

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.




***************************
CDMA2000 4X20.B06
***************************

Date:   April 4, 2006

Base:   4x20.B05
MMI:    2.90F
LH:     X3.00A

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        4x20.B05 and can be installed together with other 4x20.B05 function
        groups.

        This version is an engineering version

Enhancements:
=============

	None

Known Bugs:
===========

    Even with the new sasflash file, we can still observe occasional linkhandler
	crashes, especially when the B88 is present.

    Loading a 4x20 version from a version < 4x20 and vice versa will lead to a crash
	on the first startup.

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.




***************************
CDMA2000 4X20.B05
***************************

Date:   March 30, 2006

Base:   4x20.B05
MMI:    2.90F
LH:     X3.00A

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        4x20.B05 and can be installed together with other 4x20.B05 function
        groups.

        This version is an engineering version

Enhancements:
=============

	None

Known Bugs:
===========

    Even with the new sasflash file, we can still observe occasional linkhandler
	crashes, especially when the B88 is present.

    Loading a 4x20 version from a version < 4x20 and vice versa will lead to a crash
	on the first startup.

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.




***************************
CDMA2000 4X10.B01
***************************

Date:   March 29, 2006

Base:   4x10.B01
MMI:    2.71E
LH:     V2.58

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        4x10.B01 and can be installed together with other 4x10.B01 function
	groups.

Enhancements:
=============

	None


Known Bugs:
===========

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.



***************************
CDMA2000 4X20.B03
***************************

Date:   March 29, 2006

Base:   4x20.B01
MMI:    2.90F
LH:     X3.00A

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        4x20.B01 and can be installed together with other 4x20.B01 function
        groups.

        This version is an engineering version

Enhancements:
=============

	None

Known Bugs:
===========

    Even with the new sasflash file, we can still observe occasional linkhandler
	crashes, especially when the B88 is present.

    Loading a 4x20 version from a version < 4x20 and vice versa will lead to a crash
	on the first startup.

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.




***************************
CDMA2000 4X20.B02
***************************

Date:   March 22, 2006

Base:   4x20.B01
MMI:    2.90F
LH:     X3.00A

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        4x20.B01 and can be installed together with other 4x20.B01 function
        groups.

        This version is an engineering version

Enhancements:
=============

	None

Known Bugs:
===========

    Even with the new sasflash file, we can still observe occasional linkhandler
	crashes, especially when the B88 is present.

    Loading a 4x20 version from a version < 4x20 and vice versa will lead to a crash
	on the first startup.

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.




***************************
CDMA2000 4X10.A10
***************************

Date:   March 15, 2006

Base:   4x10.A10
MMI:    2.71E
LH:     V2.58

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        4x10.A10 and can be installed together with other 4x10.A10 function
	groups.

Enhancements:
=============

	None


Known Bugs:
===========

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.



***************************
CDMA2000 4X20.B01
***************************

Date:   March 14, 2006

Base:   4x20.B01
MMI:    2.90F
LH:     X3.00A

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        4x20.B01 and can be installed together with other 4x20.B01 function
        groups.

        This version is an engineering version

Enhancements:
=============

	None

Known Bugs:
===========

    Even with the new sasflash file, we can still observe occasional linkhandler
	crashes, especially when the B88 is present.

    Loading a 4x20 version from a version < 4x20 and vice versa will lead to a crash
	on the first startup.

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.




***************************
CDMA2000 4X20.A31
***************************

Date:   March 9, 2006

Base:   4x20.A30
MMI:    2.90F
LH:     X3.00A

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        4x20.A30 and can be installed together with other 4x20.A30 function
        groups.

        This version is an engineering version

Enhancements:
=============

	None

Known Bugs:
===========

    Even with the new sasflash file, we can still observe occasional linkhandler
	crashes, especially when the B88 is present.

    Loading a 4x20 version from a version < 4x20 and vice versa will lead to a crash
	on the first startup.

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.




***************************
CDMA2000 4X20.A30
***************************

Date:   March 6, 2006

Base:   4x20.A30
MMI:    2.90F
LH:     X3.00A

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        4x20.A30 and can be installed together with other 4x20.A30 function
        groups.

        This version is an engineering version

Enhancements:
=============

	None

Known Bugs:
===========

    Even with the new sasflash file, we can still observe occasional linkhandler
	crashes, especially when the B88 is present.

    Loading a 4x20 version from a version < 4x20 and vice versa will lead to a crash
	on the first startup.

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.




***************************
CDMA2000 4X20.A26
***************************

Date:   February 28, 2006

Base:   4x20.A25
MMI:    2.90E
LH:     X3.00A

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        4x20.A25 and can be installed together with other 4x20.A25 function
        groups.

        This version is an engineering version

Enhancements:
=============

	None

Known Bugs:
===========

    Even with the new sasflash file, we can still observe occasional linkhandler
	crashes, especially when the B88 is present.

    Loading a 4x20 version from a version < 4x20 and vice versa will lead to a crash
	on the first startup.

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.




***************************
CDMA2000 4X20.A25
***************************

Date:   February 17, 2006

Base:   4x20.A25
MMI:    2.90E
LH:     X3.00A

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        4x20.A25 and can be installed together with other 4x20.A25 function
        groups.

        This version is an engineering version

Enhancements:
=============

	Timeout for system selftest fixed (patch)

Known Bugs:
===========

    Even with the new sasflash file, we can still observe occasional linkhandler
	crashes, especially when the B88 is present.

    Loading a 4x20 version from a version < 4x20 and vice versa will lead to a crash
	on the first startup.

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.




***************************
CDMA2000 4X20.A21
***************************

Date:   February 14, 2006

Base:   4x20.A20
MMI:    2.90E
LH:     X3.00A

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        4x20.A20 and can be installed together with other 4x20.A20 function
        groups.

        This version is an engineering version

Enhancements:
=============

	none

Known Bugs:
===========

    Even with the new sasflash file, we can still observe occasional linkhandler
	crashes, especially when the B88 is present.

    Loading a 4x20 version from a version < 4x20 and vice versa will lead to a crash
	on the first startup.

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.




***************************
CDMA2000 4X20.A20
***************************

Date:   February 9, 2006

Base:   4x20.A20
MMI:    2.90E
LH:     X3.00A

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        4x20.A20 and can be installed together with other 4x20.A20 function
        groups.

        This version is an engineering version

Enhancements:
=============

	Improved sasflash, which reduces the amount of linkhandler crashes

Known Bugs:
===========

    Even with the new sasflash file, we can still observe occasional linkhandler
	crashes, especially when the B88 is present.

    Loading a 4x20 version from a version < 4x20 and vice versa will lead to a crash
	on the first startup.

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.




***************************
CDMA2000 4X10.A01
***************************

Date:   February 7, 2005

Base:   4x10.A01
MMI:    2.71E
LH:     V2.58

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        4x10.A01 and can be installed together with other 4x10.A01 function
	groups.

Enhancements:
=============

	None


Known Bugs:
===========

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.



***************************
CDMA2000 4X00.F08
***************************

Date:   January 25, 2005

Base:   V4.00
MMI:    2.71E
LH:     V2.58

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        V4.00 and can be installed together with other V4.00 function
	groups.

	This is a release candidate for V4.01

Enhancements:
=============

	Smart Alignment Measurement is now available with the K80 option


Known Bugs:
===========

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.



***************************
CDMA2000 4X20.A16
***************************

Date:   January 24, 2005

Base:   4x20.A15
MMI:    2.90E
LH:     X2.59C

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        4x20.A15 and can be installed together with other 4x20.A15 function
        groups.

        This version is an engineering version

Enhancements:
=============

	Regular Sasflash, everything should work again

Known Bugs:
===========

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.




***************************
CDMA2000 4X00.F07
***************************

Date:   January 20, 2005

Base:   V4.00
MMI:    2.71E
LH:     V2.58

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        V4.00 and can be installed together with other V4.00 function
	groups.

	This is a release candidate for V4.01

Enhancements:
=============

	Fix of an incompatible drc2kmod.dld version


Known Bugs:
===========

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.



***************************
CDMA2000 3X80.H96
***************************

Date:   January 20, 2005

Base:   3x80.H95
MMI:    2.71E
LH:     V2.58

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3x80.H96 and can be installed together with other 3x80.H96 function
	groups.

        This version is a release candidate for V3.85

Enhancements:
=============

	Fixes yellow boxes which result from an incompatible drc2kmod.dld file


Known Bugs:
===========

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.



***************************
CDMA2000 4X20.A15
***************************

Date:   January 20, 2005

Base:   4x20.A15
MMI:    2.90E
LH:     X2.59C

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        4x20.A15 and can be installed together with other 4x20.A15 function
        groups.

        This version is an engineering version

Enhancements:
=============

	None

Known Bugs:
===========

    Vocoder will not be loaded in this version. This leads to a lot of yellow
	boxes on startup

    Registering in signaling will lead to a linkhandler crash

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.




***************************
CDMA2000 4X00.F06
***************************

Date:   January 12, 2005

Base:   V4.00
MMI:    2.71E
LH:     V2.58

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        V4.00 and can be installed together with other V4.00 function
	groups.

	This is a release candidate for V4.00

Enhancements:
=============

	None


Known Bugs:
===========

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.



***************************
CDMA2000 4X20.A10
***************************

Date:   December 21, 2005

Base:   4x20.A05
MMI:    2.90E
LH:     V2.59C

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        4x20.A10 and can be installed together with other 4x20.A10 function
        groups.

        This version is an engineering version

Enhancements:
=============

	None

Known Bugs:
===========

    Vocoder will not be loaded in this version. This leads to a lot of yellow
	boxes on startup

    Registering in signaling will lead to a linkhandler crash

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.




***************************
CDMA2000 4X20.A05
***************************

Date:   December 15, 2005

Base:   4x20.A05
MMI:    2.90E
LH:     V2.59C

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        4x20.A05 and can be installed together with other 4x20.A05 function
        groups.

        This version is an engineering version

Enhancements:
=============

	None

Known Bugs:
===========

    Vocoder will not be loaded in this version. This leads to a lot of yellow
	boxes on startup

    Registering in signaling will lead to a linkhandler crash

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.




***************************
CDMA2000 4X00.F05
***************************

Date:   December 12, 2005

Base:   4x00.F05
MMI:    2.71E
LH:     V2.58

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        4x00.F05 and can be installed together with other 4x00.F05 function
	groups.

	This is a release candidate for V4.00

Enhancements:
=============

	None


Known Bugs:
===========

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.



***************************
CDMA2000 4X00.F01
***************************

Date:   December 6, 2005

Base:   4x00.F01
MMI:    2.71E
LH:     V2.58

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        4x00.F01 and can be installed together with other 4x00.F01 function
	groups.

	This is an engineering version

Enhancements:
=============

	none - identical to 3x80.H95


Known Bugs:
===========

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.



***************************
CDMA2000 3X80.H95
***************************

Date:   December 5, 2005

Base:   3x80.H95
MMI:    2.71E
LH:     V2.58

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3x80.H95 and can be installed together with other 3x80.H95 function
	groups.

        This version is a release candidate for V3.85

Enhancements:
=============

	Fix in smart alignment measurement for the item.cpp yellow box


Known Bugs:
===========

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.



***************************
CDMA2000 4X20.A01
***************************

Date:   November 30, 2005

Base:   4x20.A01
MMI:    2.90D
LH:     V2.59C

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        4x20.A01 and can be installed together with other 4x20.A01 function
        groups.

        This version is an engineering version

Enhancements:
=============

	None

Known Bugs:
===========

    Vocoder will not be loaded in this version. This leads to a lot of yellow
	boxes on startup

    Registering in signaling will lead to a linkhandler crash

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.




***************************
CDMA2000 3X80.H90
***************************

Date:   November 23, 2005

Base:   3x80.H90
MMI:    2.71E
LH:     V2.58

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3x80.H90 and can be installed together with other 3x80.H80 *and*
        3x80.H90 function groups.

        This version is an engineering version

Enhancements:
=============

	Smart Alignment: Building BASE3X80.H90 with CD2K3X80.H82 code


Known Bugs:
===========

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.



***************************
CDMA2000 3X80.H82
***************************

Date:   November 22, 2005

Base:   3x80.H80
MMI:    2.71E
LH:     V2.58

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3x80.H80 and can be installed together with other 3x80.H80 function
        groups.

        This version is an engineering version

Enhancements:
=============

	Smart Alignment: Recomputed intermediate result delay for PvF meas
                         Changed result_is_valid method to match Smart Align

Known Bugs:
===========

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.




***************************
CDMA2000 3X80.H81
***************************

Date:   November 17, 2005

Base:   3x80.H80
MMI:    2.71E
LH:     V2.58

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3x80.H80 and can be installed together with other 3x80.H80 function
        groups.

        This version is an engineering version

Enhancements:
=============

	Smart Alignment: Recomputed intermediate result delay

Known Bugs:
===========

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.





***************************
CDMA2000 3X80.H80
***************************

Date:   November 16, 2005

Base:   3x80.H80
MMI:    2.71E
LH:     V2.58

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3x80.H80 and can be installed together with other 3x80.H80 function
        groups.

        This version is an engineering version

Enhancements:
=============

	(Final?) improvements in smart alignment measurement

Known Bugs:
===========

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.





***************************
CDMA2000 4X00.D11
***************************

Date:   November 11, 2005

Base:   4x00.D10
MMI:    2.90C
LH:     V2.59A

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        4x00.D10 and can be installed together with other 4x00.D10 function
        groups.

        This version is an engineering version

Enhancements:
=============

	None

Known Bugs:
===========

    Vocoder will not be loaded in this version. This leads to a lot of yellow
	boxes on startup

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.




***************************
CDMA2000 4X00.D10
***************************

Date:   November 8, 2005

Base:   4x00.D10
MMI:    2.90C
LH:     V2.59A

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        4x00.D10 and can be installed together with other 4x00.D10 function
        groups.

        This version is an engineering version

Enhancements:
=============

	None

Known Bugs:
===========

    Vocoder will not be loaded in this version. This leads to a lot of yellow
	boxes on startup

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.




***************************
CDMA2000 3X80.H73
***************************

Date:   October 27, 2005

Base:   3x80.H70
MMI:    2.71E
LH:     V2.58

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3x80.H70 and can be installed together with other 3x80.H70 function
        groups.

        This version is an engineering version

Enhancements:
=============

	Smart Alignment measurement uses its own dld file again, so it works
		together with WCDMA


Known Bugs:
===========

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.





***************************
CDMA2000 3X80.H72
***************************

Date:   October 26, 2005

Base:   3x80.H70
MMI:    2.71E
LH:     V2.58

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3x80.H70 and can be installed together with other 3x80.H70 function
        groups.

        This version is an engineering version

Enhancements:
=============

	Smart Alignment: fix for lower tx connector limits
			 improvement of trigger timeout setting (not complete yet)


Known Bugs:
===========

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.





***************************
CDMA2000 4X00.D05
***************************

Date:   October 26, 2005

Base:   4x00.DO5
MMI:    2.90C
LH:     V2.58

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        4x00.D01 and can be installed together with other 4x00.D01 function
        groups.

        This version is an engineering version

Enhancements:
=============

	Smaller MMI improvements & FSW cleanup

Known Bugs:
===========

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.




***************************
CDMA2000 3X80.H71
***************************

Date:   October 20, 2005

Base:   3x80.H71
MMI:    2.71E
LH:     V2.58

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3x80.H70 and can be installed together with other 3x80.H70 function
        groups.

        This version is an engineering version

Enhancements:
=============

	MMI fix for Smart alignment measurement

Known Bugs:
===========

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.





***************************
CDMA2000 4X00.D02
***************************

Date:   October 19, 2005

Base:   4x00.DO1
MMI:    2.90B
LH:     V2.58

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        4x00.D01 and can be installed together with other 4x00.D01 function
        groups.

        This version is an engineering version

Enhancements:
=============

	None

Known Bugs:
===========

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.




***************************
CDMA2000 3X80.H70
***************************

Date:   October 18, 2005

Base:   3x80.H70
MMI:    2.71D
LH:     V2.58

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3x80.H70 and can be installed together with other 3x80.H70 function
        groups.

        This version is an engineering version

Enhancements:
=============

	Removed hang in smart alignment measurement/nsig generator on a reset

Known Bugs:
===========

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.





***************************
CDMA2000 4X00.D01
***************************

Date:   October 12, 2005

Base:   4x00.DO1
MMI:    2.90B
LH:     V2.58

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        4x00.D01 and can be installed together with other 4x00.D01 function
        groups.

        This version is an engineering version

Enhancements:
=============

	None

Known Bugs:
===========

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.




***************************
CDMA2000 3X80.H65
***************************

Date:   October 7, 2005

Base:   3x80.H65
MMI:    2.71D
LH:     V2.58

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3x80.H65 and can be installed together with other 3x80.H65 function
        groups.

        This version is an engineering version

Enhancements:
=============

	Some smart alignment improvements

Known Bugs:
===========

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.





***************************
CDMA2000 4X00.C11
***************************

Date:   September 20, 2005

Base:   4x00.C10
MMI:    2.90B
LH:     V2.58

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        4x00.C10 and can be installed together with other 4x00.C10 function
        groups.

        This version is an engineering version

Enhancements:
=============

	Smart Alignment improvements

        Fixes for existing and new CD2K LH board detection


Known Bugs:
===========

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.




***************************
CDMA2000 3X80.H62
***************************

Date:   September 23, 2005

Base:   3x80.H60
MMI:    2.71C
LH:     V2.58

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3x80.H60 and can be installed together with other 3x80.H60 function
        groups.

        This version is an engineering version

Enhancements:
=============

	Smart Alignment now supports PCS frequency settings

Known Bugs:
===========

    Motorola V60 gets muted when it receives a call waiting message. This may be a
	phone issue.

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.





***************************
CDMA2000 3X80.H15
***************************

Date:   september 23, 2005

Base:   3x80.H11
MMI:    2.70M
LH:     V2.58

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3x80.H11 and can be installed together with other 3x80.H11 function
        groups.

        This version is a release candidate for V3.81

Enhancements:
=============

	Smart Alignment switched off, as this is a release candidate for V3.81

	Bug fix for an uninitialized pointer access in linkhandler interface

	Bug fix for "unknown call type" in signaling

	Bug fix for faulty environment switching in signaling

	Bug fix for faulty trigger settings in NonSig-NPM


Known Bugs:
===========

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.





***************************
CDMA2000 4X00.C10
***************************

Date:   September 20, 2005

Base:   4x00.C10
MMI:    2.90A
LH:     V2.58

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        4x00.C10 and can be installed together with other 4x00.C10 function
        groups.

        This version is an engineering version

Enhancements:
=============

	First integration


Known Bugs:
===========

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.





***************************
CDMA2000 3X80.H61
***************************

Date:   September 20, 2005

Base:   3x80.H60
MMI:    2.71C
LH:     V2.58

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3x80.H60 and can be installed together with other 3x80.H60 function
        groups.

        This version is an engineering version

Enhancements:
=============

	Smart Alignment improvements, especially close to connector limits

Known Bugs:
===========

    Motorola V60 gets muted when it receives a call waiting message. This may be a
	phone issue.

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.





***************************
CDMA2000 3X80.H60
***************************

Date:   September 16, 2005

Base:   3x80.H60
MMI:    2.71C
LH:     V2.58

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3x80.H60 and can be installed together with other 3x80.H60 function
        groups.

        This version is an engineering version

Enhancements:
=============

	Smart Alignment activated again, some improvements regarding connector limits

Known Bugs:
===========

    Motorola V60 gets muted when it receives a call waiting message. This may be a
	phone issue.

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.





***************************
CDMA2000 3X80.H56
***************************

Date:   September 15, 2005

Base:   3x80.H55
MMI:    2.71B
LH:     V2.58

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3x80.H55 and can be installed together with other 3x80.H55 function
        groups.

        This version is an engineering version

Enhancements:
=============

	Fixed Samsung bug "segment.c" (uninitialized pointer in lh_itrfc.cpp)

	Fixed LG bug "sig_gmem.cpp" (late call reconfiguration message)

	Deactivated smart alignment measurement for engineering release

Known Bugs:
===========

    Motorola V60 gets muted when it receives a call waiting message. This may be a
	phone issue.

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.





***************************
CDMA2000 3X80.H55
***************************

Date:   September 9, 2005

Base:   3x80.H55
MMI:    2.71B
LH:     V2.58

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3x80.H55 and can be installed together with other 3x80.H55 function
        groups.

        This version is an engineering version

Enhancements:
=============

	New MMI version for smart alignment measurement, not supported yet by FSW

	Improvements for smart alignment measurement
	(connector limits, support of MMI 2.71B)


Known Bugs:
===========

    Motorola V60 gets muted when it receives a call waiting message. This may be a
	phone issue.

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.





***************************
CDMA2000 3X80.H51
***************************

Date:   September 7, 2005

Base:   3x80.H50
MMI:    2.71A
LH:     V2.58

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3x80.H50 and can be installed together with other 3x80.H50 function
        groups.

        This version is an engineering version

Enhancements:
=============

	NPM NSig trigger fix

	Improvements in Smart Alignment

	New drunipvs.dld for PVF and Smart Alignment

        New Classes for Power vs. Frame and Smart Alignment

Known Bugs:
===========

    Motorola V60 gets muted when it receives a call waiting message. This may be a
	phone issue.

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.




***************************
CDMA2000 3X80.H50
***************************

Date:   August 25, 2005

Base:   3x80.H50
MMI:    2.70M
LH:     V2.58

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3x80.H50 and can be installed together with other 3x80.H50 function
        groups.

        This version is an engineering version

Enhancements:
=============

	First integration

Known Bugs:
===========

    Motorola V60 gets muted when it receives a call waiting message. This may be a
	phone issue.

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.





***************************
CDMA2000 3X80.H14
***************************

Date:   August 19, 2005

Base:   3x80.H11
MMI:    2.70M
LH:     V2.58

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3x80.H11 and can be installed together with other 3x80.H11 function
        groups.

        This version is an engineering version

Enhancements:
=============

	Further improved implementation of smart alignment measurement

Known Bugs:
===========

    Motorola V60 gets muted when it receives a call waiting message. This may be a
	phone issue.

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.





***************************
CDMA2000 3X80.H13
***************************

Date:   August 17, 2005

Base:   3x80.H11
MMI:    2.70M
LH:     V2.58

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3x80.H11 and can be installed together with other 3x80.H11 function
        groups.

        This version is an engineering version

Enhancements:
=============

	Improved implementation of smart alignment measurement

Known Bugs:
===========

    Motorola V60 gets muted when it receives a call waiting message. This may be a
	phone issue.

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.





***************************
CDMA2000 3X80.H12
***************************

Date:   August 15, 2005

Base:   3x80.H11
MMI:    2.70L
LH:     V2.58

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3x80.H11 and can be installed together with other 3x80.H11 function
        groups.

        This version is an engineering version

Enhancements:
=============

	First implementation of smart alignment measurement

Known Bugs:
===========

    Motorola V60 gets muted when it receives a call waiting message. This may be a
	phone issue.

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.





***************************
CDMA2000 3X80.H11
***************************

Date:   August 10, 2005

Base:   3x80.H10
MMI:    2.70L
LH:     V2.58

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3x80.H10 and can be installed together with other 3x80.H10 function
        groups.

        This version is a release candidate for V3.80

Enhancements:
=============

	Fixed Reset-bug in MMI

Known Bugs:
===========

    Motorola V60 gets muted when it receives a call waiting message. This may be a
	phone issue.

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.





***************************
CDMA2000 3X80.H10
***************************

Date:   August 9, 2005

Base:   3x80.H10
MMI:    2.70K
LH:     V2.58

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3x80.H10 and can be installed together with other 3x80.H10 function
        groups.

        This version is a release candidate for V3.80

Enhancements:
=============

	None

Known Bugs:
===========

    Motorola V60 gets muted when it receives a call waiting message. This may be a
	phone issue.

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.





***************************
CDMA2000 3X80.H08
***************************

Date:   July 27, 2005

Base:   3x80.H06
MMI:    2.70I
LH:     V.58

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3x80.H06 and can be installed together with other 3x80.H06 function
        groups.

        This version is a release candidate for V3.80

Enhancements:
=============

	Replaced red box in LH for ESN with yellow box

	Better logging for linkhandler error reports

	Linkhandler can now create yellow boxes in FSW


Known Bugs:
===========

    Motorola V60 gets muted when it receives a call waiting message. This may be a
	phone issue.

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.





***************************
CDMA2000 3X60.J67
***************************

Date:   July 27, 2005

Base:   V3.61
MMI:    2.51B
LH:     V2.51H

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        V3.61 and can be installed together with other V3.61 function
        groups.

        This version is a release candidate.


Enhancements:
=============

	Fix for ESN crash

Known Bugs:
===========

    Motorola V60 gets muted when it receives a call waiting message. This may be a
	phone issue.

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.






***************************
CDMA2000 3X80.H07
***************************

Date:   July 22, 2005

Base:   3x80.H06
MMI:    2.70I
LH:     V.57

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3x80.H06 and can be installed together with other 3x80.H06 function
        groups.

        This version is a debug version, only meant to debug the ESN error

Enhancements:
=============

	None

Known Bugs:
===========

    Too many call drops after the combination interband handoff - RF channel handoff

    Motorola V60 gets muted when it receives a call waiting message. This may be a
	phone issue.

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.





***************************
CDMA2000 3X80.H06
***************************

Date:   July 20, 2005

Base:   3x80.H05
MMI:    2.70I
LH:     X2.57A

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3x80.H05 and can be installed together with other 3x80.H05 function
        groups.

        This version is a debug version, only meant to debug the ESN error

Enhancements:
=============

	Bug fix of soft key for power control bits

	Additional logging for analyzing the wrong ESN bug


Known Bugs:
===========

    Too many call drops after the combination interband handoff - RF channel handoff

    Motorola V60 gets muted when it receives a call waiting message. This may be a
	phone issue.

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.





***************************
CDMA2000 3X80.H05
***************************

Date:   July 15, 2005

Base:   3x80.H05
MMI:    2.70H
LH:     V.57

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3x80.H05 and can be installed together with other 3x80.H05 function
        groups.

        This version is an engineering version.

Enhancements:
=============

	Bug fixes for crashes after call drops in fallback mode


Known Bugs:
===========

    Too many call drops after the combination interband handoff - RF channel handoff

    Motorola V60 gets muted when it receives a call waiting message. This may be a
	phone issue.

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.





***************************
CDMA2000 3X60.J66
***************************

Date:   July 6, 2005

Base:   V3.61
MMI:    2.51B
LH:     V2.51G

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        V3.61 and can be installed together with other V3.61 function
        groups.

        This version is a release candidate.


Enhancements:
=============

	Fix for Vocoder Crash at LG

Known Bugs:
===========

    Motorola V60 gets muted when it receives a call waiting message. This may be a
	phone issue.

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.






***************************
CDMA2000 3X80.H01
***************************

Date:   July 5, 2005

Base:   3x80.H01
MMI:    2.70H
LH:     V.57

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3x80.H01 and can be installed together with other 3x80.H01 function
        groups.

        This version is an engineering version.

Enhancements:
=============

	None

Known Bugs:
===========

    Motorola V60 gets muted when it receives a call waiting message. This may be a
	phone issue.

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.





***************************
CDMA2000 3X80.G02
***************************

Date:   July 1, 2005

Base:   3x80.G01
MMI:    2.70G
LH:     X2.56E

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3x80.G01 and can be installed together with other 3x80.G01 function
        groups.

        This version is an engineering version.

Enhancements:
=============

	Untested fixes for the vocoder crash

	Crash fix after call drop after handoff with fallback

	Enhanced Logging for Vocoder crash

	Fix for Hostname timeout

Known Bugs:
===========

    Motorola V60 gets muted when it receives a call waiting message. This may be a
	phone issue.

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.





***************************
CDMA2000 3X80.G01
***************************

Date:   June 22, 2005

Base:   3x80.G01
MMI:    2.70G
LH:     X2.56D

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3x80.G01 and can be installed together with other 3x80.G01 function
        groups.

        This version is an engineering version.

Enhancements:
=============

	Untested fixes for the vocoder crash

	Crash fix after call drop after handoff with fallback

Known Bugs:
===========

    Motorola V60 gets muted when it receives a call waiting message. This may be a
	phone issue.

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.






***************************
CDMA2000 3X80.F05
***************************

Date:   June 20, 2005

Base:   3x80.F05
MMI:    2.70G
LH:     X2.56C

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3x80.F05 and can be installed together with other 3x80.F05 function
        groups.

        This version is an engineering version.

Enhancements:
=============

	Improved IP-Settings

Known Bugs:
===========

    Motorola V60 gets muted when it receives a call waiting message. This may be a
	phone issue.

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.






***************************
CDMA2000 3X60.J65
***************************

Date:   June 15, 2005

Base:   V3.61
MMI:    2.51B
LH:     V2.51F

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        V3.61 and can be installed together with other V3.61 function
        groups.

        This version is a release candidate.


Enhancements:
=============

	Fix for Vocoder Crash at LG

	Fix for FER suppression crash at Motorola


Known Bugs:
===========

    Motorola V60 gets muted when it receives a call waiting message. This may be a
	phone issue.

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.






***************************
CDMA2000 3X80.F01
***************************

Date:   June 10, 2005

Base:   3x80.F01
MMI:    2.70G
LH:     X2.56C

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3x80.F01 and can be installed together with other 3x80.F01 function
        groups.

        This version is an engineering version.

Enhancements:
=============

	None

Known Bugs:
===========

    Motorola V60 gets muted when it receives a call waiting message. This may be a
	phone issue.

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.






***************************
CDMA2000 3X80.E05
***************************

Date:   June 3, 2005

Base:   3x80.E05
MMI:    2.70G
LH:     X2.56C

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3x80.E05 and can be installed together with other 3x80.E05 function
        groups.

        This version is an engineering version.

Enhancements:
=============

	Enhanced linkhandler logging
	Enhanced FSW logging, using rotating logging files

Known Bugs:
===========

    Motorola V60 gets muted when it receives a call waiting message. This may be a
	phone issue.

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.






***************************
CDMA2000 3X80.E03
***************************

Date:   June 2, 2005

Base:   3x80.E02
MMI:    2.70G
LH:     X2.56C

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3x80.E02 and can be installed together with other 3x80.E02 function
        groups.

        This version is an engineering version.

Enhancements:
=============

	Enhancend linkhandler logging!

Known Bugs:
===========

    Motorola V60 gets muted when it receives a call waiting message. This may be a
	phone issue.

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.






***************************
CDMA2000 3X80.E02
***************************

Date:   June 1, 2005

Base:   3x80.E02
MMI:    2.70G
LH:     X2.56B

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3x80.E02 and can be installed together with other 3x80.E02 function
        groups.

        This version is an engineering version.

Enhancements:
=============

	None

Known Bugs:
===========

    Motorola V60 gets muted when it receives a call waiting message. This may be a
	phone issue.

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.






***************************
CDMA2000 3X80.D12
***************************

Date:   May 27, 2005

Base:   3x80.D10
MMI:    2.70F
LH:     X2.56B

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3x80.D10 and can be installed together with other 3x80.D10 function
        groups.

        This version is an engineering version.

Enhancements:
=============

	Linkhandler and FSW have enhanced debugging activated

	Warning: This enhanced debugging is for debug purposes only!!!

Known Bugs:
===========

    Motorola V60 gets muted when it receives a call waiting message. This may be a
	phone issue.

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.






***************************
CDMA2000 3X80.D11
***************************

Date:   May 24, 2005

Base:   3x80.D10
MMI:    2.70F
LH:     X2.56A

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3x80.D10 and can be installed together with other 3x80.D10 function
        groups.

        This version is an engineering version.

Enhancements:
=============

	Fixes Vocoder Crash

	Prevents double mobile registration

	Avoids crash for reconfiguration message after call loss

	Protects linkhandler path for B96 generator


Known Bugs:
===========

    Motorola V60 gets muted when it receives a call waiting message. This may be a
	phone issue.

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.






***************************
CDMA2000 3X80.D10
***************************

Date:   May 23, 2005

Base:   3x80.D10
MMI:    2.70F
LH:     X2.56

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3x80.D10 and can be installed together with other 3x80.D10 function
        groups.

        This version is an engineering version.

Enhancements:
=============

	Improvements for B96 self test support

	Fixes for B83 self test in remote mode

	Fixes for IP-Parameters


Known Bugs:
===========

    Motorola V60 gets muted when it receives a call waiting message. This may be a
	phone issue.

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.






***************************
CDMA2000 3X60.J64
***************************

Date:   May 23, 2005

Base:   V3.61
MMI:    2.51B
LH:     V2.51E

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        V3.61 and can be installed together with other V3.61 function
        groups.

        This version is a release candidate.


Enhancements:
=============

	Fixes Vocoder Crash

	Prevents double mobile registration

	Avoids crash for reconfiguration message after call loss


Known Bugs:
===========

    Motorola V60 gets muted when it receives a call waiting message. This may be a
	phone issue.

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.






***************************
CDMA2000 3X60.J63
***************************

Date:   May 13, 2005

Base:   V3.61
MMI:    2.51B
LH:     X2.51X

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        V3.61 and can be installed together with other V3.61 function
        groups.

        This version is a release candidate.


Enhancements:
=============

	Fixes Linkhandler lockup in unpatient call establish remote procedure


Known Bugs:
===========

    Motorola V60 gets muted when it receives a call waiting message. This may be a
	phone issue.

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.






***************************
CDMA2000 3X80.D05
***************************

Date:   May 11, 2005

Base:   3x80.D05
MMI:    2.70F
LH:     X2.56

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3x80.D05 and can be installed together with other 3x80.D05 function
        groups.

        This version is an engineering version.

Enhancements:
=============

	None

Known Bugs:
===========

    Motorola V60 gets muted when it receives a call waiting message. This may be a
	phone issue.

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.






***************************
CDMA2000 3X60.J62
***************************

Date:   May 11, 2005

Base:   V3.61
MMI:    2.51B
LH:     V2.51D

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        V3.61 and can be installed together with other V3.61 function
        groups.

        This version is a release candidate.


Enhancements:
=============

	Avoids Linkhandler message stack overflow

	Avoids red box when we receive a call reconfiguration message from the linkhandler
	after we already dropped/lost the call

Known Bugs:
===========

    Motorola V60 gets muted when it receives a call waiting message. This may be a
	phone issue.

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.






***************************
CDMA2000 3X80.D02
***************************

Date:   May 06, 2005

Base:   3x80.D01
MMI:    2.70F
LH:     X2.56

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3x80.D01 and can be installed together with other 3x80.D01 function
        groups.

        This version is an engineering version.

Enhancements:
=============

	Self test in remote mode should work now

	Interrupted continuous self test with change to CDMA2000 works now

Known Bugs:
===========

    Motorola V60 gets muted when it receives a call waiting message. This may be a
	phone issue.

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.






***************************
CDMA2000 3X80.D01
***************************

Date:   May 02, 2005

Base:   3x80.D01
MMI:    2.70F
LH:     X2.56

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3x80.D01 and can be installed together with other 3x80.D01 function
        groups.

        This version is an engineering version.

Enhancements:
=============

	13k Vococder supported again

	B96 self test support fixed

Known Bugs:
===========

    B83 self test crashes when interrupted in continuous mode by changing to IMT2000

    B83 self test issues in remote mode (switching between IMT2000 and self test)

    Red box in certain IP Par and CDMA2000 signaling situations

    Motorola V60 gets muted when it receives a call waiting message. This may be a
	phone issue.

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.






***************************
CDMA2000 3X80.C16
***************************

Date:   April 27, 2005

Base:   3x80.C15
MMI:    2.70F
LH:     X2.56

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3x80.C15 and can be installed together with other 3x80.C15 function
        groups.

        This version is an engineering version.

Enhancements:
=============

	Fixed boot-up issue when LH-options were not present

	New drc2kmod.dld

Known Bugs:
===========

    B83 self test crashes when interrupted in continuous mode by changing to IMT2000

    B83 self test issues in remote mode (switching between IMT2000 and self test)

    After B83 self test, the 1xEV-DO generator can't be switched on (fix in next base version)

    B96 self test doesn't confirm properly

    Red box in certain IP Par and CDMA2000 signaling situations

    Motorola V60 gets muted when it receives a call waiting message. This may be a
	phone issue.

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.






***************************
CDMA2000 3X80.C15
***************************

Date:   April 26, 2005

Base:   3x80.C15
MMI:    2.70F
LH:     X2.56

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3x80.C15 and can be installed together with other 3x80.C15 function
        groups.

        This version is an engineering version.

Enhancements:
=============

	Selftest B83 with IMT2000 installed

	Fixed netclock issue for NSig generators

	Bug fixes for IP Par

	Loading of B88 and Vocoder in startup phase

Known Bugs:
===========

    B83 self test crashes when interrupted in continuous mode by changing to IMT2000

    B83 self test issues in remote mode (switching between IMT2000 and self test)

    After B83 self test, the 1xEV-DO generator can't be switched on (fix in next base version)

    B96 self test doesn't confirm properly

    Red box in certain IP Par and CDMA2000 signaling situations

    Motorola V60 gets muted when it receives a call waiting message. This may be a
	phone issue.

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.






***************************
CDMA2000 3X80.C05
***************************

Date:   April 13, 2005

Base:   3x80.C05
MMI:    2.70F
LH:     X2.55

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3x80.C05 and can be installed together with other 3x80.C05 function
        groups.

        This version is an engineering version.

Enhancements:
=============

	Several bug fixes, especially the memory access error

	Improvements for TxTimeError & PnSyncError

	Support of central TCP/IP menu


Known Bugs:
===========

    Motorola V60 gets muted when it receives a call waiting message. This may be a
	phone issue.

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.






***************************
CDMA2000 3X60.J61
***************************

Date:   April 7, 2005

Base:   V3.61
MMI:    2.51B
LH:     V2.51C

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        V3.61 and can be installed together with other V3.61 function
        groups.

        This version is a release candidate.


Enhancements:
=============

	Avoids TxTimeError of 0.00 in case of PnSeqError

Known Bugs:
===========

    Motorola V60 gets muted when it receives a call waiting message. This may be a
	phone issue.

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.






***************************
CDMA2000 3X80.C01
***************************

Date:   April 7, 2005

Base:   3x80.C01
MMI:    2.70F
LH:     X2.54

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3x80.C01 and can be installed together with other 3x80.C01 function
        groups.

        This version is an engineering version.

Enhancements:
=============

	Central LH configuration report added

	Includes B96 self test support (not yet tested)

	Improvements for TCP/IP parameters

	Another TxTimeError measurement logic update


Known Bugs:
===========

    Occasional memory access error (still under investigation)

    Motorola V60 gets muted when it receives a call waiting message. This may be a
	phone issue.

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.


***************************
CDMA2000 3X60.J60
***************************

Date:   April 6, 2005

Base:   V3.61
MMI:    2.51B
LH:     V2.51C

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        V3.61 and can be installed together with other V3.61 function
        groups.

        This version is a release candidate.


Enhancements:
=============

	New Dr2kmod DSP application that allows the display of measurements results
	even when we have a PN-Seq-Error

	TxTimeError display logic revised according to DSP changes

	Power settings for measurement in signalling state Signal OFF corrected


Known Bugs:
===========

    Motorola V60 gets muted when it receives a call waiting message. This may be a
	phone issue.

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.






***************************
CDMA2000 3X80.B35
***************************

Date:   March 29, 2005

Base:   3x80.B35
MMI:    2.70E
LH:     X2.54

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3x80.B35 and can be installed together with other 3x80.B35 function
        groups.

        This version is an engineering version.

Enhancements:
=============

	Improvements for B83 self test (necessary files not yet in Base)

	Improvements for B96 self test support	(necessary files not yet in Base)

	Improvements for TCP/IP parameters

	New TxTimeError measurement logic

	Support of new MMI method for Call Waiting Indicator


Known Bugs:
===========

    Occasional memory access error (under investigation)

    Motorola V60 gets muted when it receives a call waiting message. This may be a
	phone issue.

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.



***************************
CDMA2000 3X60.J59
***************************

Date:   March 28, 2005

Base:   V3.61
MMI:    2.51B
LH:     V2.51C

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        V3.61 and can be installed together with other V3.61 function
        groups.

        This version is a release candidate.


Enhancements:
=============

	Power settings for manual mode & power control bits = auto corrected

	TxTimeError measurement: activation logic improved


Known Bugs:
===========

    Motorola V60 gets muted when it receives a call waiting message. This may be a
	phone issue.

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.






***************************
CDMA2000 3X60.J58
***************************

Date:   March 18, 2005

Base:   V3.61
MMI:    2.51B
LH:     V2.51C

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        V3.61 and can be installed together with other V3.61 function
        groups.

        This version is a release candidate.


Enhancements:
=============

	Access board again supported

Known Bugs:
===========

    Motorola V60 gets muted when it receives a call waiting message. This may be a
	phone issue.

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.






***************************
CDMA2000 3X60.J57
***************************

Date:   March 17, 2005

Base:   V3.61
MMI:    2.51B
LH:     V2.51C

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        V3.61 and can be installed together with other V3.61 function
        groups.

        This version is a release candidate.


Enhancements:
=============

	Initialization of Mobile Node Home IP Addr.

	TxTimeError for NonSig has 2 digits now

	Access board again supported

Known Bugs:
===========

    Motorola V60 gets muted when it receives a call waiting message. This may be a
	phone issue.

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.






***************************
CDMA2000 3X80.B30
***************************

Date:   March 15, 2005

Base:   3x80.B30
MMI:    2.70E
LH:     X2.54

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3x80.B30 and can be installed together with other 3x80.B30 function
        groups.

        This version is an engineering version.

Enhancements:
=============

	Improvements in non-sig parameter class

	LH Interface improvements

	TCP/IP singular interface for the static parameters: improvements

	B83 self test: support through lh interface


Known Bugs:
===========

    Memory violation in non-sig, when both Overview measurement and generator are on

    Motorola V60 gets muted when it receives a call waiting message. This may be a
	phone issue.

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.



***************************
CDMA2000 3X60.J56
***************************

Date:   March 9, 2005

Base:   V3.61
MMI:    2.51A_SP01
LH:     V2.51C

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        V3.61 and can be installed together with other V3.61 function
        groups.

        This version is a release candidate.


Enhancements:
=============

	Initial RC settings corrected

Known Bugs:
===========

    Motorola V60 gets muted when it receives a call waiting message. This may be a
	phone issue.

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.






***************************
CDMA2000 3X80.B25
***************************

Date:   March 9, 2005

Base:   3x80.B25
MMI:    2.70E
LH:     X2.53

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3x80.B25 and can be installed together with other 3x80.B25 function
        groups.

        This version is an engineering version.

Enhancements:
=============

	Non Signaling modulation measurments added: ACP, IQ/IF-Analyzer

	Improvements in non-sig parameter class

	LH Interface improvements

	Linkhandler ping now always available

	TCP/IP singular interface for the static parameters

Known Bugs:
===========

    Memory violation in non-sig, when both Overview measurement and generator are on

    Motorola V60 gets muted when it receives a call waiting message. This may be a
	phone issue.

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.



***************************
CDMA2000 3X60.J55
***************************

Date:   March 4, 2005

Base:   V3.61
MMI:    2.51A_SP01
LH:     V2.51X

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        V3.61 and can be installed together with other V3.61 function
        groups.

        This version is a release candidate.


Enhancements:
=============

	Initialization issues of N-Sig generator solved

	TxTimeError rules for sig and n-sig established

	Path allocation timeout raised for measurements

	Autoranging in n-sig stabilized

Known Bugs:
===========

    After switching the nsig generator on, RC or FrameRate have to be adapted to
	enforce the changes on the linkhandler. Otherwise, we will have no proper
	power control and the measurement results will be instable.

    Motorola V60 gets muted when it receives a call waiting message. This may be a
	phone issue.

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.






***************************
CDMA2000 3X60.J54
***************************

Date:   March 1, 2005

Base:   V3.61
MMI:    2.51A
LH:     V2.51X

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        V3.61 and can be installed together with other V3.61 function
        groups.

        This version is a release candidate.


Enhancements:
=============

	N-Sig H-PSK measurement works

Known Bugs:
===========

    O-QPSK doesn't workanymore with RC >= 3 AND TxTimeError switched ON

    Motorola V60 gets muted when it receives a call waiting message. This may be a
	phone issue.

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.






***************************
CDMA2000 3X80.B20
***************************

Date:   March 1, 2005

Base:   3x80.B20
MMI:    2.70D
LH:     X2.53

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3x80.B20 and can be installed together with other 3x80.B20 function
        groups.

        This version is an engineering version.

Enhancements:
=============

	Non Signaling modulation measurments added: Overview, EVM, MGE, PE.

	Corrected Tx timing error measurement algorithm.

	Initial implementation of NonSig params class.

	LH Interface improvements

Known Bugs:
===========

    TCP/IP is removed from CDMA2000 but implementaion in the base class is not yet enabled.

    Motorola V60 gets muted when it receives a call waiting message. This may be a
	phone issue.

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.



***************************
CDMA2000 3X60.J53
***************************

Date:   February 25, 2005

Base:   V3.61
MMI:    2.51A
LH:     V2.51B

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        V3.61 and can be installed together with other V3.61 function
        groups.

        This version is a release candidate.


Enhancements:
=============

	Tx Time Error works now

Known Bugs:
===========

    FTM in H-PSK hasn't worked yet

    Motorola V60 gets muted when it receives a call waiting message. This may be a
	phone issue.

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.






***************************
CDMA2000 3X60.J52
***************************

Date:   February 24, 2005

Base:   V3.61
MMI:    2.51A
LH:     V2.51B

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        V3.61 and can be installed together with other V3.61 function
        groups.

        This version is a release candidate.


Enhancements:
=============

	Tx-Time-Error enabling now dependent on trigger and generator state

	Transfer of Long Code Mask to DSP in non-signaling mode

	Fixed path-bug in Power vs. Frame measurement


Known Bugs:
===========

    Motorola V60 gets muted when it receives a call waiting message. This may be a
	phone issue.

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.






***************************
CDMA2000 3X80.B15
***************************

Date:   February 15, 2005

Base:   3x80.B15
MMI:    2.70C
LH:     X2.52

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3x80.B15 and can be installed together with other 3x80.B15 function
        groups.

        This version is an engineering version.

	The MMI Base is patched from Thomas Feddersen.

	MMI parameters for new TCP/IP menu in system setup cause yellow boxes.


Enhancements:
=============

	Enhanced functionality of the new linkhandler interface, including logging

Known Bugs:
===========

    Yellow boxes for USB parameter 101, 102, 103, 104, 109

    Motorola V60 gets muted when it receives a call waiting message. This may be a
	phone issue.

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.




***************************
CDMA2000 3X80.B10
***************************

Date:   February 8, 2005

Base:   3x80.B10
MMI:    2.70C
LH:     X2.52

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3x80.B10 and can be installed together with other 3x80.B10 function
        groups.

        This version is an engineering version.

	The MMI Base is patched from Thomas Feddersen.

	MMI parameters for new TCP/IP menu in system setup cause yellow boxes.


Enhancements:
=============

	ACP Non-Signalling measurements.

Known Bugs:
===========

    Parameter type error in TCP/IP settings for static ip address result in
	yellow boxes at cmu startup and entering TCP/IP page of setup menu.

    Parameter type error in TCP/IP settings for dynamic	host name when successful
	dynamic addressing is returned from C2K LH.

    Motorola V60 gets muted when it receives a call waiting message. This may be a
	phone issue.

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.




***************************
CDMA2000 3X80.B05
***************************

Date:   February 1, 2005

Base:   3x80.B05
MMI:    2.70B
LH:     X2.52

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3x80.B05 and can be installed together with other 3x80.B05 function
        groups.

        This version is an engineering version.

	The MMI Base is patched from Thomas Feddersen.

	MMI parameters for new TCP/IP menu in system setup cause yellow and
	red boxes (see below).


Enhancements:
=============

	Common interface class for the CD2K linkhandler, with it's own
	resource management.

	CDP Non-Signalling measurements.

	TCP/IP static and dynamic settings in the setup menu.

	MIP Authentication Type.

Known Bugs:
===========

    Parameter type error in TCP/IP settings for static ip address result in
	yellow boxes at cmu startup and entering TCP/IP page of setup menu.

    Parameter type error in TCP/IP settings for dynamic	host name when successful
	dynamic addressing is returned from C2K LH.

    Addressing type results in tree.c error - red box for first two activations.

    Motorola V60 gets muted when it receives a call waiting message. This may be a
	phone issue.

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.




***************************
CDMA2000 3X60.J51
***************************

Date:   January 28, 2005

Base:   3x60.J50
MMI:    2.51A
LH:     V2.51A

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3x60.J50 and can be installed together with other 3x60.J50 function
        groups.

        This version is a release candidate.


Enhancements:
=============

	Fixed Linkhandler and FSW crashes for cases when supported service options
	and supported mux options exceeded internal and standard limits

	Fixed a call drop problem in a GPIB script with
	handoff speech to loopback, set attenuation, RF channel handoff


Known Bugs:
===========

    Motorola V60 gets muted when it receives a call waiting message. This may be a
	phone issue.

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.






***************************
CDMA2000 3X80.A11
***************************

Date:   January 25, 2005

Base:   3x80.A11
MMI:    2.70A
LH:     X2.50C

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3x80.A10 and can be installed together with other 3x80.A10 function
        groups.

        This version is an EXPERIMENTAL VERSION only!


Enhancements:
=============

	One common interface class for the CD2K linkhandler, with it's own
	resource management

Known Bugs:
===========

    Call drop when changing external attenuation and then trying to perform an
	RF channel handoff

    Motorola V60 gets muted when it receives a call waiting message. This may be a
	phone issue.

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.



***************************
CDMA2000 3X80.B01
***************************

Date:   January 24, 2005

Base:   3x80.B01
MMI:    2.70B
LH:     X2.50C

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3x80.B01 and can be installed together with other 3x80.B01 function
        groups.

        This version is an engineering version.

	******************** WARNING!! *********************
	The CD2K fgroups other than the 800 Cellular fgroup result in errors
	at startup. Remove the 1900, 2200 and 450 CD2K frgoups to use this build.


Enhancements:
=============

	New MMI for common TCPIP parameters - not supported yet by FSW

	New MMI behavior for CallWaitingIndicator - not supported yet by FSW

	New MMI for MIP Authentication type - not supported yet by FSW

Known Bugs:
===========

    Call drop when changing external attenuation and then trying to perform an
	RF channel handoff

    Motorola V60 gets muted when it receives a call waiting message. This may be a
	phone issue.

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.



***************************
CDMA2000 3X60.J50
***************************

Date:   January 18, 2005

Base:   3x60.J50
MMI:    2.51A
LH:     V2.50c

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3x60.J50 and can be installed together with other 3x60.J50 function
        groups.

        This version is an engineering version


Enhancements:
=============

	Fixed erraneous power control bit settings in the linkhandler after hard handoff

Known Bugs:
===========

    Call drop when changing external attenuation and then trying to perform an
	RF channel handoff - not reproducible

    Motorola V60 gets muted when it receives a call waiting message. This may be a
	phone issue.

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.




***************************
CDMA2000 3X80.A10
***************************

Date:   January 17, 2005

Base:   3x80.A10
MMI:    2.70A
LH:     V2.50B

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3x80.A10 and can be installed together with other 3x80.A10 function
        groups.

        This version is an engineering version


Enhancements:
=============

	New MMI for non-signalling: not supported yet by FSW

Known Bugs:
===========

    Call drop when changing external attenuation and then trying to perform an
	RF channel handoff

    Motorola V60 gets muted when it receives a call waiting message. This may be a
	phone issue.

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.


***************************
CDMA2000 3X60.J45
***************************

Date:   January 17, 2005

Base:   3x60.J45
MMI:    2.51A
LH:     V2.50B

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3x60.J45 and can be installed together with other 3x60.J45 function
        groups.

        This version is an engineering version


Enhancements:
=============

	Support of K80, improved & tested]

	Support of more than 40 Service Option in a capabilities report

	Corrected frame rate settings for RC 2 and 5 in non-sig

	Corrected power control bit settings for RC changes in non-sig

	Corrected SO33 RLP settings for rate 2

	Improved Layer 1 logging in the linkhandler


Known Bugs:
===========

    Call drop when changing external attenuation and then trying to perform an
	RF channel handoff

    Motorola V60 gets muted when it receives a call waiting message. This may be a
	phone issue.

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.




***************************
CDMA2000 3X60.J40
***************************

Date:   January 4, 2005

Base:   3x60.j40
MMI:    2.50Z
LH:     V2.49F

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3x60.J40 and can be installed together with other 3x60.J40 function
        groups.

        This version is an engineering version


Enhancements:
=============

	Support of Option K80 - CDMA2000 Non-Signaling
		Untested (or doesn't work yet)


Known Bugs:
===========

    RC settings for Non-Signalling might be erraneous. Feedback from Qualcomm needed
 	in to resolve if this is indeed a CMU (linkhandler) issue.

    Motorola V60 gets muted when it receives a call waiting message. This may be a
	phone issue.

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.




***************************
CDMA2000 3X80.A05
***************************

Date:   January 3rd, 2005

Base:   3x80.A05
MMI:    2.50Z
LH:     V2.49F

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3x80.A05 and can be installed together with other 3x80.A05 function
        groups.

        This version is an engineering version


Enhancements:
=============

	None

Known Bugs:
===========

    RC settings for Non-Signalling might be erraneous. Feedback from Qualcomm needed
 	in to resolve if this is indeed a CMU (linkhandler) issue.

    Motorola V60 gets muted when it receives a call waiting message. This may be a
	phone issue.

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.




***************************
CDMA2000 3X80.A01
***************************

Date:   December 20, 2004

Base:   3x80.A01
MMI:    2.50Z
LH:     V2.49F

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3x80.A01 and can be installed together with other 3x80.A01 function
        groups.

        This version is an engineering version


Enhancements:
=============

	None

Known Bugs:
===========

    RC settings for Non-Signalling might be erraneous. Feedback from Qualcomm needed
 	in to resolve if this is indeed a CMU (linkhandler) issue.

    Motorola V60 gets muted when it receives a call waiting message. This may be a
	phone issue.

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.




***************************
CDMA2000 3X60.J35
***************************

Date:   December 12, 2004

Base:   3x60.J35
MMI:    2.50Z
LH:     V2.49F

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3x60.J35 and can be installed together with other 3x60.J35 function
        groups.

        This version is a release candidate for V3.60!


Enhancements:
=============

	Call loss detection switched off for all measurements

	Bug fix for FPC measurement crash

Known Bugs:
===========

    RC settings for Non-Signalling might be erraneous. Feedback from Qualcomm needed
 	in to resolve if this is indeed a CMU (linkhandler) issue.

    Motorola V60 gets muted when it receives a call waiting message. This may be a
	phone issue.

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.




***************************
CDMA2000 3X60.J31
***************************

Date:   December 07, 2004

Base:   3x60.J30
MMI:    2.50Z
LH:     V2.49D

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3x60.J30 and can be installed together with other 3x60.J30 function
        groups.

        This version is a release candidate for V3.60!


Enhancements:
=============

	Manual MaxPower limits are now adapted to the connector limits.

Known Bugs:
===========

    One rarely occuring red bux for FPC measurement

    RC settings for Non-Signalling might be erraneous. Feedback from Qualcomm needed
 	in to resolve if this is indeed a CMU (linkhandler) issue.

    Motorola V60 gets muted when it receives a call waiting message. This may be a
	phone issue.

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.




***************************
CDMA2000 3X60.J30
***************************

Date:   December 06, 2004

Base:   3x60.J30
MMI:    2.50Z
LH:     V2.49D

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3x60.J30 and can be installed together with other 3x60.J30 function
        groups.

        This version is a release candidate for V3.60!


Enhancements:
=============

	MinPower measurements now support mobiles which operate a very low power
	levels ( < 53 dBm )

	Bug fix for SO33 Execute Option Ctrl Message

	Bug fix for red box in FPC measurement

	Bug fixes for RLP and Ping measurements in remote mode

Known Bugs:
===========

    One rarely occuring red bux for FPC measurement

    RC settings for Non-Signalling might be erraneous. Feedback from Qualcomm needed
 	in to resolve if this is indeed a CMU (linkhandler) issue.

    Motorola V60 gets muted when it receives a call waiting message. This may be a
	phone issue.

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.




***************************
CDMA2000 3X60.J22
***************************

Date:   November 23, 2004

Base:   3x60.J20
MMI:    2.50Z
LH:     V2.49C

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3x60.J20 and can be installed together with other 3x60.J20 function
        groups.

        This version is a release candidate for V3.60!


Enhancements:
=============

	Bug fix for RC handoff

	Bug fix for FPC/SCH for data rates > 9.600 bps

	Bug fix for red box when entering Non-Sig

Known Bugs:
===========

    Motorola V60 gets muted when it receives a call waiting message. This may be a
	phone issue.

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.




***************************
CDMA2000 3X60.J20
***************************

Date:   November 22, 2004

Base:   3x60.J20
MMI:    2.50Z
LH:     V2.49B

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3x60.J20 and can be installed together with other 3x60.J20 function
        groups.

        This version is a release candidate for V3.60!


Enhancements:
=============

	Bug fix for red box in CDMA2000 signalling

Known Bugs:
===========

    Motorola V60 gets muted when it receives a call waiting message. This may be a
	phone issue.

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.




***************************
CDMA2000 3X60.J14
***************************

Date:   November 19, 2004

Base:   3x60.J10
MMI:    2.50Z
LH:     V2.49B

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3x60.J10 and can be installed together with other 3x60.J10 function
        groups.

        This version is a release candidate for V3.60!


Enhancements:
=============

	Turbo Coding is nuw fully supported

	2 different linkhandler memory leaks fixed

	Power vs. Frame measurement restarts on several analyzer parameters

	Recalculated Walsh Code settings for SCH channels now are being sent to the
		linkhandler after data rate change.

	The QOF bug of 3x60.13 turned out to be no bug at all but a correct implementation.


Known Bugs:
===========

    Motorola V60 gets muted when it receives a call waiting message. This may be a
	phone issue.

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.




***************************
CDMA2000 3X60.J13
***************************

Date:   November 11, 2004

Base:   3x60.J10
MMI:    2.50Z
LH:     V2.49A

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3x60.J10 and can be installed together with other 3x60.J10 function
        groups.

        This version is a release candidate for V3.60!


Enhancements:
=============

	Walsh Code setting control now also works in Signal OFF state,
		Old GPIB commands now refer to TDSO

	Fixed bug when changing RF Channel in Alerting state

	Fixed problem in Non Signalling where the gains for the channels were not set
		past -1.0 dB.

Known Bugs:
===========

    Turbo Coding is not properly supported. This issue must have existed for a very
	long time (since it has first been implemented) but never showed up.

    Motorola V60 gets muted when it receives a call waiting message. This may be a
	phone issue.

    The settings allow the allocation of the same walsh code with QOF=0 for one
	channel and QOF!=0 for another channel. To my knowledge, this isn't allowed.
	The fix requires a minor, but not interface compatible base system change.

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.




***************************
CDMA2000 3X60.J12
***************************

Date:   November 08, 2004

Base:   3x60.J10
MMI:    2.50Y
LH:     V2.49

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3x60.J10 and can be installed together with other 3x60.J10 function
        groups.

        This version is a release candidate for V3.60!


Enhancements:
=============

	SCH walsh code and qof settings now moved into S032/S033. This allows
		better initialization of the mobile settings

	DataCall now carries invalid state flag over between CDMA2000 function groups

Known Bugs:
===========

    The settings allow the allocation of the same walsh code with QOF=0 for one
	channel and QOF!=0 for another channel. To my knowledge, this isn't allowed.
	The fix requires a minor, but not interface compatible base system change.

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.




***************************
CDMA2000 3X60.J11
***************************

Date:   November 04, 2004

Base:   3x60.J10
MMI:    2.50X
LH:     X2.49

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3x60.J10 and can be installed together with other 3x60.J10 function
        groups.

        This version is an engineering version!


Enhancements:
=============

	The linkhandler uses a new Xilinx. This fixes a problem with a new lot
	of linkhandler boards that would crash when booting the linkhandler.

Known Bugs:
===========

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.




***************************
CDMA2000 3X60.J10
***************************

Date:   November 02, 2004

Base:   3x60.J10
MMI:    2.50X
LH:     X2.48C

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3x60.J10 and can be installed together with other 3x60.J10 function
        groups.

        This version is an engineering version!


Enhancements:
=============

	Improved stability in Power vs. Frame Measurement (NSig)

	Usage of more stabile IF-Trigger Detector (NSig)

	Bug fixes in interband handoff and remote debug mode

Known Bugs:
===========

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.




***************************
CDMA2000 3X60.J05
***************************

Date:   October 22, 2004

Base:   3x60.J05
MMI:    2.50X
LH:     X2.48C

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3x60.J05 and can be installed together with other 3x60.J05 function
        groups.

        This version is an engineering version!


Enhancements:
=============

	All measurements can now run as MinPower measurements (PowerControlBits = AllDown)

	Cancellation of handoff preparation now works without yellow box (in RDM)

Known Bugs:
===========

    With the Kyocera 2255 phone, we can watch a crash (#763) which is not
  	reproducable with any other phone or in any other situation.

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.




***************************
CDMA2000 3X60.J01
***************************

Date:   October 15, 2004

Base:   3x60.J01
MMI:    2.50W
LH:     X2.48

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3x60.J01 and can be installed together with other 3x60.J01 function
        groups.

        This version is an engineering version!


Enhancements:
=============

	Min Power runs again

Known Bugs:
===========

    Min & Max Power measurements do not compensate for external attenuation

    With the Kyocera 2255 phone, we can watch a crash (#763) which is not
  	reproducable with any other phone or in any other situation.

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.




***************************
CDMA2000 3X60.I36
***************************

Date:   October 08, 2004

Base:   3x60.I35
MMI:    2.50W
LH:     X2.47C

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3x60.I35 and can be installed together with other 3x60.I35 function
        groups.

        This version is an engineering version!


Enhancements:
=============

	FTM fully supported

Known Bugs:
===========

    With the Kyocera 2255 phone, we can watch a crash (#763) which is not
  	reproducable with any other phone or in any other situation.

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.




***************************
CDMA2000 3X60.I35
***************************

Date:   October 06, 2004

Base:   3x60.I35
MMI:    2.50V
LH:     X2.47A

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3x60.I35 and can be installed together with other 3x60.I35 function
        groups.

        This version is an engineering version!


Enhancements:
=============

	Some bug fixes in SO33 and FDA

Known Bugs:
===========

    FTM: Zero long code mask not yet supported

    With the Kyocera 2255 phone, we can watch a crash (#763) which is not
  	reproducable with any other phone or in any other situation.

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.




***************************
CDMA2000 3X60.I32
***************************

Date:   October 04, 2004

Base:   3x60.I30
MMI:    2.50V
LH:     X2.47A

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3x60.I30 and can be installed together with other 3x60.I30 function
        groups.

        This version is an engineering version!


Enhancements:
=============

	FTM works now (untested)

Known Bugs:
===========

    With the Kyocera 2255 phone, we can watch a crash (#763) which is not
  	reproducable with any other phone or in any other situation.

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.




***************************
CDMA2000 3X60.I31
***************************

Date:   October 01, 2004

Base:   3x60.I30
MMI:    2.50V
LH:     X2.47

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3x60.I30 and can be installed together with other 3x60.I30 function
        groups.

        This version is an engineering version!


Enhancements:
=============

	FTM improvements

Known Bugs:
===========

    With the Kyocera 2255 phone, we can watch a crash (#763) which is not
  	reproducable with any other phone or in any other situation.

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.




***************************
CDMA2000 3X60.I30
***************************

Date:   September 29, 2004

Base:   3x60.I30
MMI:    2.50V
LH:     X2.45A

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3x60.I30 and can be installed together with other 3x60.I30 function
        groups.

        This version is an engineering version!


Enhancements:
=============

	Frame Rate after Reset now valid

Known Bugs:
===========

    With the Kyocera 2255 phone, we can watch a crash (#763) which is not
  	reproducable with any other phone or in any other situation.

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.




***************************
CDMA2000 3X60.I25
***************************

Date:   September 27, 2004

Base:   3x60.I25
MMI:    2.50V
LH:     X2.45A

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3x60.I25 and can be installed together with other 3x60.I25 function
        groups.

        This version is an engineering version!


Enhancements:
=============

	Support of Factory Test Mode parameters except ESN and zero long code mask

	Yellow box for RF Expected Power fixed

	several MMI bug fixes

Known Bugs:
===========

    Frame Rate doesn't get updated after reset

    With the Kyocera 2255 phone, we can watch a crash (#763) which is not
  	reproducable with any other phone or in any other situation.

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.




***************************
CDMA2000 3X60.I20
***************************

Date:   September 20, 2004

Base:   3x60.I20
MMI:    2.50U
LH:     X2.45

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3x60.I20 and can be installed together with other 3x60.I20 function
        groups.

        This version is an engineering version!


Enhancements:
=============

	FDA adjust for signalling

	Burst in H-PSK fixed

	Some TCP/IP issues fixed

Known Bugs:
===========

    No FDA adjust for non-signalling

    Frame Rate doesn't get updated after reset

    With the Kyocera 2255 phone, we can watch a crash (#763) which is not
  	reproducable with any other phone or in any other situation.

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.




***************************
CDMA2000 3X60.I15
***************************

Date:   September 9, 2004

Base:   3x60.I15
MMI:    2.50T
LH:     X2.45

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3x60.I15 and can be installed together with other 3x60.I15 function
        groups.

        This version is an engineering version!


Enhancements:
=============

	FDA adjust for signalling (not tested)

Known Bugs:
===========

    No FDA adjust for non-signalling

    Frame Rate doesn't get updated after reset

    With the Kyocera 2255 phone, we can watch a crash (#763) which is not
  	reproducable with any other phone or in any other situation.

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.




***************************
CDMA2000 3X60.I03
***************************

Date:   September 8, 2004

Base:   3x60.I01
MMI:    2.50T
LH:     X2.45

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3x60.I01 and can be installed together with other 3x60.I01 function
        groups.

        This version is an engineering version!


Enhancements:
=============

	Further Improved parameter handover for interband handoffs

	System time setting

	CDP limit lines corrected

	CDP support for SO33 calls

	Suppression of message boxes in remote mode


Known Bugs:
===========

    Adjust problems with FDA

    Frame Rate doesn't get updated after reset

    With the Kyocera 2255 phone, we can watch a crash (#763) which is not
  	reproducable with any other phone or in any other situation.

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.




***************************
CDMA2000 3X60.I02
***************************

Date:   August 26, 2004

Base:   3x60.I01
MMI:    2.50T
LH:     X2.44z

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3x60.I01 and can be installed together with other 3x60.I01 function
        groups.

        This version is an engineering version!


Enhancements:
=============

	Improved parameter handover for interband handoffs

Known Bugs:
===========

    Adjust problems with FDA

    Frame Rate doesn't get updated after reset

    With the Kyocera 2255 phone, we can watch a crash (#763) which is not
  	reproducable with any other phone or in any other situation.

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.




***************************
CDMA2000 3X60.I01
***************************

Date:   August 17, 2004

Base:   3x60.I01
MMI:    2.50S
LH:     X2.43b

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3x60.I01 and can be installed together with other 3x60.I01 function
        groups.

        This version is an engineering version!


Enhancements:
=============

	Search Window Size

	Improvements of display of special call features

	Message box for Call Waiting ACK

	Configurable SMS lenghth

	fixed handoff bug from handoff prep directly to fgroup (via menu select)

Known Bugs:
===========

    Adjust problems with FDA

    Frame Rate doesn't get updated after reset

    With the Kyocera 2255 phone, we can watch a crash (#763) which is not
  	reproducable with any other phone or in any other situation.

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.




***************************
CDMA2000 3X60.H05
***************************

Date:   August 4, 2004

Base:   3x60.H05
MMI:    2.50R
LH:     X2.43

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3x60.H05 and can be installed together with other 3x60.H05 function
        groups.

        This version is an engineering version!


Enhancements:
=============

	Bug fix for O-QPSK

	Bug fixes in aborted interband handoffs

Known Bugs:
===========

    With the Kyocera 2255 phone, we can watch a crash (#763) which is not
  	reproducable with any other phone or in any other situation.

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.




***************************
CDMA2000 3X60.H01
***************************

Date:   JUly 28, 2004

Base:   3x60.H01
MMI:    2.50R
LH:     X2.43

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3x60.H01 and can be installed together with other 3x60.H01 function
        groups.

        This version is an engineering version!


Enhancements:
=============

	Added SO33 network initiated call response

	Fixed a hang when a phone is not being picked up

	Fixed switching from TDSO to other service class while call is being connected

Known Bugs:
===========

    In O-QPSK, after an RC handoff, the measurement are running with gated RF signal (at times)

    CMU freezes when after selecting a function group for a handoff, this new function
	group is loading and we pull the connector of the phone

    With the Kyocera 2255 phone, we can watch a crash (#763) which is not
  	reproducable with any other phone or in any other situation.

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.




***************************
CDMA2000 3X60.G05
***************************

Date:   JUly 21, 2004

Base:   3x60.G05
MMI:    2.50R
LH:     X2.43

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3x60.G05 and can be installed together with other 3x60.G05 function
        groups.

        This version is an engineering version!


Enhancements:
=============

	Call Waiting Indicator now disabled in disconnected state

	Network initiated dormancy for service control message SO33

	Optimization for Power control bit modes hold and pattern

	removed bug when changing service classes while call is connecting

Known Bugs:
===========

    Some special call features don't work yet as expected (calls connecting when they should
	be busy, etc.)

    In O-QPSK, after an RC handoff, the measurement are running with gated RF signal (at times)

    CMU freezes when after selecting a function group for a handoff, this new function
	group is loading and we pull the connector of the phone

    With the Kyocera 2255 phone, we can watch a crash (#763) which is not
  	reproducable with any other phone or in any other situation.

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.




***************************
CDMA2000 3X60.G02
***************************

Date:   JUly 16, 2004

Base:   3x60.G01
MMI:    2.50Q
LH:     X2.42A

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3x60.G01 and can be installed together with other 3x60.G01 function
        groups.

        This version is an engineering version!


Enhancements:
=============

	Restart of measurements on RF Selectivity

	Non-Signalling support of RF Selectivity

	Bug fixes for drc2kmod.dld portation

	Improved TCP/IP synchronization with the linkhandler


Known Bugs:
===========

    Some special call features don't work yet as expected (calls connecting when they should
	be busy, etc.)

    In O-QPSK, after an RC handoff, the measurement are running with gated RF signal (at times)

    CMU freezes when after selecting a function group for a handoff, this new function
	group is loading and we pull the connector of the phone

    With the Kyocera 2255 phone, we can watch a crash (#763) which is not
  	reproducable with any other phone or in any other situation.

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.




***************************
CDMA2000 3X60.G01
***************************

Date:   JUly 13, 2004

Base:   3x60.G01
MMI:    2.50Q
LH:     X2.41A

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3x60.G01 and can be installed together with other 3x60.G01 function
        groups.

        This version is an engineering version!


Enhancements:
=============

	None

Known Bugs:
===========

    Some special call features don't work yet as expected (calls connecting when they should
	be busy, etc.)

    In O-QPSK, after an RC handoff, the measurement are running with gated RF signal (at times)

    CMU freezes when after selecting a function group for a handoff, this new function
	group is loading and we pull the connector of the phone

    With the Kyocera 2255 phone, we can watch a crash (#763) which is not
  	reproducable with any other phone or in any other situation.

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.




***************************
CDMA2000 3X60.F06
***************************

Date:   JUly 12, 2004

Base:   3x60.F05
MMI:    2.50Q
LH:     X2.41A

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3x60.F05 and can be installed together with other 3x60.F05 function
        groups.

        This version is an engineering version!


Enhancements:
=============

	Support of RF Selectivity for Signalling, not yet for non-signalling

Known Bugs:
===========

    Some special call features don't work yet as expected (calls connecting when they should
	be busy, etc.)

    In O-QPSK, after an RC handoff, the measurement are running with gated RF signal (at times)

    CMU freezes when after selecting a function group for a handoff, this new function
	group is loading and we pull the connector of the phone

    With the Kyocera 2255 phone, we can watch a crash (#763) which is not
  	reproducable with any other phone or in any other situation.

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.




***************************
CDMA2000 3X60.F05
***************************

Date:   JUly 6, 2004

Base:   3x60.F05
MMI:    2.50P
LH:     X2.41A

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3x60.F05 and can be installed together with other 3x60.F05 function
        groups.

        This version is an engineering version!


Enhancements:
=============

	dsp.cpp error fixed

Known Bugs:
===========

    Some special call features don't work yet as expected (calls connecting when they should
	be busy, etc.)

    In O-QPSK, after an RC handoff, the measurement are running with gated RF signal (at times)

    CMU freezes when after selecting a function group for a handoff, this new function
	group is loading and we pull the connector of the phone

    With the Kyocera 2255 phone, we can watch a crash (#763) which is not
  	reproducable with any other phone or in any other situation.

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.




***************************
CDMA2000 3X60.E12
***************************

Date:   JUly 2, 2004

Base:   3x60.E10
MMI:    2.50P
LH:     X2.41A

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3x60.E10 and can be installed together with other 3x60.E10 function
        groups.

        This version is an engineering version!


Enhancements:
=============

	Special Call features (Caller ID, Intercept, Reorder, Busy, Ignore, Call Waiting)

	Completed switch of drcdmod.dld to drc2kmod.dld

Known Bugs:
===========

    Some special call features don't work yet as expected (calls connecting when they should
	be busy, etc.)

    Yellow "DSP" box due to a bug in the base system.

    In O-QPSK, after an RC handoff, the measurement are running with gated RF signal (at times)

    CMU freezes when after selecting a function group for a handoff, this new function
	group is loading and we pull the connector of the phone

    With the Kyocera 2255 phone, we can watch a crash (#763) which is not
  	reproducable with any other phone or in any other situation.

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.




***************************
CDMA2000 3X60.E10
***************************

Date:   June, 18 2004

Base:   3x60.E10
MMI:    2.50P
LH:     X2.41

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3x60.E10 and can be installed together with other 3x60.E10 function
        groups.

        This version is an engineering version!


Enhancements:
=============

	Modulation O-QPSK uses drc2kmod.dld

	Packet Zone ID

	Power level for manual mode corrected

Known Bugs:
===========

    In O-QPSK, after an RC handoff, the measurement are running with gated RF signal (at times)

    CMU freezes when after selecting a function group for a handoff, this new function
	group is loading and we pull the connector of the phone

    With the Kyocera 2255 phone, we can watch a crash (#763) which is not
  	reproducable with any other phone or in any other situation.

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.




***************************
CDMA2000 3X60.E01
***************************

Date:   June, 7 2004

Base:   3x60.E01
MMI:    2.50M
LH:     X2.40A

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3x60.E01 and can be installed together with other 3x60.E01 function
        groups.

        This version is an engineering version!


Enhancements:
=============

	Overview O-QPSK uses drc2kmod.dld

	No autoranging for manual mode

	New Call features (MMI only)

Known Bugs:
===========

    Overview O-QPSK runs as H-PSK measurement for RC3 and higher, and not at all for RC1,2

    Wrong power level reading in manual mode

    CMU freezes when after selecting a function group for a handoff, this new function
	group is loading and we pull the connector of the phone

    With the Kyocera 2255 phone, we can watch a crash (#763) which is not
  	reproducable with any other phone or in any other situation.

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.




***************************
CDMA2000 3X60.D11
***************************

Date:   May, 28 2004

Base:   3x60.D10
MMI:    2.50N
LH:     X2.40A

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3x60.D10 and can be installed together with other 3x60.D10 function
        groups.

        This version is an engineering version!


Enhancements:
=============

	Connect bug fixed

Known Bugs:
===========

    CMU freezes when after selecting a function group for a handoff, this new function
	group is loading and we pull the connector of the phone

    With the Kyocera 2255 phone, we can watch a crash (#763) which is not
  	reproducable with any other phone or in any other situation.

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.




***************************
CDMA2000 3X60.D10
***************************

Date:   May, 27 2004

Base:   3x60.D10
MMI:    2.50M
LH:     X2.40A

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3x60.D10 and can be installed together with other 3x60.D10 function
        groups.

        This version is an engineering version!


Enhancements:
=============

	Path error in remote debug mode fixed

	PRef error fixed

	Channel Power shows correct values again for non-active channels

	Enhancements for S033

Known Bugs:
===========

    The second call connect leads to a fatal crash

    CMU freezes when after selecting a function group for a handoff, this new function
	group is loading and we pull the connector of the phone

    With the Kyocera 2255 phone, we can watch a crash (#763) which is not
  	reproducable with any other phone or in any other situation.

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.




***************************
CDMA2000 3X60.D05
***************************

Date:   May, 14 2004

Base:   3x60.D05
MMI:    2.50L
LH:     X2.40

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3x60.D05 and can be installed together with other 3x60.D05 function
        groups.

        This version is an engineering version!


Enhancements:
=============

	*rst error fixed, phones will also register in other band classes than USCell

Known Bugs:
===========

    CMU freezes when after selecting a function group for a handoff, this new function
	group is loading and we pull the connector of the phone

    With the Kyocera 2255 phone, we can watch a crash (#763) which is not
  	reproducable with any other phone or in any other situation.

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.




***************************
CDMA2000 3X60.D01
***************************

Date:   May, 04 2004

Base:   3x60.D01
MMI:    2.50K
LH:     X2.40

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3x60.D01 and can be installed together with other 3x60.D01 function
        groups.

        This version is an engineering version!


Enhancements:
=============

	OLTR error fixed

	*rst does not lead to crash anymore

	CD2K->AMPS handoff fixed

	CD2K->CD2K handoff fixed

	SO33 improvements

	PING measurement repeat interval


Known Bugs:
===========

    Phones will not register in other band classes other than US Cellular

    CMU freezes when after selecting a function group for a handoff, this new function
	group is loading and we pull the connector of the phone

    With the Kyocera 2255 phone, we can watch a crash (#763) which is not
  	reproducable with any other phone or in any other situation.

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.




***************************
CDMA2000 3X60.C15
***************************

Date:   April 16, 2004

Base:   3x60.C16
MMI:    2.50I
LH:     X2.38

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3x60.C15 and can be installed together with other 3x60.C15 function
        groups.

        This version is an engineering version!


Enhancements:
=============

	Version Control on startup

	DHCP error box

	TDSO RC's update fixed


Known Bugs:
===========

    CMU freezes when after selecting a function group for a handoff, this new function
	group is loading and we pull the connector of the phone

    With the Kyocera 2255 phone, we can watch a crash (#763) which is not
  	reproducable with any other phone or in any other situation.

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.




***************************
CDMA2000 3X60.C11
***************************

Date:   April 12, 2004

Base:   3x60.C10
MMI:    2.50I
LH:     X2.38

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3x60.C10 and can be installed together with other 3x60.C10 function
        groups.

        This version is an engineering version!


Enhancements:
=============

	GPIB-commands for new 3x60.xxx features

	Wrong measurements conditions added


Known Bugs:
===========

    CMU freezes when after selecting a function group for a handoff, this new function
	group is loading and we pull the connector of the phone

    With the Kyocera 2255 phone, we can watch a crash (#763) which is not
  	reproducable with any other phone or in any other situation.

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.




***************************
CDMA2000 3X60.C10
***************************

Date:   April 6, 2004

Base:   3x60.C10
MMI:    2.50H
LH:     X2.36A

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3x60.C10 and can be installed together with other 3x60.C10 function
        groups.

        This version is an engineering version!


Enhancements:
=============

	Failed Call Timeout

	SO33 improvements

	Gain Extension

	Service Negotiation


Known Bugs:
===========

    CMU freezes when after selecting a function group for a handoff, this new function
	group is loading and we pull the connector of the phone

    With the Kyocera 2255 phone, we can watch a crash (#763) which is not
  	reproducable with any other phone or in any other situation.

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.




***************************
CDMA2000 3X60.B10
***************************

Date:   March 26, 2004

Base:   3x60.C01
MMI:    2.50H
LH:     X2.34c

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3x60.C01 and can be installed together with other 3x60.C01 function
        groups.

        This version is an engineering version!


Enhancements:
=============

	Improvements for SO33 - TCP/IP and DHCP Failure behavior


Known Bugs:
===========

    CMU freezes when after selecting a function group for a handoff, this new function
	group is loading and we pull the connector of the phone

    With the Kyocera 2255 phone, we can watch a crash (#763) which is not
  	reproducable with any other phone or in any other situation.

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.




***************************
CDMA2000 3X60.B05
***************************

Date:   March 9, 2004

Base:   3x60.B02
MMI:    2.50G
LH:     X2.34

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3x60.B05 and can be installed together with other 3x60.B01 function
        groups.

        This version is an engineering version!


Enhancements:
=============

	Ping/Time restart & some bug fixes

	Improvements for SO33 configuration


Known Bugs:
===========

    CMU freezes when after selecting a function group for a handoff, this new function
	group is loading and we pull the connector of the phone

    With the Kyocera 2255 phone, we can watch a crash (#763) which is not
  	reproducable with any other phone or in any other situation.

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.



***************************
CDMA2000 3X60.B03
***************************

Date:   March 3, 2004

Base:   3x60.B01
MMI:    2.50G
LH:     X2.33A

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3x60.B01 and can be installed together with other 3x60.B01 function
        groups.

        This version is an engineering version!


Enhancements:
=============

	Phase/Time measurement improved graphics

	Improvements for SO33 configuration


Known Bugs:
===========

    CMU freezes when after selecting a function group for a handoff, this new function
	group is loading and we pull the connector of the phone

    With the Kyocera 2255 phone, we can watch a crash (#763) which is not
  	reproducable with any other phone or in any other situation.

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.



***************************
CDMA2000 3X60.B02
***************************

Date:   February 26, 2004

Base:   3x60.B01
MMI:    2.50F
LH:     X2.33A

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3x60.B01 and can be installed together with other 3x60.B01 function
        groups.

        This version is an engineering version!


Enhancements:
=============

	PING measurement

	Phase/Time measurements run for scalar values

	SO33-Call to mobile in dormant state

Known Bugs:
===========

    CMU freezes when after selectiong a function group for a handoff, this new function
	group is loading and we pull the connector of the phone

    With the Kyocera 2255 phone, we can watch a crash (#763) which is not
  	reproducable with any other phone or in any other situation.

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.



***************************
CDMA2000 3X60.B01
***************************

Date:   February 23, 2004

Base:   3x60.B01
MMI:    2.50F
LH:     X2.33

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3x60.B01 and can be installed together with other 3x60.B01 function
        groups.

        This version is an engineering version!


Enhancements:
=============

	RLP measurement

	SO33 partly implemented

	PING measurement

	Dynamic FER report size

	FPC enhancements

	Status Report suppression

	Code allocation management for foward channels

	Support of SW-Option K87

	MMI-Demo for Timing/Phase measurements

	RFChannel update for Non-Signaling

	Support of status event register for all NPower measurements

Known Bugs:
===========

    CMU freezes when after selectiong a function group for a handoff, this new function
	group is loading and we pull the connector of the phone

    With the Kyocera 2255 phone, we can watch a crash (#763) which is not
  	reproducable with any other phone or in any other situation.

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.



***************************
CDMA2000 3X60.A05
***************************

Date:   January 28, 2004

Base:   3x60.A05
MMI:    2.50C
LH:     X2.31z

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3x60.A05 and can be installed together with other 3x60.A05 function
        groups.

        This version is an engineering version!


Enhancements:
=============

	Exchange of GroupConfig with MeasConfig, resulting improvements in trigger settings.

	Integration of 3x60.A05

Known Bugs:
===========

    CMU freezes when after selectiong a function group for a handoff, this new function
	group is loading and we pull the connector of the phone

    With the Kyocera 2255 phone, we can watch a crash (#763) which is not
  	reproducable with any other phone or in any other situation.

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.



***************************
CDMA2000 3X51.F35
***************************

Date:   December 17, 2003

Base:   V3.51
MMI:    2.50A
LH:     V2.30

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        V3.50 and can be installed together with other V3.50 function
        groups.

        This version is an engineering version!


Enhancements:
=============

	MMI Simulation of the new SO33 features

Known Bugs:
===========

    CMU freezes when after selectiong a function group for a handoff, this new function
	group is loading and we pull the connector of the phone

    With the Kyocera 2255 phone, we can watch a crash (#763) which is not
  	reproducable with any other phone or in any other situation.

    IF trigger level setting doesn't work with the dynamic setting but converts
        the setting according to the RF trigger level

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.



***************************
CDMA2000 3X50.F23
***************************

Date:   December 11, 2003

Base:   V3.50
MMI:    2.30B
LH:     V2.30

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        V3.50 and can be installed together with other V3.50 function
        groups.

        This version is a release candidate!


Enhancements:
=============

	Handoff problem to an unsupported function group solved

	Handoff problem in connection with packet data service solved

	CDP issue of stale data after a certain manual procedure solved

	Initialization of the linkhandler when selecting SO33 in Disconnected state

Known Bugs:
===========

    CMU freezes when after selectiong a function group for a handoff, this new function
	group is loading and we pull the connector of the phone

    With the Kyocera 2255 phone, we can watch a crash (#763) which is not
  	reproducable with any other phone or in any other situation.

    IF trigger level setting doesn't work with the dynamic setting but converts
        the setting according to the RF trigger level

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.



***************************
CDMA2000 3X50.F22
***************************

Date:   December 3, 2003

Base:   V3.50
MMI:    2.30A
LH:     V2.30

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        V3.50 and can be installed together with other V3.50 function
        groups.

        This version is a release candidate!


Enhancements:
=============

	PROC and CONF commands are now identical in functionality

	BS established SO33 call prohibited

Known Bugs:
===========

    With the Kyocera 2255 phone, we can watch a crash (#763) which is not
  	reproducable with any other phone or in any other situation.

    IF trigger level setting doesn't work with the dynamic setting but converts
        the setting according to the RF trigger level

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.



***************************
CDMA2000 3X50.F21
***************************

Date:   November 21, 2003

Base:   V3.50
MMI:    2.20K
LH:     V2.30

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        V3.50 and can be installed together with other V3.50 function
        groups.

        This version is a release candidate!


Enhancements:
=============

	Improvement for Status Event Register Flag

Known Bugs:
===========

    With the Kyocera 2255 phone, we can watch a crash (#763) which is not
  	reproducable with any other phone or in any other situation.

    IF trigger level setting doesn't work with the dynamic setting but converts
        the setting according to the RF trigger level

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.



***************************
CDMA2000 3X50.F20
***************************

Date:   November 14, 2003

Base:   3X50.F20
MMI:    2.20K
LH:     V2.30

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3X50.F20 and can be installed together with other 3X50.F20 function
        groups.

        This version is a release candidate!


Enhancements:
=============

	Improvement for Status Event Register Flag

Known Bugs:
===========

    IF trigger level setting doesn't work with the dynamic setting but converts
        the setting according to the RF trigger level

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.



***************************
CDMA2000 3X50.F15
***************************

Date:   November 07, 2003

Base:   3X50.F15
MMI:    2.20J
LH:     V2.30

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3X50.F15 and can be installed together with other 3X50.F15 function
        groups.

        This version is a release candidate!


Enhancements:
=============

	I/Q Imbalance Limit check works now

	Handover from Us-Cell to PCS with Reset works

Known Bugs:
===========

    IF trigger level setting doesn't work with the dynamic setting but converts
        the setting according to the RF trigger level

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.



***************************
CDMA2000 3X50.F11
***************************

Date:   November 05, 2003

Base:   3X50.F10
MMI:    2.20J
LH:     V2.30

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3X50.F10 and can be installed together with other 3X50.F10 function
        groups.

        This version is an engineering release!


Enhancements:
=============

	Improvements for channel configuration

	I/Q Imbalance measurement activated


Known Bugs:
===========

    No Limit check yet for I/Q Imbalance

    IF trigger level setting doesn't work with the dynamic setting but converts
        the setting according to the RF trigger level

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.



***************************
CDMA2000 3X50.F10
***************************

Date:   October 31, 2003

Base:   3X50.F10
MMI:    2.20J
LH:     V2.30

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3X50.F10 and can be installed together with other 3X50.F10 function
        groups.

        This version is an engineering release!


Enhancements:
=============

	Option deteciont for 8k/13k speech coder

	Impovements for the Code Channel Configuration (not visible to user)

Known Bugs:
===========

    IF trigger level setting doesn't work with the dynamic setting but converts
        the setting according to the RF trigger level

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.



***************************
CDMA2000 3X50.F06
***************************

Date:   October 28, 2003

Base:   3X50.F05
MMI:    2.20J
LH:     X2.29A

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3X50.F05 and can be installed together with other 3X50.F05 function
        groups.

        This version is an engineering release!


Enhancements:
=============

	A freeze in GPIB mode when we do handoffs has been removed

Known Bugs:
===========

    Option detection for 13 speech coder doesn't work

    IF trigger level setting doesn't work with the dynamic setting but converts
        the setting according to the RF trigger level

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.



***************************
CDMA2000 3X50.F05
***************************

Date:   October 24, 2003

Base:   3X50.F05
MMI:    2.20I
LH:     X2.29A

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3X50.F05 and can be installed together with other 3X50.F05 function
        groups.

        This version is an engineering release!


Enhancements:
=============

    Setting the current RC in remote mode now checks the limits of the service options.

    Red box in siglhtsk.cpp (unexepcted message) fixed


Known Bugs:
===========

    Option detection for 13 speech coder doesn't work

    IF trigger level setting doesn't work with the dynamic setting but converts
        the setting according to the RF trigger level

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.



***************************
CDMA2000 3X50.F01
***************************

Date:   October 16, 2003

Base:   3X50.F01
MMI:    2.20H
LH:     X2.29A

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3X50.F01 and can be installed together with other 3X50.F01 function
        groups.

        This version is an engineering release!


Enhancements:
=============

    Option detection for B85 fixed


Known Bugs:
===========

    IF trigger level setting doesn't work with the dynamic setting but converts
        the setting according to the RF trigger level

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.



***************************
CDMA2000 3X50.E02
***************************

Date:   October 10, 2003

Base:   3X50.E01
MMI:    2.20H
LH:     X2.29A

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3X50.E01 and can be installed together with other 3X50.E01 function
        groups.

        This version is an engineering release!


Enhancements:
=============

    Fixed the Halt-issue for Power vs Frame

    Fixed the crash when we send an SMS with an FPC measurement running

    GPIB for I/Q Analyzer O-QPSK available

Known Bugs:
===========

    IF trigger level setting doesn't work with the dynamic setting but converts
        the setting according to the RF trigger level

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.



***************************
CDMA2000 3X50.E01
***************************

Date:   October 09, 2003

Base:   3X50.E01
MMI:    2.20G
LH:     X2.29A

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3X50.E01 and can be installed together with other 3X50.E01 function
        groups.

        This version is an engineering release!


Enhancements:
=============

    Restart on connect control parameters for I/Q Analyzer and ACP improved

    Issues for Channel filter settings in CDP & other HPSK measurements resolved

Known Bugs:
===========

    Red box when we try to send a SMS and an FPC measurement is runing in the
 	background

    IF trigger level setting doesn't work with the dynamic setting but converts
        the setting according to the RF trigger level

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.



***************************
CDMA2000 3X50.D11
***************************

Date:   October 03, 2003

Base:   3X50.D11
MMI:    2.20F
LH:     X2.29A

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3X50.D10 and can be installed together with other 3X50.D10 function
        groups.

        This version is an engineering release!


Enhancements:
=============

    I/Q Analyzer O-QPSK supported

    Error #755 and #756 (initialization after Signal Off to Signal On) fixed

    Non-Signalling Measurements work for HPSK and QPSK

Known Bugs:
===========

    IF trigger level setting doesn't work with the dynamic setting but converts
        the setting according to the RF trigger level

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.



***************************
CDMA2000 3X50.D10
***************************

Date:   September 26, 2003

Base:   3X50.D10
MMI:    2.20F
LH:     X2.28A

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3X50.D05 and can be installed together with other 3X50.D05 function
        groups.

        This version is an early engineering release


Enhancements:
=============

    MSI = 0 (empty SIM-Card) now supported

    Fix for NonSig HPSK

Known Bugs:
===========

    QPSK measurement not working properly in non-signalling mode.

    I/Q-Analyzer:   - O-QPSK does not work yet.

    IF trigger level setting doesn't work with the dynamic setting but converts
        the setting according to the RF trigger level

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.



***************************
CDMA2000 3X50.D05
***************************

Date:   September 23, 2003

Base:   3X50.DO5
MMI:    2.20E
LH:     X2.28A

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3X50.D05 and can be installed together with other 3X50.D05 function
        groups.

        This version is an early engineering release


Enhancements:
=============

    Improved Power vs Frame measurement.

    Improved I/Q HPSK Analyzer Constellation diagram

Known Bugs:
===========

    HPSK measurement not working properly in non-signalling mode.

    I/Q-Analyzer:   - O-QPSK does not work yet.

    *RST GPIB command causes red box.

    IF trigger level setting doesn't work with the dynamic setting but converts
        the setting according to the RF trigger level

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.



***************************
CDMA2000 3X50.D02
***************************

Date:   September 16, 2003

Base:   3X50.DO1
MMI:    2.20E
LH:     X2.28A

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3X50.D01 and can be installed together with other 3X50.D01 function
        groups.

        This version is an early engineering release


Enhancements:
=============

    Improved Power vs Frame measurement

    Improved I/Q HPSK Analyzer Constellation diagram

Known Bugs:
===========

    Power vs Frame: Timeout in single shot mode currently ony at 7.5 seconds,
                    we want to have no timeout at all.

    I/Q-Analyzer:   - O-QPSK doesn't work

    IF trigger level setting doesn't work with the dynamic setting but converts
        the setting according to the RF trigger level

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.




***************************
CDMA2000 3X50.D01
***************************

Date:   September 12, 2003

Base:   3X50.DO1
MMI:    2.20E
LH:     X2.28A

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3X50.D01 and can be installed together with other 3X50.D01 function
        groups.

        This version is an early engineering release


Enhancements:
=============

    Improved Power vs Frame measurement

    Bug fix for the NSig Generator (initialization when switching it ON).

Known Bugs:
===========

    Power vs Frame: - restart on several parameters doesn't work
                    - IF trigger seems to react on falling edge only, no matter what the setting is

    I/Q-Analyzer:   - O-QPSK doesn't work at all
                    - several settings in H-PSK mode don't work

    IF trigger level setting doesn't work with the dynamic setting but converts
        the setting according to the RF trigger level

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.




***************************
CDMA2000 3X50.C05
***************************

Date:   September 5, 2003

Base:   3X50.C05
MMI:    2.20D
LH:     X2.28A

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3X50.C05 and can be installed together with other 3X50.C05 function
        groups.

        This version is an early engineering release


Enhancements:
=============

    Added Power Ramp measurement in non-signalling

    Added I/Q Analyzer in signalling

    All measurements now work with DDC Filter 4m0 due to FER issue

    Channels send now on proper frequency after reset


Known Bugs:
===========

    IF trigger level setting doesn't work with the dynamic setting but converts
        the setting according to the RF trigger level

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.




***************************
CDMA2000 3X50.B16
***************************

Date:   August 19, 2003

Base:   3X50.B15
MMI:    2.20C
LH:     X2.28

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3X50.B15 and can be installed together with other 3X50.B15 function
        groups.

        This version is an early engineering release


Enhancements:
=============

    Improved measurement Power vs. Frames in Non-Signalling

    Added I/Q-Analyzer for Signalling O-QPSK and HPSK

    Solved an FER issue resulting from reloading the DDC Filter while FER is
    running. All application now use the DDC-Filter 4m0.


Known Bugs:
===========

    IF trigger level setting doesn't work with the dynamic setting but converts
        the setting according to the RF trigger level

    SCH1 support has not been tested. This is due to the fact that currently no
        known phone supports SCH1.

    Bugs according to current state of product support database.




***************************
CDMA2000 3X50.B15
***************************

Date:   August 15, 2003

Base:   3X50.B15
MMI:    2.20C
LH:     X2.28

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3X50.B15 and can be installed together with other 3X50.B15 function
        groups.

        This version is an early engineering release


Enhancements:
=============

	New State "Incoming SMS"

	Only one common trigger for all NonSig measurements (not sufficiently tested)


Known Bugs:
===========

	IF trigger level setting doesn't work with the dynamic setting but converts
		the setting according to the RF trigger level

	SCH1 support has not been tested. This is due to the fact that currently no
		known phone supports SCH1.

	Bugs according to current state of product support database.



***************************
CDMA2000 3X50.B10
***************************

Date:   August 07, 2003

Base:   3X50.B10
MMI:    2.20A
LH:     X2.28

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3X50.B10 and can be installed together with other 3X50.B10 function
        groups.

        This version is an early engineering release


Enhancements:
=============

	Mobile originated SMA

	Save/Recall

	Usage of the new DRC2KMOD.DLD (for EV-DV)

	Support of the new path allocation for the connectors


Known Bugs:
===========

	Save/Recall doesn't work 100% yet

	IF trigger level setting doesn't work with the dynamic setting but converts
		the setting according to the RF trigger level

	SCH1 support has not been tested. This is due to the fact that currently no
		known phone supports SCH1.

	Bugs according to current state of product support database.



***************************
CDMA2000 3X40.F32
***************************

Date:   July 29, 2003

Base:   V3.41
MMI:    2.00J-SP01
LH:     V2.27D

General Remarks
===============

	This release is the same as version 3x40.F31, but with a new sasflash.fw file.

        This release of CDMA2000 software is based on the CMU base system
        V3.41 and can be installed together with other V3.41 and V3x40.F2x function
        groups.

        This version is a release candidate


Enhancements:
=============

	Using sasflash.fw v2.27D.

	Integration of V3.41


Known Bugs:
===========

	IF trigger level setting doesn't work with the dynamic setting but converts
		the setting according to the RF trigger level

	SCH1 support has not been tested. This is due to the fact that currently no
		known phone supports SCH1.

	Bugs according to current state of product support database.



***************************
CDMA2000 3X40.F31
***************************

Date:   July 25, 2003

Base:   V3.41
MMI:    2.00J-SP01
LH:     V2.27C

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        V3.41 and can be installed together with other V3.41 and V3x40.F2x function
        groups.

        This version is a release candidate


Enhancements:
=============

	Bug Fixes for product support database errors #740

	Bug Fix for a freeze of the CMU when we send SMS in SO6
		(this bug fix solves possibly several other freezes)

	Integration of V3.41


Known Bugs:
===========

	IF trigger level setting doesn't work with the dynamic setting but converts
		the setting according to the RF trigger level

	SCH1 support has not been tested. This is due to the fact that currently no
		known phone supports SCH1.

	Bugs according to current state of product support database.



***************************
CDMA2000 3X40.F30
***************************

Date:   July 22, 2003

Base:   V3.41
MMI:    2.00J-SP01
LH:     V2.27B

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        V3.41 and can be installed together with other V3.41 and V3x40.F2x function
        groups.

        This version is a release candidate


Enhancements:
=============

	Bug Fixes for product support database errors #739, #734, #735

	Integration of V3.41


Known Bugs:
===========

	IF trigger level setting doesn't work with the dynamic setting but converts
		the setting according to the RF trigger level

	SCH1 support has not been tested. This is due to the fact that currently no
		known phone supports SCH1.

	Bugs according to current state of product support database.



***************************
CDMA2000 3X40.F29
***************************

Date:   July 16, 2003

Base:   V3.41
MMI:    2.00J
LH:     V2.27A

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        V3.41 and can be installed together with other V3.41 and V3x40.F2x function
        groups.

        This version is a release candidate


Enhancements:
=============

	Integration of V3.41


Known Bugs:
===========

	IF trigger level setting doesn't work with the dynamic setting but converts
		the setting according to the RF trigger level

	SCH1 support has not been tested. This is due to the fact that currently no
		known phone supports SCH1.

	Bugs according to current state of product support database.



***************************
CDMA2000 3X40.F28
***************************

Date:   July 14, 2003

Base:   3x40.F24
MMI:    2.00J
LH:     V2.27A

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        V3x40.F24 and can be installed together with other V3x40.F2x function
        groups.

        This version is not a release candidate


Enhancements:
=============

	Freezing of CMU fixed #731

	Red Box in FER measurementremoved (untested fix!!!) #733

	Error in Nonsignalling fixed #732


Known Bugs:
===========

	IF trigger level setting doesn't work with the dynamic setting but converts
		the setting according to the RF trigger level

	SCH1 support has not been tested. This is due to the fact that currently no
		known phone supports SCH1.

	Bugs according to current state of product support database.



***************************
CDMA2000 3X40.F27
***************************

Date:   July 11, 2003

Base:   3x40.F24
MMI:    2.00J
LH:     V2.27A

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        V3x40.F24 and can be installed together with other V3x40.F2x function
        groups.

        This version is not a release candidate


Enhancements:
=============

	FER timing issue after channel handoff fixed

	OLTR DSP error fixed

	Protocol Revision error fixed

Known Bugs:
===========

	IF trigger level setting doesn't work with the dynamic setting but converts
		the setting according to the RF trigger level

	SCH1 support has not been tested. This is due to the fact that currently no
		known phone supports SCH1.

	Bugs according to current state of product support database.



***************************
CDMA2000 3X40.F25
***************************

Date:   July 02, 2003

Base:   3x40.F24
MMI:    2.00J
LH:     V2.27

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        V3x40.F24 and can be installed together with other V3x40.F2x function
        groups.

        This version is not a release candidate


Enhancements:
=============

	Several bug fixes

Known Bugs:
===========

	IF trigger level setting doesn't work with the dynamic setting but converts
		the setting according to the RF trigger level

	SCH1 support has not been tested. This is due to the fact that currently no
		known phone supports SCH1.

	Timing problem of FER after RF channel handoff

	Bugs according to current state of product support database.



***************************
CDMA2000 3X40.F24
***************************

Date:   June 23, 2003

Base:   3x40.F21/F22
MMI:    2.00I
LH:     X2.26Y

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        V3x40.F21/22 and can be installed together with other V3x40.F2x function
        groups.

        This version is a release candidate for the CDMA2000 V3.40


Enhancements:
=============

	Several bug fixes

Known Bugs:
===========

	IF trigger level setting doesn't work with the dynamic setting but converts
		the setting according to the RF trigger level

	SCH1 support has not been tested. This is due to the fact that currently no
		known phone supports SCH1.

	Bugs according to current state of product support database.


***************************
CDMA2000 3X40.F23
***************************

Date:   June 20, 2003

Base:   3x40.F21/F22
MMI:    2.00I
LH:     X2.26

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        V3x40.F22 and can be installed together with other V3x40.F2x function
        groups.

        This version is a release candidate for the CDMA2000 V3.40


Enhancements:
=============

	Power level of correction processor set to -147 dB after Functiongroup i
 		left.

	Initialization for Handoffs improved

	Improved environment switching on call establish


Known Bugs:
===========

	IF trigger level setting doesn't work with the dynamic setting but converts
		the setting according to the RF trigger level

	SCH1 support has not been tested. This is due to the fact that currently no
		known phone supports SCH1.

	Bugs according to current state of product support database.


***************************
CDMA2000 3X40.F22
***************************

Date:   June 12, 2003

Base:   V3.40
MMI:    2.00I
LH:     V2.25

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        V3.40 and can be installed together with other V3x40.F2x function
        groups.

        This version is a release candidate for the CDMA2000 V3.40


Enhancements:
=============

	SMS receive with ACK now drops the call after ACK (thus solving the issue
		of unacknowledged SMS for some phones)

	NPower measurement now supports trigger settings

	3 dBm toggling in MS Power between RF channel handoff's resolved

	optimized reaction of FER measurements on changes of the signalling state

	Several bugs removed


Known Bugs:
===========

	IF trigger level setting doesn't work with the dynamic setting but converts
		the setting according to the RF trigger level

	SCH1 support has not been tested. This is due to the fact that currently no
		known phone supports SCH1.

	Bugs according to current state of product support database.


***************************
CDMA2000 3X40.F21
***************************

Date:   June 05, 2003

Base:   V3.40
MMI:    2.00H
LH:     X2.24

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        V3.40 and can be installed together with other V3x40.F21 function
        groups.

        It is an engineering version for test and presentation of the current
        status of the CDMA2000 development.


Enhancements:
=============

	After call established the correct frame rate is now supported.

	Patch for MaxPower measurement in connection with RF channel handoff.

	Several bugs removed


Known Bugs:
===========

	SCH1 support has not been tested. This is due to the fact that currently no
		known phone supports SCH1.

	Min Power OQPSK and GOP don't show valid results if entered from NPower


***************************
CDMA2000 3X40.F10
***************************

Date:   May 29, 2003

Base:   V3x40.F10
MMI:    2.00H
LH:     X2.22C

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        V3x40.F10 and can be installed together with other V3x40.F10 function
        groups.

        It is an engineering version for test and presentation of the current
        status of the CDMA2000 development.


Enhancements:
=============

	"Accept Mobile Originated Call" selection decides if all Service Options are
	accepted or only the selected Service Option

	Corrected parameter initialization when connecting a call.

	Mobile originated SO55 call supported

	Several bugs removed.

Known Bugs:
===========

	SCH1 support has not been tested. This is due to the fact that currently no
		known phone supports SCH1.

	Min Power OQPSK and GOP don't show valid results if entered from NPower


***************************
CDMA2000 3X40.F06
***************************

Date:   May 22, 2003

Base:   V3x40.F05
MMI:    2.00G
LH:     X2.22A

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        V3x40.F05 and can be installed together with other V3x40.F05 function
        groups.

        It is an engineering version for test and presentation of the current
        status of the CDMA2000 development.


Enhancements:
=============

	Linkhandler Version check now for all IMT2000 function groups on startup

	Improved parameter initialization when connecting a call.

	Several bugs removed.

Known Bugs:
===========

	NPower and ACP don't initialize properly, when a call is being connected

	SCH1 support has not been tested. This is due to the fact that currently no
		known phone supports SCH1.

	Red Box in OLTR when running remote READ in Signal OFF state

	Min Power OQPSK and GOP don't show valid results if entered from NPower


***************************
CDMA2000 3X40.F05
***************************

Date:   May 19, 2003

Base:   V3x40.F05
MMI:    2.00F
LH:     X2.21

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        V3x40.F05 and can be installed together with other V3x40.F01 function
        groups.

        It is an engineering version for test and presentation of the current
        status of the CDMA2000 development.


Enhancements:
=============

	Improved parameter initialization when connecting a call.

	Several bugs removed.

Known Bugs:
===========

	SCH1 support has not been tested. This is due to the fact that currently no
		known phone supports SCH1.

	Red Box in OLTR when running remote READ in Signal OFF state

	Min Power OQPSK and GOP don't show valid results if entered from NPower


***************************
CDMA2000 3X40.F01
***************************

Date:   May 09, 2003

Base:   V3x40.F01
MMI:    2.00F
LH:     X2.21

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        V3x40.F01 and can be installed together with other V3x40.F01 function
        groups.

        It is an engineering version for test and presentation of the current
        status of the CDMA2000 development.


Enhancements:
=============

	None

Known Bugs:
===========

	SCH1 support has not been tested. This is due to the fact that currently no
		known phone supports SCH1.

	Red Box in OLTR when running remote READ in Signal OFF state

	Min Power OQPSK and GOP don't show valid results if entered from NPower


***************************
CDMA2000 3X40.E10
***************************

Date:   May 05, 2003

Base:   V3x40.E10
MMI:    2.00E
LH:     X2.21

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        V3x40.E10 and can be installed together with other V3x40.E10 function
        groups.

        It is an engineering version for test and presentation of the current
        status of the CDMA2000 development.


Enhancements:
=============

	None

Known Bugs:
===========

	SCH1 support has not been tested. This is due to the fact that currently no
		known phone supports SCH1.

	Red Box in OLTR when running remote READ in Signal OFF state

	Min Power OQPSK and GOP don't show valid results if entered from NPower


***************************
CDMA2000 3X40.E05
***************************

Date:   April 29, 2003

Base:   V3x40.E05
MMI:    2.00E
LH:     X2.21

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        V3x40.E05 and can be installed together with other V3x40.E05 function
        groups.

        It is an engineering version for test and presentation of the current
        status of the CDMA2000 development.


Enhancements:
=============

	None

Known Bugs:
===========

	SCH1 support has not been tested. This is due to the fact that currently no
		known phone supports SCH1.

	Red Box in OLTR when running remote READ in Signal OFF state

	Min Power OQPSK and GOP don't show valid results if entered from NPower


***************************
CDMA2000 3X40.E01
***************************

Date:   April 18, 2003

Base:   V3x40.E01
MMI:    2.00D
LH:     V2.20x

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        V3x40.E01 and can be installed together with other V3x40.E01 function
        groups.

        It is an engineering version for test and presentation of the current
        status of the CDMA2000 development.

        It is a candidate for a release.



Enhancements:
=============

	ACP measurement implemente.

	Power Step Size implemented.

	Turbo Coding implemented


Known Bugs:
===========

	SCH1 support has not been tested. This is due to the fact that currently no
		known phone supports SCH1.

	Red Box when after handoff out of OLTR

	Min Power OQPSK and GOP don't show valid results if entered from NPower


***************************
CDMA2000 3X21.C26
***************************

Date:   March 13, 2003

Base:   V3.21
MMI:    1.60I
LH:     V2.20

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        V3.21 and can be installed together with other V3.21 and 3x21.C20 function
        groups.

        It is an engineering version for test and presentation of the current
        status of the CDMA2000 development.

        It is a candidate for a release.



Enhancements:
=============

	Bug in splatter test fixed.

	Crash of CMU when switching of a CD2K function group to other function groups
		(e.g. GSM) early after startup fixed.
		Since this crash couldn't be reproduced in RSA, this fix is currently
		untested.


Known Bugs:
===========

	SCH1 support has not been tested. This is due to the fact that currently no
		known phone supports SCH1.

	In the overview measurement, when the DSP measurement is in HALT mode
		and we switch the environment flag, the ChannelQuality measurement
		will go to off or the DSP measurement will be suppressed.
		This can only be resolved by restarting the DSP
		measurement and then switching ChannelQuality to ON (if necessary)

	When the call is released in manual mode, it can happen that the DSP
		measurement is then on OFF; simly switch it to ON again


***************************
CDMA2000 3X21.C20
***************************

Date:   February 26, 2003

Base:   3X21.C20
MMI:    1.60I
LH:     V2.20

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        V3.21 and can be installed together with other V3.20 and 3x21.C20 function
        groups.

        It is an engineering version for test and presentation of the current
        status of the CDMA2000 development.

        It is a candidate for a release.



Enhancements:
=============

	SCH1 support now activated

	Several bug fixes, especially in Call Released after Handoff(Fallback)


Known Bugs:
===========

	SCH1 support has not been tested. This is due to the fact that currently no
		known phone supports SCH1.

	In the overview measurement, when the DSP measurement is in HALT mode
		and we switch the environment flag, the ChannelQuality measurement
		will go to off or the DSP measurement will be suppressed.
		This can only be resolved by restarting the DSP
		measurement and then switching ChannelQuality to ON (if necessary)

	When the call is released in manual mode, it can happen that the DSP
		measurement is then on OFF; simly switch it to ON again


***************************
CDMA2000 3X20.C19
***************************

Date:   February 19, 2003

Base:   V3.20
MMI:    1.60I
LH:     V2.19

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        V3.20 and can be installed together other V3.20 and 3x20.C19 function
        groups.

        It is an engineering version for test and presentation of the current
        status of the CDMA2000 development.

        It may be a candidate for a release.



Enhancements:
=============

	Improvements on Sidband Suppression Correction. To reduce uncertainty of result in
	PCS band the Base System Version 3.21 will be necessary

	Access Probe problem fixed


Known Bugs:
===========

	In the overview measurement, when the DSP measurement is in HALT mode
		and we switch the environment flag, the ChannelQuality measurement
		will go to off or the DSP measurement will be suppressed.
		This can only be resolved by restarting the DSP
		measurement and then switching ChannelQuality to ON (if necessary)

	SCH1 is still deactivated



***************************
CDMA2000 3X20.C18
***************************

Date:   February 14, 2003

Base:   V3.20
MMI:    1.60I
LH:     V2.19

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        V3.20 and can be installed together other V3.20 and 3x20.C18 function
        groups.

        It is an engineering version for test and presentation of the current
        status of the CDMA2000 development.

        It may be a candidate for a release.



Enhancements:
=============

	Linkhandler bugfixes

	Improved switching of environments in manual mode

Known Bugs:
===========

	In the overview measurement, when the DSP measurement is in HALT mode
		and we switch the environment flag, the ChannelQuality measurement
		will go to off. This can only be resolved by restarting the DSP
		measurement and then switching ChannelQuality to ON

	SCH1 is still deactivated

	GPIB command set according to Excel sheet



***************************
CDMA2000 3X20.C17
***************************

Date:   February 10, 2003

Base:   V3.20
MMI:    1.60I
LH:     V2.18a

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        V3.20 and can be installed together other V3.20 and 3x20.C17 function
        groups.

        It is an engineering version for test and presentation of the current
        status of the CDMA2000 development.

        It is NOT a candidate for a release.



Enhancements:
=============

	Several linkhandler bugfixes

	Environment switching and resource allocation now after Call establish and release

Known Bugs:
===========

	When switching between local/global environments, the DSP measurements have
		manually to be switched to OFF and ON, same when we have a call established
		or released

	SCH1 is still deactivated

	GPIB command set according to Excel sheet



***************************
CDMA2000 3X20.C16
***************************

Date:   January 31, 2003

Base:   V3.20
MMI:    1.60G
LH:     V2.18

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        V3.20 and can be installed together other V3.20 and 3x20.C16 function
        groups.

        It is an engineering version for test and presentation of the current
        status of the CDMA2000 development.

        It is NOT a candidate for a release.



Enhancements:
=============

	Support Speech Coder CMU-B85 Var. 12 – i.e. 8K, 8K Enhanced and 13K Speech Coder

	Support of BS initiated call SO33
	Initial support of SCH1 (including FER) - currently untested

	Improvement in resource allocation of FER measurements

	Bugfix for erraneous power reading


Known Bugs:
===========
	When switching between local/global environments, the DSP measurements have
		manually to be switched to OFF and ON

	GPIB command set according to Excel sheet



***************************
CDMA2000 3X20.C15
***************************

Date:   January 24, 2003

Base:   V3.20
MMI:    1.60G
LH:     V2.17a

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        V3.20 and can be installed together other V3.20 and 3x20.C15 function
        groups.

        It is an engineering version for test and presentation of the current
        status of the CDMA2000 development.

        It is NOT a candidate for a release.



Enhancements:
=============

	Support Speech Coder CMU-B85 Var. 12 – i.e. 8K, 8K Enhanced and 13K Speech Coder

	Initial support of Service Option 33 (IP connection)
	Support of 153.6/230.4 kbps in F-SCH
	Initial support of SCH1 (including FER) - currently untested
	Possibility to inject Frame Errors in the Forward Link
	Configurable Power Control Bit Pattern


	Configurable measurement environment combined with resource allocation

	Code Domain Power Measurement
		Configurable IQ Leakage Check
		Spreading Rate configurable 16 or 32


Known Bugs:
===========
	When switching between local/global environments, the measurement has
		manually to be switched to OFF and ON

	GPIB command set according to Excel sheet



***************************
CDMA2000 3X20.C10
***************************

Date:   January 13, 2003

Base:   3x20.C10
MMI:    1.60F
LH:     V2.17

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3X20.C10 and can be installed together other C10 function groups.

        It is an engineering version for test and presentation of the current
        status of the CDMA2000 development.

        It is NOT a candidate for a release.

Enhancements:
=============
	Power Control Bits Pattern now supported
	Limit Lines for CDP now support IQ-Leakage

Known Bugs:
===========
        Red box on a hard handoff in TDSO
        SCHO default setting has to be 35
	CDP spreading factor change will issue yellow boxes, not yet supported

GPIB command set according to Excel sheet



***************************
CDMA2000 3X20.C05
***************************

Date:   January 07, 2003

Base:   3x20.C05
MMI:    1.60E
LH:     V2.16

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3X20.C05 and can be installed together other C05 function groups.

        It is an engineering version for test and presentation of the current
        status of the CDMA2000 development.

        It is NOT a candidate for a release.

Enhancements:
=============
	Injected FER: No yellow boxes anymore but yet no functionality either
	SO33: Reconfiguration of a parameter while the connection is established
	      will now terminate the call.


Known Bugs:
===========
        Red box on a hard handoff in TDSO
        SCHO default setting has to be 35

GPIB command set according to Excel sheet



***************************
CDMA2000 3X20.C01
***************************

Date:   December 19, 2002

Base:   3x20.C01
MMI:    1.60E
LH:     V2.15

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3X20.C01 and can be installed together other C01 function groups.

        It is an engineering version for test and presentation of the current
        status of the CDMA2000 development.

        It is NOT a candidate for a release.

Enhancements:
=============
        SO33: basic functionality for a MS initiated call
        CDP: New limit mode check



Known Bugs:
===========
        Red box on a hard handoff in TDSO
        SCHO default setting has to be 35

GPIB command set according to Excel sheet



***************************
CDMA2000 3X10.D21
***************************

Date:   October 17, 2002

Base:   3x10.D20
MMI:    1.50J
LH:     V2.04b

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3X10.D20 and can be installed together other D20 function groups.

        It is a general maintenance release and type approval candidate
        for the V3.10 and to keep the CDMA2000 customers on the most current
        base system and ease the use of other function groups, like GSM, TDMA.

Enhancements:
=============
	Bug fix: Trigger setting corrected in NSig


Known Bugs:
===========
        -/-

GPIB command set according to Excel sheet



***************************
CDMA2000 3X10.D20
***************************

Date:   October 14, 2002

Base:   3x10.D20
MMI:    1.50J
LH:     V2.04b

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3X10.D20 and can be installed together other D15 function groups.

        It is a general maintenance release and type approval candidate
        for the V3.10 and to keep the CDMA2000 customers on the most current
        base system and ease the use of other function groups, like GSM, TDMA.

Known Bugs:
===========
        -/-

GPIB command set according to Excel sheet




***************************
CDMA2000 3X10.D15
***************************

Date:   October 1ß, 2002

Base:   3x10.D15
MMI:    1.50J
LH:     V2.04b

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3X10.D15 and can be installed together other D15 function groups

        It is a general maintenance release to keep the CDMA2000 customers
        on the most current base system and ease the use of other function
        groups, like GSM, TDMA.

Known Bugs:
===========
        -/-

GPIB command set according to Excel sheet

***************************
CDMA2000 3X10.D05
***************************

Date:   October 03, 2002

Base:   3x10.D05
MMI:    1.50I
LH:     V2.04a

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3X10.D05 and can be installed together other D05 function groups

        It is a general maintenance release to keep the CDMA2000 customers
        on the most current base system and ease the use of other function
        groups, like GSM, TDMA.

Known Bugs:
===========
        The signalling part of he CDMA2000 function groups does not appear in
        the reset dialog.

GPIB command set according to Excel sheet

***************************
CDMA2000 3X10.C15
***************************

Date:   September 24, 2002

Base:   3x10.C15
MMI:    1.50H
LH:     V2.04

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3X10.C15 and can be installed together other C15 function groups

        It is a general maintenance release to keep the CDMA2000 customers
        on the most current base system and ease the use of other function
        groups, like GSM, TDMA.

GPIB command set according to Excel sheet


***************************
CDMA2000 3X10.C05
***************************

Date:   September 12, 2002

Base:   3x10.C05
MMI:    1.50H
LH:     V2.04

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3X10.C05 and can be installed together other C05 function groups

        It is a general maintenance release to keep the CDMA2000 customers
        on the most current base system and ease the use of other function
        groups, like GSM, TDMA.


New Features:
=============
        The IMSI and MCC of a registered phone can be taken over to the user
        settings for later use like calls to not-yet-registered phones.

Enhancements:
=============
        Decoupled status requests / status responses from the rest of
        signalling messages for better responsiveness and more predictable
        handoff times.

Further Annotations:
====================

Standby/Access Probe Power
	Measurements running in the background must be switched OFF

GPIB command set according to Excel sheet

Known Bugs:
===========
        In rare circumstances, there may be a hang when aborting a TDSO
        call-in-progress by pressing Signal OFF


***************************
CDMA2000 3X10.C01
***************************

Date:   September 03, 2002

Base:   3x10.C01
MMI:    1.50G
LH:     V2.03b

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3X10.C01 and can be installed together other C01 function groups

        It is a general maintenance release to keep the CDMA2000 customers
        on the most current base system and ease the use of other function
        groups, like GSM, TDMA.


New Features:
=============
        -/-

Enhancements:
=============
        Trigger response in non signalling mode corrected
        Fixed a rare bug in the non signalling generator

Further Annotations:
====================

Standby/Access Probe Power
	Measurements running in the background must be switched OFF

GPIB command set according to Excel sheet

Known Bugs:
===========
        In rare circumstances, there may be a hang when aborting a TDSO
        call-in-progress by pressing Signal OFF


***************************
CDMA2000 3X10.B06
***************************

Date:   August 26, 2002

Base:   3x10.B05
MMI:    1.50F
LH:     V2.03a

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3X10.B05 and can be installed together other B01 function groups

        It is a general maintenance release to keep the CDMA2000 customers
        on the most current base system and ease the use of other function
        groups, like GSM, TDMA.


New Features:
=============
        -/-

Enhancements:
=============
        -/-

Further Annotations:
====================

Standby/Access Probe Power
	Measurements running in the background must be switched OFF

GPIB command set according to V3.09

Known Bugs:
===========
        In rare circumstances, there may be a hang when aborting a TDSO
        call-in-progress by pressing Signal OFF


***************************
CDMA2000 3X10.B03
***************************

Date:   August 23, 2002

Base:   3x10.B01
MMI:    1.50F
LH:     V2.03a

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3X10.B01 and can be installed together other B01 function groups

        It is a general maintenance release to keep the CDMA2000 customers
        on the most current base system and ease the use of other function
        groups, like GSM, TDMA.


New Features:
=============
        -/-

Enhancements:
=============
        Modulation non signalling OQPSK (FIXED)

Further Annotations:
====================

Standby/Access Probe Power
	Measurements running in the background must be switched OFF

GPIB command set according to V3.09

Known Bugs:
===========
        In rare circumstances, there may be a hang when aborting a TDSO
        call-in-progress by pressing Signal OFF



***************************
CDMA2000 3X10.B02
***************************

Date:   August 21, 2002

Base:   3x10.B01
MMI:    1.50F
LH:     V2.03a

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3X10.B01 and can be installed together other B01 function groups

        It is a general maintenance release to keep the CDMA2000 customers
        on the most current base system and ease the use of other function
        groups, like GSM, TDMA.


New Features:
=============
        -/-

Enhancements:
=============
        Various bugfixes.

Further Annotations:
====================

Standby/Access Probe Power
	Measurements running in the background must be switched OFF

GPIB command set according to V3.09

Known Bugs:
===========
        In rare circumstances, there may be a hang when aborting a TDSO
        call-in-progress by pressing SIgnal OFF


***************************
CDMA2000 3X10.B01
***************************

Date:   August 14, 2002

Base:   3x10.B01
MMI:    1.50E
LH:     X2.03

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3X10.B01 and can be installed together other B01 function groups

        It is a general maintenance release to keep the CDMA2000 customers
        on the most current base system and ease the use of other function
        groups, like GSM, TDMA.


New Features:
=============
        -/-

Enhancements:
=============
        Improved level auto ranging in certain circumstances


Further Annotations:
====================

Standby/Access Probe Power
	Measurements running in the background must be switched OFF

GPIB command set according to V3.09

Known Bugs:
===========
        In rare circumstances, there may be a hang when aborting a TDSO
        call-in-progress by pressing SIgnal OFF

        Pressing "Send SMS" twice fast in a row may trigger a system error.


***************************
CDMA2000 3X10.A55
***************************

Date:   July 30, 2002

Base:   3x10.A55
MMI:    1.50D
LH:     V2.03

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        3X10.A55 and can be installed together other A55 function groups

New Features:
=============
        SMS
        Extended trigger output
        Support for B17 (if you had one)
        Manual expected power


Further Annotations:
====================

Standby/Access Probe Power
	Measurements running in the background must be switched OFF

GPIB command set according to V3.09

Known Bugs:
===========
        In rare circumstances, there may be a hang when aborting a TDSO
        call-in-progress by pressing SIgnal OFF

        Pressing "Send SMS" twice fast in a row may trigger a system error.



***************************
CDMA2000 3X07.B35
***************************

Date:   June 19, 2002

Base:   V3.07 / V3.08
MMI:    1.30D
LH:     V2.02b

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        V3.07/V3.08 and can be installed together with TDMA/AMPS V3.07 and all
	other V3.07/V3.08 Function Groups

New Features:
=============

        Improved level range for Open Loop Power Response measurement
        Added support for CMU-B83 Var12/14


Further Annotations:
====================

Standby/Access Probe Power
	Measurements running in the background must be switched OFF

GPIB command set according to B33/B34 version (remote 3x07.b32.xls).

Known Bugs:
===========
        Rx frequency display in Band class 3 (JTACS) is not correct for
        channels 1 -- 799. However, this affects only the display, the
        frequency settings on the hardware are correct.


***************************
CDMA2000 3X07.B34
***************************

Date:   June 12, 2002

Base:   V3.07 / V3.08
MMI:    1.30D
LH:     V2.02a

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        V3.07/V3.08 and can be installed together with TDMA/AMPS V3.07 and all
	other V3.07/V3.08 Function Groups

New Features:
=============

        Corrected expected power handling for certain cases.
        Signalling trigger output disabled when SIGNAL OFF.
        NonSignalling trigger output disabled when generator OFF.
        Improved filtering for Access/Standby Probe measurement.


Further Annotations:
====================

Standby/Access Probe Power
	Measurements running in the background must be switched OFF

GPIB command set according to B32/B33 version (remote 3x07.b32.xls).

Known Bugs:
===========
        -/-


***************************
CDMA2000 3X07.B33
***************************

Date:   June 05, 2002

Base:   V3.07 / V3.08
MMI:    1.30D
LH:     V2.02a

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        V3.07/V3.08 and can be installed together with TDMA/AMPS V3.07 and all
	other V3.07/V3.08 Function Groups

New Features:
=============

        Expanded overrange reserve for Rx level.


Further Annotations:
====================

Standby/Access Probe Power
	Measurements running in the background must be switched OFF

GPIB command set according to B32 version (remote 3x07.b32.xls).

Known Bugs:
===========

With Access/Standby power measurement switched ON, CMU will transmit signal even if
	Signalling is switched OFF




***************************
CDMA2000 3X07.B32
***************************

Date:	May 30, 2002

Base:   V3.07 / V3.08
MMI:    1.30D
LH:     V2.02

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        V3.07/V3.08 and can be installed together with TDMA/AMPS V3.07 and all
	other V3.07/V3.08 Function Groups

New Features:
=============

        - / -


Further Annotations:
====================

Fix in NPOW measurement

Standby/Access Probe Power
	Measurements running in the background must be switched OFF

GPIB command set according extra xls-sheet (remote 3x07.b32.xls)

Known Bugs:
===========

With Access/Standby power measurement switched ON, CMU will transmit signal even if
	Signalling is switched OFF





***************************
CDMA2000 3X07.B31
***************************

Date:	May 23, 2002

Base:   V3.07 / V3.08
MMI:    1.30D
LH:     V2.02

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        V3.07/V3.08 and can be installed together with TDMA/AMPS V3.07 and all
	other V3.07/V3.08 Function Groups

New Features:
=============

        - / -


Further Annotations:
====================

Standby/Access Probe Power
	Measurements running in the background must be switched OFF

Various bug fixes

Better syncronization for Access/Standby power measurement

Power setting for OLTR measurement improved

GPIB command set according extra xls-sheet (remote 3x07.b31.xls)

Known Bugs:
===========

With Access/Standby power measurement switched ON, CMU will transmit signal even if
	Signalling is switched OFF



***************************
CDMA2000 3X07.B30
***************************

Date:	May 9, 2002

Base:   V3.07 / V3.08
MMI:    1.30B
LH:     V2.02

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        V3.07 and can be installed together with TDMA/AMPS V3.07 and all
	other V3.07 Function Groups

New Features:
=============

	- Service Option 55
	- User-definable delay for voice loopback
	- Confidence Level for FER in Overview Measurement
	- WPOW measurement in Connection Control
	- Enhanced Template for Gated Output Power measurement


Further Annotations:
====================

Standby/Access Probe Power
	Measurements running in the background must be switched OFF

Various bug fixes

Faster Handoffs

PROCedure:BSSignal:CHANnel:FFCH[?] now working

Changed and additional GPIB commands for Overview Channel Quality

Changed and additional GPIB commands for configuration of GOP template

Autoranging for Maximum Output Power enhanced

Due to the nature of the WPOW power detector, this measurement works best
in the level range around 0dBm (typically -10dBm to +30dBm on RF2). This
measurement is provided as a help to find the right the external attenuation
values for the given test setup.


GPIB command set according extra xls-sheet (remote 3x07.b30.xls)

Known Bugs:
===========

        - / -





***************************
CDMA2000 3X07.B28
***************************

Date:	April 17, 2002

Base:   V3.07
MMI:    1.20N
LH:     V2.01

General Remarks
===============

        This release of CDMA2000 software is based on the CMU base system
        V3.07 and can be installed together with GSM V3.07, TDMA V3.07.

New Features:
=============

	- Support for 8k/8k Enhanced Speech Coder (CMU-B85)
	- Support for IQ Access Board (CMU-B82)

	- Standby/Access Probe Power measurement
	- Open Loop Time Response measurement
	- Forward Power Control measurement

	- Test Data Service Option (Service Option 32)
	- Quick Paging Channel
	- Call reconfiguration: SO changes, RC changes


Further Annotations:
====================

Standby/Access Probe Power
	Measurements running in the background must be switched OFF

Known Bugs:
===========

        - / -

