********************************
V5.21
********************************

New features compared to V5.20

none

Bug fixes compared to V5.20

1. rare freezes when switching from remote to local mode solved
2. selftest problems with internal rf loopback and new frontends solved



********************************
V5.20
********************************

New features compared to V5.15

1. support of new CMU hardware boards:
	CMU-B21v14	 1135.4580.02
	CMU-B66/B68	 1135.5070.53
	Digital Board	 1100.1956.05 and product index: >=10.02
2. new SW option CMU-K49 2G continuous sync
3. selftest internal loopback supports new frontends (1100.3120.02, product index >=10.03) 

Bug fixes compared to V5.15

1. improved stability of the CMU GPIB interface


********************************
V5.15
********************************

New features compared to V5.14

none

Bug fixes compared to V5.14

1. Selftest accuracy of Aux Tx CMU-B96 level at high frequencies improved

Note:
Version V5.10 to V5.15 does not support these new hardware modules:
CMU-B21v14 1135.4580.02
CMU-B66/B68 1135.5070.53
Digital Board 1100.1956.05 and TAZ: >=10.02
If your CMU is equipped with any of these hardware modules install V5.08, V5.20 or higher


********************************
V5.14
********************************

New features compared to V5.13

none

Bug fixes compared to V5.13

1. Freeze when copying logs via CMU version manager on FMR7 CMUs fixed



********************************
V5.13
********************************

New features compared to V5.12

none

Bug fixes compared to V5.12

1. RF Power Trigger level settings (high, medium, low) were not handled correctly. This was already fixed in Base V5.07 and is now also fixed in the V5.1x branch.
2. Sporadic startup problems on CMUs equipped with FMR7 and B53 solved


********************************
V5.12
********************************

New features compared to V5.11

none

Bug fixes compared to V5.11

1. rare FMR7 CMU startup / initial function group use problems fixed



********************************
V5.11
********************************

New features compared to V5.10

1. none

Bug fixes compared to V5.10

1. FMR7 CMU reset does not freeze anymore when CF card was removed before
2. FW Update on FMR7 CMUs without IQIF board does not show any warnings and is speed up
3. stability of FMR7 CMU startup / initial function group use improved
4. FMR7 CMUs do not stop after FW update with "automatic install" and removed CF card
5. fixed GSM wired sync trigger problem on slave CMU



********************************
V5.10
********************************

New features compared to V5.05

1. Frequency dependent external attenuation has 100 instead of 50 steps now, RX and TX are configurable seperately
2. Tool for easier retrievement of log files at the command prompt
3. Support of Power Quicc III module CMU-B56var54 for CMU var10 (service tester)

Bug fixes compared to V5.05

none


********************************
V5.08
********************************

New features compared to V5.07

1. Support of new CMU hardware boards:
	CMU-B21v14	1135.4580.02
	CMU-B66/B68	1135.5070.53
	Digital Board	1100.1956.05 and TAZ: >=10.02
2. Support of Power Quicc III module CMU-B56var54 for CMU var10 (service tester)

Bug fixes compared to V5.07

none

!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!
Important Notes: 

1. The V5.08 is a new branch and not compatible to previous versions V5.00 to V5.07
   This means no function groups V5.00 to V5.07 can be installed on this base software V5.08
2. The V5.08 is later than the V5.1x releases. 
   It supports the new hardware (CMU-B21v14 1135.4580.02, CMU-B66/B68 1135.5070.53, Digital Board 1100.1956.05 and TAZ: >=10.02) but it does not contain any V5.1x features or bugfixes
3. Version V5.1x does not support the new hardware (CMU-B21v14 1135.4580.02, CMU-B66/B68 1135.5070.53, Digital Board 1100.1956.05 and TAZ: >=10.02)
!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!



********************************
V5.07
********************************

New features compared to V5.06

1. none

Bug fixes compared to V5.06

1. RF Power Trigger level settings (high, medium, low) were not handled correctly. This is fixed now.
2. On FMR7 CMUs software installation does not crash anymore when the CF card is removed during the installation process



********************************
V5.06
********************************

New features compared to V5.05

1. none

Bug fixes compared to V5.05

1. FMR7 CMU reset does not freeze anymore when CF card was removed before
2. FW Update on FMR7 CMUs without IQIF board does not show any warnings and is speed up
3. stability of FMR7 CMU startup / initial function group use improved
4. FMR7 CMUs do not stop after FW update with "automatic install" and removed CF card
5. fixed GSM wired sync trigger problem on slave CMU

Note: 
These bugfixes are not part of the V5.10 since the V5.06 was released later than the V5.10.
In the V5.1x branch the bugfixes are available since version V5.11


********************************
V5.05
********************************

New features compared to V5.04

1. support of new software options CMU-K18, CMU-K19, CMU-K25

Bug fixes compared to V5.04

1. Binary data transfer via GPIB was truncated sometimes. This caused problems in AGPS applications.




********************************
V5.04
********************************

New features compared to V5.03

1. new Rf spectrum command CONFigure:SPECtrum:CONTrol:MODe[?] to set the display mode (CUR, AVG, MIN, MAX)

Bug fixes compared to V5.03

1. combined command for user correction CONFigure:USER:CORRection:LOSS:TABLe did not adjust all parameters in the hardware
2. GPIB error handling with multiple commands seperated by semicolons in one line corrected



********************************
V5.03
********************************

New features compared to V5.01

none


Bug fixes compared to V5.01

1. rare crashes of the B83var22 during continuous selftest fixed
2. limit violations of frontend selftest fixed




********************************
V5.01
********************************

New features compared to V5.00

1. Support of the software option CMU-K90

Bug fixes compared to V5.00

1. Harddrives with huge internal write cache work without corrupting the file system
2. The return format of the SYSTEM:OPTION? command is compatible to previous CMU releases



********************************
V5.00
********************************

New features compared to V4.53

1. Support of CMUs equipped with a FMR7
2. New mode for GPIB subarray commands: average power (PAVG)
3. At the DOS prompt the US keyboard is active by default

Bug fixes compared to V4.53

1. Rare crashes of the CMU-B21v14 module in low ambient air temperatures fixed
2. Maintenance internal loopback tests work correctly with enabled external attenuation



********************************
V4.53
********************************

New features compared to V4.52

none

Bug fixes compared to V4.52

1. Rare crashes of the CMU-B56v54 WCDMA Signalling module in low ambient air temperatures fixed
2. Sporadic crashes of the signal generator in the Rf function group solved





********************************
V4.52
********************************

New features compared to V4.51

none

Bug fixes compared to V4.51

1. GPIB control was locked after creating new directories in the DATA menu




********************************
V4.50/V4.51
********************************

New features compared to V4.35

1. SW options CMU-K42 and CMU-K43 (GPRS/EGPRS) are available for CMU200var30 now
2. in the remote mode report display, the output can be filtered to show measurement results only 


Bug fixes compared to V4.35

1. FMR processor is correctly displayed at Setup->Hardware Equipment



********************************
V4.35
********************************

New features compared to V4.34

none

Bug fixes compared to V4.34

1. problem with 1xEV-DO band option handling in V4.34 solved
2. system crash when switching function groups in remote debug mode solved



********************************
V4.34
********************************

New features compared to V4.33

1. optmized GPIB performance for CMU200var10 (Service Tester)

Bug fixes compared to V4.33

none



********************************
V4.33
********************************

New features compared to V4.32

1. improved fan control for higher ambient air temperatures

Bug fixes compared to V4.32

none



********************************
V4.32
********************************

New features compared to V4.31

1. CMU200v10 (Service Tester) supports SW Option CMU-K53 (Bluetooth) now

Bug fixes compared to V4.31

none



********************************
V4.31
********************************

New features compared to V4.30

none

Bug fixes compared to V4.30

1. rare communication problems in the CMU-B68 selftest fixed
2. rare system crashes when switching between GSM DATS and WCDMA fixed



********************************
V4.30
********************************

New features compared to V4.24

1. K47, K48, U62, B99, B53v14 is supported for CMU200 Variant 10
2. Support for B85 Variant 22 speech coder
3. Audio THD measurement added


Bug fixes compared to V4.24

1. none



********************************
V4.24
********************************

New features compared to V4.23

none

Bug fixes compared to V4.23

1. compatibility problems with CDMA2000 and 1xEV-DO solved



********************************
V4.23
********************************

New features compared to V4.21

1. new remote command DEFault:RFGenerator:GLIStmode[?]
   sets the Rf generator list mode paramaters to their default values
2. Rf loopback in continuous selftest has adapted limits for frontends rev 8 and 9
3. Audio: new A-weithing filter
4. Audio: new Bandpass 500Hz...5kHz
5. Audio: upper limit of analyer and generator is 21kHz instead of 20kHz
6. Audio: the THD+N measurement additionally displays the SINAD value

Bug fixes compared to V4.21

1. the marker in Rf Spectrum returned sometimes incorrect power levels



********************************
V4.21
********************************

New features compared to V4.20

none

Bug fixes compared to V4.20

1. correct indication of the rf measurement status in the remote status register
2. the halt state in the continuous selftest works again



********************************
V4.20
********************************

New features compared to V4.15

1. Support of new IQIF board version 4
2. all CMU log files are also stored as Zip file
3. support of B54v54 (new PPC module)
4. support of B83v22 (new PPC module)
5. Rf Generator list mode
6. IQ versus slot retriggered


Bug fixes compared to V4.15

1. stability of continuous selftest improved




********************************
V4.15
********************************

New features compared to V4.10

1. Support of new RXTX board version 16


Bug fixes compared to V4.10

1. Stability of long term speech tests in WCDMA improved
2. sporadical internal system errors with FE power meter fixed
3. synronisation of GPIB comand "*OPC?" optimized



********************************
V4.10
********************************

New features compared to V4.01

1. New SW options K901, K902 and K903 instead of K100, K200 and K300
2. SW options can now also be enabled with this remote command:
   SYSTem:OPTions:ACTivation <string>


Bug fixes compared to V4.00

1. Stability of long term speech tests in WCDMA improved



********************************
V4.01
********************************

New features compared to V4.00

1. if the shutdown of the CMU is interrupted a check of the file structure
   of the harddisk is done during the next startup (FMR6 only)


Bug fixes compared to V4.00

none



********************************
V4.00
********************************

New features compared to V3.85

1. support of CMU200 variant 10 (service tester)
2. support of CMU200 variant 30 (non signalling tester)
3. new remote commands to configure binary data formats:
     SYSTem:REMote:FORMat:NUMeric IEEE754|SCPI
     SYSTem:REMote:FORMat:BORDer NORM|SWAP


Bug fixes compared to V3.85

none



********************************
V3.85
********************************

New features compared to V3.81

1. new option CMU-K14 FM stereo transmitter
2. smart alignment support for CDMA2000 and WCDMA


Bug fixes compared to V3.81

1. problems with CMU-B96 and frontpanel type FMR5+ fixed
2. Internal Aux TxW LoopPath 2 selftest in Maintenance Menu was failed when a CMU is equipped with WCDMA and DDC400 (CMU-U65v02)



********************************
V3.81
********************************

New features compared to V3.80

none

Bug fixes compared to V3.80

1. avoid red box when the generator is switched off immediately after changing the modulation type
2. sporadical startup problems with fast FMRs fixed
3. in maintenance menu : B96 loopback test also available for WCDMA

********************************
V3.80
********************************

New features compared to V3.61

1. 	support of wideband auxiliary tx genererator (B96)
2.	support of additional RX DSP (B55) on USU (B21v14) for DATS (K92)
3.	new measurement IQ vs Slot (K48)
4.	TCP/IP settings for B21v14 and B83 are available in "Setup" menu
5.	Frequency dependent attenuation extended to 50 adjustabe values


Bug fixes compared to V3.61

none


********************************
V3.61
********************************

New features compared to V3.60

1. 	new SW option K80 (all CDMA 2000 non signalling bands)

Bug fixes compared to V3.60

1.	Level errors when Tx or Rx only are active corrected
2.	IQIF board eprom is writable now
3.	continuous selftest also fails when Auxtx selftest is failed


********************************
V3.60
********************************

New features compared to V3.54

1.	base and functions groups can be installed in one step 
2.	Remote service tool can change and delete SW versions on the CMU
3.	CMU display can be switched completely off via remote (screen saver)
4. 	frequency dependent attenuation
5. 	auto detection if CMU is controlled via GPIB or COM port
6.	IF3 selftest for RXTX boards > rev. 12
7.	remote debug mode
8.	task priority management changed, e.g. if a generator or signalling is switched on in remote mode, it suppresses other CMU Tx signals
9.	System identity in maintenance menu shows more details about installed HW

Bug fixes compared to V3.54

1.	Fan does not go to full speed after continuous selftest
2.	Log files do not get lost after three CMU startups
3.	Rx measurements are better synchronized with correction processor settings 
4.	B95 settings do not get lost when switching off the CMU 


******************************************************************
Note:
If you upgrade a CMU from an older SW version to the V3.60, the FM calibration in maintenance menu must be executed.
******************************************************************



********************************
V3.54
********************************

New features compared to V3.53

none

Bug fixes compared to V3.53

1.      Handover / channel change problems in IS136/AMPS solved
2.      Selftests in maintenance menu works with B95 and U99 now
3.	Sporadical slot timing problems in GSM solved



********************************
V3.53
********************************

New features compared to V3.52

1.      RF spectrum Remote Marker returns X and Y value now

Bug fixes compared to V3.52

1.      increased timeout for Continuous selftest
2.      corrections for identity.dat file
3. 	GSM modulation measurement show no sporadical phase errors anymore on CMUs with a U65u04


********************************
V3.52
********************************

New features compared to V3.50:

1.   new RF Genarator modulation mode "DSB"
2.   new RF Genarator mode "Low Spur Mode"
2.   extended AUXTX Selftest in Maintenance Menu
1. HW options:
        B17             Support of I/Q-IF Board for RF and GSM

Bug fixes compared to V3.52

1. corrected handling of frequency alternation mode in rf generator
2. AUC Filter 300KHZ is set for AM loop during FM calibration
3. selftest problems in maintenance menu with digital board 2 solved


********************************
V3.50
********************************

New features compared to V3.42:

 1. changes in LH selftest
 2. RF Generator: FM Modulation added, only for TX
 3. changes in RF AUXTX: independent Generator objects for TX and AUXTX
 4. added tests in maintenance:      Internal AUXTX Loop P1
                                     Internal AUXTX Loop P2
                                     Internal RF Loop P2
 5. new remote commands:        SYSTem:OPTions:MEQuipment?
                                SYSTem:REMote:ADDRess:SECondary:UNMap

Bug fixes compared to V3.42:

 1. internal loopback test now works correctly after L1Copro Level Calibration
 2. adaptations for fast FMRs such as FMR6+


********************************
V3.42
********************************

Bug fixes compared to V3.41:

1. fixed Reset problem: RF Power versus Time is displayed correctly now
2. fixed system error which occured when recalling files of V3.21 and V3.25
3. fixed system error which occured when changing between GSM, BLTH, AMPS and IS136
4. fixed system error in bla.cpp
5. fixed rounding error when setting RF frequency
6. improved service tool for CMU-B21Var02

********************************
V3.41
********************************

Bug fixes compared to V3.40:

1.	improvement for CMU-B88 initialization
2.	correction of nonvolatile RAM consistency check during system startup

********************************
V3.40
********************************

New features compared to V3.21:

1.	HW Options:
	CMU-B95:	 	AUXTX Board
	CMU-U65 Var04:		WDDC400
	CMU-B88:		1xEV-DO for CMU-B83
2. 	Redesign of Data Menu: in recall the preselected tree from the save menu is selected
3.	Setup Menu: Baudrates for serial interface
4. 	speed improvements
5.	GotoLocal command *GTL for remote local switch for COM interface
6.	version check for recall Data
7.	hotkey selection remain even after a menu change
8.	added tests in maintenance: 	AUXTX Selftest
					Interal AUXTX Looptest
					Linkhandler Selftest
9.	ESC key doesn't open menu select anymore

Bug fixes compared to V3.21:

1.	prefered menu mechanism improved for remote local switch
2.	default measurement mechanism improved after partial reset

*******************************
V3.21
*******************************

New features compared to V3.20:

1. B82 option poll

Bug fixes compared to V3.20

1. correction for taskexception when changing from remote to local
2. fixed bug in RF concerning Reference Marker
3. digital board WADC works also correctly now when an IQIF board is present
4. filter handling in correction processor modified to solve problems according spectrum measurements
5. B85 option poll results can also be queried in remote mode now
6. Startup problems on CMUs equipped with B83 solved

MS Base SW V3.21 works with all V3.2X function groups.

*******************************
V3.20
*******************************
New features compared to V3.10:

1. HW options:
	B9		AUXTX Board for CRTU
	B21 Var14	USU
	B52 Var14	Speech Coder for CMU B21 Var14
	B53 Var14	Signalling Module for Bluetooth
	B54 Var14	Signalling Module for GSM/TDMA/AMPS
	B78		L1Copro for BTS
	B95		Additional RF Generator
2. SW Options:
	K38		Uplink Generator for GSM-BTS
	K45		AMR @ GSM-MS
3. measurement statusbits to report asynchronous events to the remote interface
4. new GotoLocal command *GTL for remote local switch


Bug fixes compared to V3.10:

1. correction processor version string is displayed completely now
2. fixed bug in remote trace when switched frequently between LOCAL and REMOTE
3. eliminated flickering of notice messages
4. fixed bug occuring when recalling files from floppy or PCMCIA card on FMR6
5. separate start screen for CRTU-RU
6. changed message to "Unable to match contents. Please check input" if a wrong keycode was fed in
7. K0 now enables K43
8. bug fix for versionmanager:  Update Base with new Service Pack works again
9. bug fix for remote local transition


*****************************
V3.10
*****************************

New features compared to V3.08

1.  Save - Recall functionality: user configurations of individual function groups can be stored to a file and recalled
2.  partial reset: reset of individual function groups possible
3.  I/Q-IF Features: CMU B17/CRTU-B7
4.  on-screen help available
5.  RF trigger: redefined trigger level settings and configurable output connector for internal trigger signal
6.  RF narrow band power measurement available in manual control
7.  High contrast: A darker display can be set for high contrast
8.  TRACE: new commands for remote display
9.  improved Version Manager: no reboot necessary during installation
10. added temperature warning message box for CMU hardware overheat
11. logging features
12. RF power: Four different display modes evaluating the Current, Average, Maximum and Minimum measurement curve are available
13. Audio measurement: second audio circuit available in manual control
14. status reporting system
15. reference frequency: new command to monitor whether the CMU is synchronized to the reference frequency

Bug fixes compared to V3.08

1. fixed bug in RF Analyzer ResolutionBandWith
2. corrected extension of *.wmf files in print menu
3. some corrections for innerloop selftest

*****************************
V3.08
*****************************


New features compared to V3.07



Bug fixes compared to V3.07

1. fixed FE diagnose problem occuring with B66/B68 in continuous selftest
2. fixed bug in FM calibration occuring in the combination AMPS + Bluetooth
3. fixed bug in Version manager
4. fixed system error occuring on CMUs with many options available (overlay.c, column.c)
5. fixed system error in CMU-Z6 calibration.


****************************
V3.07
****************************

New features compared to V3.05

1.  L1 Coproboard B66/B68 is displayed correctly.
    Version and date of B66/B68 are displayed in the option display.
2.  FM Calibration:
	2.1 new result display
	2.2 works with and without B21
	2.3 possible with U99
	2.4 AMPS FM Calibration is now possible with B21 at LH Slot 2
3.  HW options:
	4.1 B82, B85 HW options are now supplied by option display
	4.2. new option B73
4.  defaultsets of baudrate in SETUP:COMM menu are independent of application
5.  support for FMR6
6.  NPOW in RF function group in remote mode.
    the frequency value is returned in NPOW with read/fetch/sample.
7.  loggings of firmware udate and versionmanager are stored in the internal/tools directory


Bug fixes compared to V3.05

1. fixed taskexception error at shutdown
2. Versionmanager V2.12: fixed exit 11 message from Version 2.11


***************************
V3.05
***************************
New features compared to V3.00

1.  compatibility with new HW options
	1.1 B66 or B68: L1 Copro for WCDMA Generator
	1.2 B17 I/Q-IF Board
	1.3 B83 CDMA2000 Signalling Unit
	1.4 RXTX Board	HW release 12
	1.5 B99/U99 RF1 with RF2 Level Range
	1.6 B71 Abis Interface
2.  compatibility with SW options
	2.1 K83-K86 CDMA2000
	2.2 K42 GPRS
	2.3 K65,K66,K75,K76 WCDMA Generator
3.  data menu and file copy via IEC bus
4.  activate/deactivate functiongroup with option display - faster startup because function group is not loaded
5.  version manager now supports base system servicepacks and AMPS/IS136 is in one installation packet
6.  rf spectrum with statistics -averaging
7.  audio with full support of 2 channels
8.  support for possibility to switch from local to remote without changing the signalling state SYST:GTRM:COMP OFF
9.  possibility to switch off parameter storage in nvl ram - performance gain: SYSTem:NONVolatile:DISable
10. trigger features
	support for timing delay for measurement trigger
	support for trigger signal output to AUX3

Bug fixes compared to V3.00

1.  corrected trigger slope in rf generator
2.  bugfixes in audio dsp application
3.  fm-calibration bugfixes
4.  audio calibration bugfixes
5.  remote mode for HSD switches


***************************
V3.00
***************************

New features compared to V2.16:

1.  New structure of FW directory to enable separate installation of Base System and Function Groups.
2.  New Version Manager to combine separate installations of Base System and Function Groups.
3.  New design of menu select.
4.  Extra hotkey for Level Scale in RF Spektrum.
5.  Reduced measurement time of AF analyzer.
6.  Multitone audio measurement added.

7.  Command *OPT with improved output string.
8.  Support of FMR6 keyboard
9.  Correction procesor sw 5.81 .
10. Versionmanager now checks whether there is enough swap space on the
    CMU hard disk after the software installation.
11. New maintenance test for Abis Board (B71) in simulator mode (Loop Test).
12. Serial number is displayed in new format.

Bug Fixes compared to V2.16:

1.  Fixed sporadically existing startup problems.
2.  Corrected options display for B81.
3.  Trigger slope for RF corrected.



***************************
V2.16
***************************

Bug Fixes compared to V2.15:
1. AUDIO:  Audio measurement corrected: ANA2 measurement error with AC coupling 2V 50Hz resolved.

***************************
V2.15
***************************

New features compared to V2.12 :
1. BASE:   New L-control design of manual control.
           Added AM modulation generator in RF function group.
           Introduced the new setting IVAL (interpolated value)  for remote
           subarray commands.
2. AUDIO:  Expanded remote command for routing speech decoder output.
           ROUTe:SPDecoder DEFault | HANDset | ANALyzer | ANA1 | ANA2 | ABOTh
3. GSM MS: Added extended modulation measurement (I/Q imbalance / origin offset).
           Added non signalling EDGE generator.
           Added non signalling EDGE modulation measurements.
           Added non signalling EDGE power ramp.
           Added non signalling EDGE spectrum.
           Enhanced Power versus PCL measurement to 7 channels.
           Added Power versus Slot(table) measurement (signalling/non signalling).
           Added Power versus Frame(table) measurement (signalling/non signalling).
           Added Power versus Slot measurement (non signalling),
           Added CS1 traffic mode (signalling/synchronized mode).
           Starting time is now changeable in signalling state CEST.

Bug Fixes compared to V2.12:
1. BASE:   Stack overflow problem that caused system error in
           MMI.CPP during startup solved.
           Solved nonvolatile RAM problem that caused system errors in
           FIELD.C and NODE.C during startup.
           Fixed the RF spectrum overload problem.
           Correct the level of the RF generator output.
           New correction processor software V5.62 is used.
           Bug in SYST:REM:ADDR:SEC? command is corrected.
           Fixed bug in calculation of start value in CONF:RANGE commands.
2. GSM MS: Bit stream and audio loop incompatibility resolved.
           Handover fall back corrected in case of handoff origin was an
           audio menu.
           Power versus PCL does not measure idle bursts any more.
           Power versus Time displays lower template failure correctly.




***************************
V2.12
***************************

New features compared to V2.11 :
1. BASE:   Software option enable function is integrated
           (for CMU-Kxx options).
2. AUDIO:  New remote commands for the subsystem audio added.
           CONF:AFAN:PRIM|SEC:FILT:VBP:CFR[?]
           CONF:AFAN:PRIM|SEC:FILT:VBP:BWID[?]
           CONF:AFAN:PRIM|SEC:FILT:VBP:BPAS[?]
           CONF:AFAN:PRIM|SEC:FILT:WEIG[?]
           Remote commands READ|FETC|SAMP:AFAN:PRIM|SEC? changed.
3. GSM MS: New signalling state ALERTING is introduced.

Bug Fixes compared to V2.11:
1. BASE:   New correction processor software V5.42 is used.
           Bug in the NON VOLATILE RAM mechanism fixed
            - caused startup problems in V2.11 and V2.10 .
2. AUDIO:  Audio measurement corrected (settling time).
3. GSM MS: Autoranging works correctly in signalling mode
            - setting signalling channel none.
           Bug in setting of the IMSI of the SIM-Card is corrected.

***************************
V2.11
***************************

This version is based on MMI BASE rev. 2.10h.

Bug Fixes compared to V2.10:
1. GSM MS: BER measurement corrected and stabilized.
2. GSM MS: Combined channel and PCL change stabilized.


***************************
V2.10
***************************

This version is based on MMI BASE rev. 2.10h.
No changes.

Note: Autoranging is now implemented.
      Default setting for Autoranging is ON in GSM MS and RF functions groups.
      To ensure compatibility with earlier versions switch Autoranging OFF using the remote command
		SENSE:LEVEL:MODE MANUAL
      This command must be invoked for every function group (=secondary address) that is used.


***************************
V2.05
***************************

New features compared to V2.04
1. BASE: new correction processor software 5.20 prepared for future variant
   of RXTX board

***************************
V2.04
***************************

New features compared to V2.03
1. BASE: new correction processor software 5.10 prepared for future variant
   of RXTX board

Bux fixes compared to V2.03:
1. BASE: Fixed two bugs in remote control that could occur on a "Device Clear"
   command


***************************
V2.03
***************************

New features compared to 2x01.c12:
1. BASE: new correction processor software 5.08
2. GSM MS: Combined powerramp / modulation measurement returns results of
   the powerramp measurement even if the modulation measurement fails

Bux fixes compared to 2x01.c12:
1. BASE: Fixed a bug in the firmware update after board change


***************************
V2.02
***************************

Bug Fixes compared to V2.00 :
1.  BASE: Upgrade to correction processor SW 5.06.
2.  BASE: The remote command "device clear" does not anymore produce a system
    error in SCPI.C .
3.  BASE: Added delays on correction processor self test.
4:  BASE: Changed tolerances of self test for frequencies > 2.2 GHz .
5.  GSM MS P/PCL: Fixed several minor problems.
6.  GSM MS: Spectrum is measured only on first hopping channel.
7.  GSM MS: Improved timeout handling of the combined power/modulation
    measurement.
8.  GSM MS BER: Improved structure of measurement task.
9.  GSM MS NSig: Fixed a bug of the GSM generator that occasionally caused
    a too long burst.
10. GSM AUDIO: Corrected a 3 dB level error in the speech coder.
11. GSM AUDIO: Changed measurement time.
12. Corrected several buggy remote commands.

New features compared to V2.00 :
1.  BASE: Generators keep their current state on a remote-to-local transition.
2.  BASE: Added serial number to output of "identity.dat".
3.  GSM MS: Handover fallback (CMU returns to synchronized state in origin
    network after call release in handover network).
4.  AUDIO: Distortion measurement.
5.  AUDIO: DC-measurement (only available in DC mode).
6.  AUDIO: Second audio analyzer (only available in remote mode).

***************************
V2.00
***************************

Bug Fixes compared to 2x00.l14 :
1. GSM MS: Modulation - Phase Error Results corrected.



