*******************************
V5.20
*******************************

New Features in V5.20 compared to V5.10:

none

Bug fixes compared to V5.10:

none

*******************************
V5.10
*******************************

New Features in V5.10 compared to V5.00:

none

Bug fixes compared to V5.00:

none

*******************************
V5.00
*******************************

New Features in V5.00 compared to V4.20:

none

Bug fixes compared to V4.20:

none


*******************************
V4.20
*******************************

New Features in V4.20 compared to V4.15:

none

Bug fixes compared to V4.15:

none


*******************************
V4.15
*******************************

New Features in V4.15 compared to V4.10:

none

Bug fixes compared to V4.15:

none



*******************************
V4.10
*******************************

New Features in V4.10 compared to V4.00:

none

Bug fixes compared to V4.00:

none




*******************************
V4.00
*******************************

New Features in V4.00 compared to V3.80:

none

Bug fixes compared to V3.80:

none



*******************************
V3.80
*******************************

New Features in V3.80 compared to V3.60:

none

Bug fixes compared to V3.60:

none


*******************************
V3.60
*******************************

New Features in V3.60 compared to V3.52:

1. IS136 Signalling: Formatted output for ESN and MSID.
2. IS136 Signalling: Alphanumeric SID transmission can be disabled.
3. IS136 Measuements: Support for the remote status bit "Measurement Results
   invalid".
4. AMPS Signalling: Formatted output for SN and MSID.
5. AMPS Measurements: SAT filter band width is now adjustable.
6. AMPS Measurements: Crest factor is now adjustable.
7. AMPS Measurements: Support for phone compressor.
8. AMPS Measurements: New modulator source : Mod. extern Ref

Bug fixes compared to V3.52:
1. IS136 and AMPS Signalling: Handoff improvements.


*******************************
V3.52
*******************************

New Features in V3.52 compared to V3.51:

1. IS136 Signalling: Equalization of CONF: and PROC: commands.
2. IS136 Signalling: Extended ESN remote command returns ESN in hex.
3. AMPS Signalling: Added Wideband Data Measurement.
4. AMPS Signalling: Extended SN remote command returns SN in hex.


*******************************
V3.51
*******************************

New Features in AMPS V3.51 compared to V3.50:

1. AMPS Signalling: Equalization of CONF: and PROC: commands.
2. AMPS RX Tests Sensitivity: Selectable notch filter.
3. AMPS RX Tests AF Analyzer: Selectable notch filter.
4. TX Test AF Level Search: Selectable Peak Measurement.

Bug fixes in AMPS V3.51 compared to V3.50:

1. AMPS Signalling: Registration issues with certain mobile chipsets fixed,
   see known problems V3.50 section 1.


*******************************
V3.50
*******************************

Bug fixes compared to V3.42:

1. AMPS FM Calibration: Works again if IS136 was selected before the AMPS FM Calibration
2. improvement for AMPS RX Test Hum&Noise: Holdofftime set to 75ms

Known Problems:

1. AMPS Signalling: Some mobiles habe problems with registration because the CMU sends the registration
   order confirmation inside the overhead message train. Try to make a (emergency) call from the mobile
   to establish a connection.


*******************************
V3.42
*******************************

Bug fixes compared to V3.41:

1. bugfix for systemerror ampscmr.cpp
2. bugfix for wrong connector settings after reset


********************************
V3.41
********************************

Bug fixes compared to V3.40:

1.	improvement for AMPS Generator

***************************
IS1MV3.40
***************************

General Remarks
===============

This release of IS1M software is based on the CMU base system V3.40 and can be
installed together with all other V3.40 Function Groups


New Features in IS136 V3.40 compared to V3.20
=============================================

* Bugfix: traffic channel change during established call on USU
* Bugfix: handoff parameter changes after handoff target selection


New Features in AMPS V3.40 compared to V3.20
============================================

* Bugfix: handoff while RX Test Hum&Noise is running
* Bugfix: handoff parameter changes after handoff target selection



