  Digistant Demo 4462					Readme.txt
  ===================

  On Diskette 1 are the following files:
  --------------------------------------------------
  - Liesmich.txt
    Textfile with common notes (german)

  - Readme.txt
    Textfile with common notes (english)

  - SetupEnglish.exe
    Start file, to open the  the english version of the LabWindows Setup program 
    and to install the program Demo 4462.

  - SetupDeutsch.exe
    Start file, to open the  the german version of the LabWindows Setup program 
    and to install the program Demo 4462.
	 
  - Demo4462.001
    Packed file, to be unpacked by Setup.

  - 4462_rs.bas  
    Programming sample in Q-Basic V4.5 for serial interface RS232 on COM1.
	  
  - 4462_rs.exe
    Executable program of the programming sample 4462_rs.bas.

  - 4462_iec.bas
    Programmers sample in Q-Basic V4.5 for the IEEE-488 interface.
    This program refers to the IEEE-488-card AT-GPIB/TNT from National Instruments.
    The used IEEE-488 functions are described in the manual ot the NI-hardware.
	
  - 4462_iec.bat
    Batch-file to load the IEEE-bus libraries for the program 4462_iec.bas.

  - 4462_iec.exe
    Executable program of the programming sample 4462_iec.bas.



  On Diskette 2 is the file:
  ---------------------------------------
  - Demo4462.002
    Packed file, to be unpacked by Setup (on Diskette 1).


  ==============================================================================================


  System Requirements for Program: Demo 4462
  ------------------------------------------

  Processor:			at least 80386 or greater
  Graphics:			at least Standard VGA 640 * 480; 256 colours
  Memory:			at least 32 MB RAM (Win 95, Win 98, Win NT 4.0) and at least 128 MB Ram (Win ME, Win 2000, Win XP)
  Hard disc:			approx. 15 MByte free memory
  Temporary Windows Dir.:	approx. 20 MB
  Operating systems:		Windows 95, Windows 98, Windows Me, Windows NT 4.0, Windows 2000, Windows XP


  Installation note Demo 2304:
  -----------------------------
  Start Setup.exe (Deutsch or English) from Diskette 1. The Demo 4462 Setup program
  will then guide you through the whole installation.

  Two directory paths are needed:
  1. Path for the LabWindows/CVI Run-Time engine
  2. Path for installation of the Demo 4462

  The Setup program creates a program folder in the start directory
  and copies into this the required files (Demo 4462) and the Deinstallation 
  Program (Deinstall Demo 4462).

  When the program is running, please enter the correct interface configuration 
  in Menu 'Settings--> Interface'.

 
  ==============================================================================================


  For your own program development, you can download the instrument
  driver for the Digistant 4462, which can be used for LAbWindows CVI 
  und LabView von National Instruments, from our Homepage at www.burster.de   

  T. Meder / 12.06.2002	