IEEE8021-PAE-MIB DEFINITIONS ::= BEGIN

-- ---------------------------------------------------------- --
-- IEEE 802.1X MIB
-- ---------------------------------------------------------- --

IMPORTS
    MODULE-IDENTITY, OBJECT-TYPE, Counter32, Counter64,
    Unsigned32, TimeTicks
        FROM SNMPv2-SMI
    MacAddress, TEXTUAL-CONVENTION, TruthValue
        FROM SNMPv2-TC
    MODULE-COMPLIANCE, OBJECT-GROUP
        FROM SNMPv2-CONF
    SnmpAdminString
        FROM SNMP-FRAMEWORK-MIB
    InterfaceIndex
        FROM IF-MIB
    ;

ieee8021paeMIB MODULE-IDENTITY
    LAST-UPDATED "200101160000Z"
    ORGANIZATION "IEEE 802.1 Working Group"
    CONTACT-INFO
        "http://grouper.ieee.org/groups/802/1/index.html"
    DESCRIPTION
        "The Port Access Entity module for managing IEEE
        802.1X."
    ::= { iso(1) std(0) iso8802(8802) ieee802dot1(1)
          ieee802dot1mibs(1) 1 }

paeMIBObjects OBJECT IDENTIFIER ::= { ieee8021paeMIB 1 }

-- ---------------------------------------------------------- --
-- Textual Conventions
-- ---------------------------------------------------------- --

PaeControlledDirections ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
        "The control mode values for the Authenticator PAE."
    SYNTAX      INTEGER {
                    both(0),
                    in(1)
                }

PaeControlledPortStatus ::= TEXTUAL-CONVENTION
    STATUS       current
    DESCRIPTION
        "The status values of the Authenticator PAE controlled
        Port."
    SYNTAX      INTEGER {
                    authorized(1),
                    unauthorized(2)
                }

PaeControlledPortControl ::= TEXTUAL-CONVENTION
    STATUS       current
    DESCRIPTION
        "The control values of the Authenticator PAE controlled
        Port."
    SYNTAX      INTEGER {
                    forceUnauthorized(1),
                    auto(2),
                    forceAuthorized(3)
                }

-- ---------------------------------------------------------- --

-- ---------------------------------------------------------- --
-- groups in the PAE MIB
-- ---------------------------------------------------------- --

dot1xPaeSystem        OBJECT IDENTIFIER ::= { paeMIBObjects 1 }
dot1xPaeAuthenticator OBJECT IDENTIFIER ::= { paeMIBObjects 2 }
dot1xPaeSupplicant    OBJECT IDENTIFIER ::= { paeMIBObjects 3 }

-- ---------------------------------------------------------- --

-- ---------------------------------------------------------- --
-- The PAE System Group
-- ---------------------------------------------------------- --

dot1xPaeSystemAuthControl OBJECT-TYPE
    SYNTAX      INTEGER { enabled(1), disabled(2) }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The administrative enable/disable state for
         Port Access Control in a System."
    REFERENCE
        "9.6.1, SystemAuthControl"
    ::= { dot1xPaeSystem 1 }

-- ---------------------------------------------------------- --
-- The PAE Port Table
-- ---------------------------------------------------------- --

dot1xPaePortTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF Dot1xPaePortEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A table of system level information for each port
        supported by the Port Access Entity.  An entry appears
        in this table for each port of this system."
    REFERENCE
        "9.6.1"
    ::= { dot1xPaeSystem 2 }

dot1xPaePortEntry OBJECT-TYPE
    SYNTAX      Dot1xPaePortEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The Port number, protocol version, and
        initialization control for a Port."
    INDEX { dot1xPaePortNumber }
    ::= { dot1xPaePortTable 1 }

Dot1xPaePortEntry ::=
    SEQUENCE {
        dot1xPaePortNumber
            InterfaceIndex,
        dot1xPaePortProtocolVersion
            Unsigned32,
        dot1xPaePortCapabilities
            BITS,
        dot1xPaePortInitialize
            TruthValue,
        dot1xPaePortReauthenticate
            TruthValue
        }

dot1xPaePortNumber OBJECT-TYPE
    SYNTAX      InterfaceIndex
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The Port number associated with this Port."
    REFERENCE
        "9.6.1, Port number"
    ::= { dot1xPaePortEntry 1 }

dot1xPaePortProtocolVersion OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The protocol version associated with this Port."
    REFERENCE
        "9.6.1, Protocol version"
    ::= { dot1xPaePortEntry 2 }

dot1xPaePortCapabilities OBJECT-TYPE
    SYNTAX      BITS {
                    dot1xPaePortAuthCapable(0),
                        -- Authenticator functions are supported
                    dot1xPaePortSuppCapable(1)
                        -- Supplicant functions are supported
                }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates the PAE functionality that this Port
        supports and that may be managed through this MIB."
    REFERENCE
        "9.6.1, PAE Capabilities"
    ::= { dot1xPaePortEntry 3 }

dot1xPaePortInitialize OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The initialization control for this Port. Setting this
        attribute TRUE causes the Port to be initialized.
        The attribute value reverts to FALSE once initialization
        has completed."
    REFERENCE
        "9.6.1.2, Initialize Port"
    ::= { dot1xPaePortEntry 4 }

dot1xPaePortReauthenticate OBJECT-TYPE
  SYNTAX TruthValue
  MAX-ACCESS read-write
  STATUS current
  DESCRIPTION
    "The reauthentication control for this port. Setting
    this attribute TRUE causes the Authenticator PAE state
    machine for the Port to reauthenticate the Supplicant.
    Setting this attribute FALSE has no effect.
    This attribute always returns FALSE when it is read."
  REFERENCE
    "9.4.1.3 Reauthenticate"
::= { dot1xPaePortEntry 5 }

-- ---------------------------------------------------------- --
-- The PAE Authenticator Group
-- ---------------------------------------------------------- --

-- ---------------------------------------------------------- --
-- The Authenticator Configuration Table
-- ---------------------------------------------------------- --

dot1xAuthConfigTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF Dot1xAuthConfigEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A table that contains the configuration objects for the
        Authenticator PAE associated with each port.
        An entry appears in this table for each port that may
        authenticate access to itself."
    REFERENCE
        "9.4.1 Authenticator Configuration"
    ::= { dot1xPaeAuthenticator 1 }

dot1xAuthConfigEntry OBJECT-TYPE
    SYNTAX      Dot1xAuthConfigEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The configuration information for an Authenticator
        PAE."
    INDEX { dot1xPaePortNumber }
    ::= { dot1xAuthConfigTable 1 }

Dot1xAuthConfigEntry ::=
    SEQUENCE {
        dot1xAuthPaeState
            INTEGER,
        dot1xAuthBackendAuthState
            INTEGER,
        dot1xAuthAdminControlledDirections
            PaeControlledDirections,
        dot1xAuthOperControlledDirections
            PaeControlledDirections,
        dot1xAuthAuthControlledPortStatus
            PaeControlledPortStatus,
        dot1xAuthAuthControlledPortControl
            PaeControlledPortControl,
        dot1xAuthQuietPeriod
            Unsigned32,
        dot1xAuthTxPeriod
            Unsigned32,
        dot1xAuthSuppTimeout
            Unsigned32,
        dot1xAuthServerTimeout
            Unsigned32,
        dot1xAuthMaxReq
            Unsigned32,
        dot1xAuthReAuthPeriod
            Unsigned32,
        dot1xAuthReAuthEnabled
            TruthValue,
        dot1xAuthKeyTxEnabled
            TruthValue
        }

dot1xAuthPaeState OBJECT-TYPE
    SYNTAX      INTEGER {
                    initialize(1),
                    disconnected(2),
                    connecting(3),
                    authenticating(4),
                    authenticated(5),
                    aborting(6),
                    held(7),
                    forceAuth(8),
                    forceUnauth(9)
                }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The current value of the Authenticator PAE state
        machine."
    REFERENCE
        "9.4.1, Authenticator PAE state"
    ::= { dot1xAuthConfigEntry 1 }

dot1xAuthBackendAuthState OBJECT-TYPE
    SYNTAX      INTEGER {
                    request(1),
                    response(2),
                    success(3),
                    fail(4),
                    timeout(5),
                    idle(6),
                    initialize(7)
                }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The current state of the Backend Authentication
        state machine."
    REFERENCE
        "9.4.1, Backend Authentication state"
    ::= { dot1xAuthConfigEntry 2 }

dot1xAuthAdminControlledDirections OBJECT-TYPE
    SYNTAX      PaeControlledDirections
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The current value of the administrative controlled
        directions parameter for the Port."
    REFERENCE
        "9.4.1, Admin Control Mode"
    ::= { dot1xAuthConfigEntry 3 }

dot1xAuthOperControlledDirections OBJECT-TYPE
    SYNTAX      PaeControlledDirections
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The current value of the operational controlled
        directions parameter for the Port."
    REFERENCE
        "9.4.1, Oper Control Mode"
    ::= { dot1xAuthConfigEntry 4 }

dot1xAuthAuthControlledPortStatus OBJECT-TYPE
    SYNTAX      PaeControlledPortStatus
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The current value of the controlled Port
        status parameter for the Port."
    REFERENCE
        "9.4.1, AuthControlledPortStatus"
    ::= { dot1xAuthConfigEntry 5 }

dot1xAuthAuthControlledPortControl OBJECT-TYPE
    SYNTAX      PaeControlledPortControl
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The current value of the controlled Port
        control parameter for the Port."
    REFERENCE
        "9.4.1, AuthControlledPortControl"
    ::= { dot1xAuthConfigEntry 6 }

dot1xAuthQuietPeriod OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value, in seconds, of the quietPeriod constant
        currently in use by the Authenticator PAE state
        machine."
    REFERENCE
        "9.4.1, quietPeriod"
    DEFVAL { 60 }
    ::= { dot1xAuthConfigEntry 7 }

dot1xAuthTxPeriod OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value, in seconds, of the txPeriod constant
        currently in use by the Authenticator PAE state
        machine."
    REFERENCE
        "9.4.1, txPeriod"
    DEFVAL { 30 }
    ::= { dot1xAuthConfigEntry 8 }

dot1xAuthSuppTimeout OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value, in seconds, of the suppTimeout constant
        currently in use by the Backend Authentication state
        machine."
    REFERENCE
        "9.4.1, suppTimeout"
    DEFVAL { 30 }
    ::= { dot1xAuthConfigEntry 9 }

dot1xAuthServerTimeout OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value, in seconds, of the serverTimeout constant
        currently in use by the Backend Authentication state
        machine."
    REFERENCE
        "9.4.1, serverTimeout"
    DEFVAL { 30 }
    ::= { dot1xAuthConfigEntry 10 }

dot1xAuthMaxReq OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value of the maxReq constant currently in use by
        the Backend Authentication state machine."
    REFERENCE
        "9.4.1, maxReq"
    DEFVAL { 2 }
    ::= { dot1xAuthConfigEntry 11 }

dot1xAuthReAuthPeriod OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value, in seconds, of the reAuthPeriod constant
        currently in use by the Reauthentication Timer state
        machine."
    REFERENCE
        "9.4.1, reAuthPeriod"
    DEFVAL { 3600 }
    ::= { dot1xAuthConfigEntry 12 }

dot1xAuthReAuthEnabled OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The enable/disable control used by the Reauthentication
        Timer state machine (8.5.5.1)."
    REFERENCE
        "9.4.1, reAuthEnabled"
    DEFVAL { false }
    ::= { dot1xAuthConfigEntry 13 }

dot1xAuthKeyTxEnabled OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value of the keyTransmissionEnabled constant
        currently in use by the Authenticator PAE state
        machine."
    REFERENCE
        "9.4.1, keyTransmissionEnabled"
    ::= { dot1xAuthConfigEntry 14 }

-- ---------------------------------------------------------- --
-- The Authenticator Statistics Table
-- ---------------------------------------------------------- --

dot1xAuthStatsTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF Dot1xAuthStatsEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A table that contains the statistics objects for the
         Authenticator PAE associated with each Port.
         An entry appears in this table for each port that may
         authenticate access to itself."
    REFERENCE
        "9.4.2 Authenticator Statistics"
    ::= { dot1xPaeAuthenticator 2 }

dot1xAuthStatsEntry OBJECT-TYPE
    SYNTAX      Dot1xAuthStatsEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The statistics information for an Authenticator PAE."
    INDEX { dot1xPaePortNumber }
    ::= { dot1xAuthStatsTable 1 }

Dot1xAuthStatsEntry ::=
    SEQUENCE {
        dot1xAuthEapolFramesRx
            Counter32,
        dot1xAuthEapolFramesTx
            Counter32,
        dot1xAuthEapolStartFramesRx
            Counter32,
        dot1xAuthEapolLogoffFramesRx
            Counter32,
        dot1xAuthEapolRespIdFramesRx
            Counter32,
        dot1xAuthEapolRespFramesRx
            Counter32,
        dot1xAuthEapolReqIdFramesTx
            Counter32,
        dot1xAuthEapolReqFramesTx
            Counter32,
        dot1xAuthInvalidEapolFramesRx
            Counter32,
        dot1xAuthEapLengthErrorFramesRx
            Counter32,
        dot1xAuthLastEapolFrameVersion
            Unsigned32,
        dot1xAuthLastEapolFrameSource
            MacAddress
        }

dot1xAuthEapolFramesRx OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of valid EAPOL frames of any type
        that have been received by this Authenticator."
    REFERENCE
        "9.4.2, EAPOL frames received"
    ::= { dot1xAuthStatsEntry 1 }

dot1xAuthEapolFramesTx OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of EAPOL frames of any type
        that have been transmitted by this Authenticator."
    REFERENCE
        "9.4.2, EAPOL frames transmitted"
    ::= { dot1xAuthStatsEntry 2 }

dot1xAuthEapolStartFramesRx OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of EAPOL Start frames that have
        been received by this Authenticator."
    REFERENCE
        "9.4.2, EAPOL Start frames received"
    ::= { dot1xAuthStatsEntry 3 }

dot1xAuthEapolLogoffFramesRx OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of EAPOL Logoff frames that have
        been received by this Authenticator."
    REFERENCE
        "9.4.2, EAPOL Logoff frames received"
    ::= { dot1xAuthStatsEntry 4 }

dot1xAuthEapolRespIdFramesRx OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of EAP Resp/Id frames that have
        been received by this Authenticator."
    REFERENCE
        "9.4.2, EAPOL Resp/Id frames received"
    ::= { dot1xAuthStatsEntry 5 }

dot1xAuthEapolRespFramesRx OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of valid EAP Response frames
        (other than Resp/Id frames) that have been
        received by this Authenticator."
    REFERENCE
        "9.4.2, EAPOL Response frames received"
    ::= { dot1xAuthStatsEntry 6 }

dot1xAuthEapolReqIdFramesTx OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of EAP Req/Id frames that have been
        transmitted by this Authenticator."
    REFERENCE
        "9.4.2, EAPOL Req/Id frames transmitted"
    ::= { dot1xAuthStatsEntry 7 }

dot1xAuthEapolReqFramesTx OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of EAP Request frames
        (other than Rq/Id frames) that have been
        transmitted by this Authenticator."
    REFERENCE
        "9.4.2, EAPOL Request frames transmitted"
    ::= { dot1xAuthStatsEntry 8 }

dot1xAuthInvalidEapolFramesRx OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of EAPOL frames that have been
        received by this Authenticator in which the
        frame type is not recognized."
    REFERENCE
        "9.4.2, Invalid EAPOL frames received"
    ::= { dot1xAuthStatsEntry 9 }

dot1xAuthEapLengthErrorFramesRx OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of EAPOL frames that have been received
        by this Authenticator in which the Packet Body
        Length field is invalid."
    REFERENCE
        "9.4.2, EAP length error frames received"
    ::= { dot1xAuthStatsEntry 10 }

dot1xAuthLastEapolFrameVersion OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The protocol version number carried in the
        most recently received EAPOL frame."
    REFERENCE
        "9.4.2, Last EAPOL frame version"
    ::= { dot1xAuthStatsEntry 11 }

dot1xAuthLastEapolFrameSource OBJECT-TYPE
    SYNTAX      MacAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The source MAC address carried in the
        most recently received EAPOL frame."
    REFERENCE
        "9.4.2, Last EAPOL frame source"
    ::= { dot1xAuthStatsEntry 12 }

-- ---------------------------------------------------------- --
-- The Authenticator Diagnostics Table
-- ---------------------------------------------------------- --

dot1xAuthDiagTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF Dot1xAuthDiagEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A table that contains the diagnostics objects for the
         Authenticator PAE associated with each Port.
         An entry appears in this table for each port that may
         authenticate access to itself."
    REFERENCE
        "9.4.3 Authenticator Diagnostics"
    ::= { dot1xPaeAuthenticator 3 }

dot1xAuthDiagEntry OBJECT-TYPE
    SYNTAX      Dot1xAuthDiagEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The diagnostics information for an Authenticator PAE."
    INDEX { dot1xPaePortNumber }
    ::= { dot1xAuthDiagTable 1 }

Dot1xAuthDiagEntry ::=
    SEQUENCE {
        dot1xAuthEntersConnecting
            Counter32,
        dot1xAuthEapLogoffsWhileConnecting
            Counter32,
        dot1xAuthEntersAuthenticating
            Counter32,
        dot1xAuthAuthSuccessWhileAuthenticating
            Counter32,
        dot1xAuthAuthTimeoutsWhileAuthenticating
            Counter32,
        dot1xAuthAuthFailWhileAuthenticating
            Counter32,
        dot1xAuthAuthReauthsWhileAuthenticating
            Counter32,
        dot1xAuthAuthEapStartsWhileAuthenticating
            Counter32,
        dot1xAuthAuthEapLogoffWhileAuthenticating
            Counter32,
        dot1xAuthAuthReauthsWhileAuthenticated
            Counter32,
        dot1xAuthAuthEapStartsWhileAuthenticated
            Counter32,
        dot1xAuthAuthEapLogoffWhileAuthenticated
            Counter32,
        dot1xAuthBackendResponses
            Counter32,
        dot1xAuthBackendAccessChallenges
            Counter32,
        dot1xAuthBackendOtherRequestsToSupplicant
            Counter32,
        dot1xAuthBackendNonNakResponsesFromSupplicant
            Counter32,
        dot1xAuthBackendAuthSuccesses
            Counter32,
        dot1xAuthBackendAuthFails
            Counter32
        }

dot1xAuthEntersConnecting OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Counts the number of times that the state machine
        transitions to the CONNECTING state from any other
        state."
    REFERENCE
        "9.4.2, 8.5.4.2.1"
    ::= { dot1xAuthDiagEntry 1 }

dot1xAuthEapLogoffsWhileConnecting OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Counts the number of times that the state machine
        transitions from CONNECTING to DISCONNECTED as a result
        of receiving an EAPOL-Logoff message."
    REFERENCE
        "9.4.2, 8.5.4.2.2"
    ::= { dot1xAuthDiagEntry 2 }

dot1xAuthEntersAuthenticating OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Counts the number of times that the state machine
        transitions from CONNECTING to AUTHENTICATING, as a
        result of an EAP-Response/Identity message being
        received from the Supplicant."
    REFERENCE
        "9.4.2, 8.5.4.2.3"
    ::= { dot1xAuthDiagEntry 3 }

dot1xAuthAuthSuccessWhileAuthenticating OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Counts the number of times that the state machine
        transitions from AUTHENTICATING to AUTHENTICATED, as a
        result of the Backend Authentication state machine
        indicating successful authentication of the Supplicant
        (authSuccess = TRUE)."
    REFERENCE
        "9.4.2, 8.5.4.2.4"
    ::= { dot1xAuthDiagEntry 4 }

dot1xAuthAuthTimeoutsWhileAuthenticating OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Counts the number of times that the state machine
        transitions from AUTHENTICATING to ABORTING, as a result
        of the Backend Authentication state machine indicating
        authentication timeout (authTimeout = TRUE)."
    REFERENCE
        "9.4.2, 8.5.4.2.5"
    ::= { dot1xAuthDiagEntry 5 }

dot1xAuthAuthFailWhileAuthenticating OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Counts the number of times that the state machine
        transitions from AUTHENTICATING to HELD, as a result
        of the Backend Authentication state machine indicating
        authentication failure (authFail = TRUE)."
    REFERENCE
        "9.4.2, 8.5.4.2.6"
    ::= { dot1xAuthDiagEntry 6 }

dot1xAuthAuthReauthsWhileAuthenticating OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Counts the number of times that the state machine
        transitions from AUTHENTICATING to ABORTING, as a result
        of a reauthentication request (reAuthenticate = TRUE)."
    REFERENCE
        "9.4.2, 8.5.4.2.7"
    ::= { dot1xAuthDiagEntry 7 }

dot1xAuthAuthEapStartsWhileAuthenticating OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Counts the number of times that the state machine
        transitions from AUTHENTICATING to ABORTING, as a result
        of an EAPOL-Start message being received
        from the Supplicant."
    REFERENCE
        "9.4.2, 8.5.4.2.8"
    ::= { dot1xAuthDiagEntry 8 }

dot1xAuthAuthEapLogoffWhileAuthenticating OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Counts the number of times that the state machine
        transitions from AUTHENTICATING to ABORTING, as a result
        of an EAPOL-Logoff message being received
        from the Supplicant."
    REFERENCE
        "9.4.2, 8.5.4.2.9"
    ::= { dot1xAuthDiagEntry 9 }

dot1xAuthAuthReauthsWhileAuthenticated OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Counts the number of times that the state machine
        transitions from AUTHENTICATED to CONNECTING, as a
        result of a reauthentication request
        (reAuthenticate = TRUE)."
    REFERENCE
        "9.4.2, 8.5.4.2.10"
    ::= { dot1xAuthDiagEntry 10 }

dot1xAuthAuthEapStartsWhileAuthenticated OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Counts the number of times that the state machine
        transitions from AUTHENTICATED to CONNECTING, as a
        result of an EAPOL-Start message being received from the
        Supplicant."
    REFERENCE
        "9.4.2, 8.5.4.2.11"
    ::= { dot1xAuthDiagEntry 11 }

dot1xAuthAuthEapLogoffWhileAuthenticated OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Counts the number of times that the state machine
        transitions from AUTHENTICATED to DISCONNECTED, as a
        result of an EAPOL-Logoff message being received from
        the Supplicant."
    REFERENCE
        "9.4.2, 8.5.4.2.12"
    ::= { dot1xAuthDiagEntry 12 }

dot1xAuthBackendResponses OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Counts the number of times that the state machine sends
        an initial Access-Request packet to the Authentication
        server (i.e., executes sendRespToServer on entry to the
        RESPONSE state). Indicates that the Authenticator
        attempted communication with the Authentication Server."
    REFERENCE
        "9.4.2, 8.5.6.2.1"
    ::= { dot1xAuthDiagEntry 13 }

dot1xAuthBackendAccessChallenges OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Counts the number of times that the state machine
        receives an initial Access-Challenge packet from the
        Authentication server (i.e., aReq becomes TRUE,
        causing exit from the RESPONSE state). Indicates that
        the Authentication Server has communication with
        the Authenticator."
    REFERENCE
        "9.4.2, 8.5.6.2.2"
    ::= { dot1xAuthDiagEntry 14 }

dot1xAuthBackendOtherRequestsToSupplicant OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Counts the number of times that the state machine
        sends an EAP-Request packet (other than an Identity,
        Notification, Failure or Success message) to the
        Supplicant (i.e., executes txReq on entry to the
        REQUEST state). Indicates that the Authenticator chose
        an EAP-method."
    REFERENCE
        "9.4.2, 8.5.6.2.3"
    ::= { dot1xAuthDiagEntry 15 }

dot1xAuthBackendNonNakResponsesFromSupplicant OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Counts the number of times that the state machine
        receives a response from the Supplicant to an initial
        EAP-Request, and the response is something other than
        EAP-NAK (i.e., rxResp becomes TRUE, causing the state
        machine to transition from REQUEST to RESPONSE,
        and the response is not an EAP-NAK). Indicates that
        the Supplicant can respond to the Authenticator's
        chosen EAP-method."
    REFERENCE
        "9.4.2, 8.5.6.2.4"
    ::= { dot1xAuthDiagEntry 16 }

dot1xAuthBackendAuthSuccesses OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Counts the number of times that the state machine
        receives an EAP-Success message from the Authentication
        Server (i.e., aSuccess becomes TRUE, causing a
        transition from RESPONSE to SUCCESS). Indicates that
        the Supplicant has successfully authenticated to
        the Authentication Server."
    REFERENCE
        "9.4.2, 8.5.6.2.5"
    ::= { dot1xAuthDiagEntry 17 }

dot1xAuthBackendAuthFails OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Counts the number of times that the state machine
        receives an EAP-Failure message from the Authentication
        Server (i.e., aFail becomes TRUE, causing a transition
        from RESPONSE to FAIL). Indicates that the Supplicant
        has not authenticated to the Authentication Server."
    REFERENCE
        "9.4.2, 8.5.6.2.6"
    ::= { dot1xAuthDiagEntry 18 }

-- ---------------------------------------------------------- --
-- The Authenticator Session Statistics Table
-- ---------------------------------------------------------- --

dot1xAuthSessionStatsTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF Dot1xAuthSessionStatsEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A table that contains the session statistics objects
        for the Authenticator PAE associated with each Port.
        An entry appears in this table for each port that may
        authenticate access to itself."
    REFERENCE
        "9.4.4"
    ::= { dot1xPaeAuthenticator 4 }

dot1xAuthSessionStatsEntry OBJECT-TYPE
    SYNTAX      Dot1xAuthSessionStatsEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The session statistics information for an Authenticator
        PAE.  This shows the current values being collected for
        each session that is still in progress, or the final
        values for the last valid session on each port where
        there is no session currently active."
    INDEX { dot1xPaePortNumber }
    ::= { dot1xAuthSessionStatsTable 1 }

Dot1xAuthSessionStatsEntry ::=
    SEQUENCE {
        dot1xAuthSessionOctetsRx
            Counter64,
        dot1xAuthSessionOctetsTx
            Counter64,
        dot1xAuthSessionFramesRx
            Counter32,
        dot1xAuthSessionFramesTx
            Counter32,
        dot1xAuthSessionId
            SnmpAdminString,
        dot1xAuthSessionAuthenticMethod
            INTEGER,
        dot1xAuthSessionTime
            TimeTicks,
        dot1xAuthSessionTerminateCause
            INTEGER,
        dot1xAuthSessionUserName
            SnmpAdminString
    }

dot1xAuthSessionOctetsRx OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of octets received in user data
        frames on this Port during the session."
    REFERENCE
        "9.4.4, Session Octets Received"
    ::= { dot1xAuthSessionStatsEntry 1 }

dot1xAuthSessionOctetsTx OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of octets transmitted in user data
        frames on this Port during the session."
    REFERENCE
        "9.4.4, Session Octets Transmitted"
    ::= { dot1xAuthSessionStatsEntry 2 }

dot1xAuthSessionFramesRx OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of user data frames received
        on this Port during the session."
    REFERENCE
        "9.4.4, Session Frames Received"
    ::= { dot1xAuthSessionStatsEntry 3 }

dot1xAuthSessionFramesTx OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of user data frames transmitted
        on this Port during the session."
    REFERENCE
        "9.4.4, Session Frames Transmitted"
    ::= { dot1xAuthSessionStatsEntry 4 }

dot1xAuthSessionId OBJECT-TYPE
    SYNTAX      SnmpAdminString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "A unique identifier for the session, in the
        form of a printable ASCII string of at least
        three characters."
    REFERENCE
        "9.4.4, Session Identifier"
    ::= { dot1xAuthSessionStatsEntry 5 }

dot1xAuthSessionAuthenticMethod OBJECT-TYPE
    SYNTAX      INTEGER {
                    remoteAuthServer(1),
                    localAuthServer(2)
                }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The authentication method used to establish the
        session."
    REFERENCE
        "9.4.4, Session Authentication Method"
    ::= { dot1xAuthSessionStatsEntry 6 }

dot1xAuthSessionTime OBJECT-TYPE
    SYNTAX      TimeTicks
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The duration of the session in seconds."
    REFERENCE
        "9.4.4, Session Time"
    ::= { dot1xAuthSessionStatsEntry 7 }

dot1xAuthSessionTerminateCause OBJECT-TYPE
    SYNTAX      INTEGER {
                    supplicantLogoff(1),
                    portFailure(2),
                    supplicantRestart(3),
                    reauthFailed(4),
                    authControlForceUnauth(5),
                    portReInit(6),
                    portAdminDisabled(7),
                    notTerminatedYet(999)
                    }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The reason for the session termination."
    REFERENCE
        "9.4.4, Session Terminate Cause"
    ::= { dot1xAuthSessionStatsEntry 8 }

dot1xAuthSessionUserName OBJECT-TYPE
    SYNTAX     SnmpAdminString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The User-Name representing the identity of the
        Supplicant PAE."
    REFERENCE
        "9.4.4, Session User Name"
    ::= { dot1xAuthSessionStatsEntry 9 }

-- ---------------------------------------------------------- --
-- The PAE Supplicant Group
-- ---------------------------------------------------------- --

-- ---------------------------------------------------------- --
-- The Supplicant Configuration Table
-- ---------------------------------------------------------- --

dot1xSuppConfigTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF Dot1xSuppConfigEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A table that contains the configuration objects for the
        Supplicant PAE associated with each port.
        An entry appears in this table for each port that may
        authenticate itself when challenged by a remote system."
    REFERENCE
        "9.5.1"
    ::= { dot1xPaeSupplicant 1 }

dot1xSuppConfigEntry OBJECT-TYPE
    SYNTAX      Dot1xSuppConfigEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The configuration information for a Supplicant PAE."
    INDEX { dot1xPaePortNumber }
    ::= { dot1xSuppConfigTable 1 }

Dot1xSuppConfigEntry ::=
    SEQUENCE {
        dot1xSuppPaeState
            INTEGER,
        dot1xSuppHeldPeriod
            Unsigned32,
        dot1xSuppAuthPeriod
            Unsigned32,
        dot1xSuppStartPeriod
            Unsigned32,
        dot1xSuppMaxStart
            Unsigned32
        }

dot1xSuppPaeState OBJECT-TYPE
    SYNTAX      INTEGER {
                    disconnected(1),
                    logoff(2),
                    connecting(3),
                    authenticating(4),
                    authenticated(5),
                    acquired(6),
                    held(7)
                }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The current state of the Supplicant PAE state
        machine (8.5.8)."
    REFERENCE
        "9.5.1, Supplicant PAE State"
    ::= { dot1xSuppConfigEntry 1 }

dot1xSuppHeldPeriod OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value, in seconds, of the heldPeriod
        constant currently in use by the Supplicant
        PAE state machine (8.5.8.1.2)."
    REFERENCE
        "9.5.1, heldPeriod"
    DEFVAL { 60 }
    ::= { dot1xSuppConfigEntry 2 }

dot1xSuppAuthPeriod OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value, in seconds, of the authPeriod
        constant currently in use by the Supplicant
        PAE state machine (8.5.8.1.2)."
    REFERENCE
        "9.5.1, authPeriod"
    DEFVAL { 30 }
    ::= { dot1xSuppConfigEntry 3 }

dot1xSuppStartPeriod OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value, in seconds, of the startPeriod
        constant currently in use by the Supplicant
        PAE state machine (8.5.8.1.2)."
    REFERENCE
        "9.5.1, startPeriod"
    DEFVAL { 30 }
    ::= { dot1xSuppConfigEntry 4 }

dot1xSuppMaxStart OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value of the maxStart constant currently in use by
        the Supplicant PAE state machine (8.5.8.1.2)."
    REFERENCE
        "9.5.1, maxStart"
    DEFVAL { 3}
    ::= { dot1xSuppConfigEntry 5 }

-- ---------------------------------------------------------- --
-- The Supplicant Statistics Table
-- ---------------------------------------------------------- --

dot1xSuppStatsTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF Dot1xSuppStatsEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A table that contains the statistics objects for the
        Supplicant PAE associated with each port.
        An entry appears in this table for each port that may
        authenticate itself when challenged by a remote system."
    REFERENCE
        "9.5.2"
    ::= { dot1xPaeSupplicant 2 }

dot1xSuppStatsEntry OBJECT-TYPE
    SYNTAX      Dot1xSuppStatsEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The statistics information for a Supplicant PAE."
    INDEX { dot1xPaePortNumber }
    ::= { dot1xSuppStatsTable 1 }

Dot1xSuppStatsEntry ::=
    SEQUENCE {
        dot1xSuppEapolFramesRx
            Counter32,
        dot1xSuppEapolFramesTx
            Counter32,
        dot1xSuppEapolStartFramesTx
            Counter32,
        dot1xSuppEapolLogoffFramesTx
            Counter32,
        dot1xSuppEapolRespIdFramesTx
            Counter32,
        dot1xSuppEapolRespFramesTx
            Counter32,
        dot1xSuppEapolReqIdFramesRx
            Counter32,
        dot1xSuppEapolReqFramesRx
            Counter32,
        dot1xSuppInvalidEapolFramesRx
            Counter32,
        dot1xSuppEapLengthErrorFramesRx
            Counter32,
        dot1xSuppLastEapolFrameVersion
            Unsigned32,
        dot1xSuppLastEapolFrameSource
            MacAddress
        }

dot1xSuppEapolFramesRx OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of EAPOL frames of any type
        that have been received by this Supplicant."
    REFERENCE
        "9.5.2, EAPOL frames received"
    ::= { dot1xSuppStatsEntry 1 }

dot1xSuppEapolFramesTx OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of EAPOL frames of any type
        that have been transmitted by this Supplicant."
    REFERENCE
        "9.5.2, EAPOL frames transmitted"
    ::= { dot1xSuppStatsEntry 2 }

dot1xSuppEapolStartFramesTx OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of EAPOL Start frames
        that have been transmitted by this Supplicant."
    REFERENCE
        "9.5.2, EAPOL Start frames transmitted"
    ::= { dot1xSuppStatsEntry 3 }

dot1xSuppEapolLogoffFramesTx OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of EAPOL Logoff frames
        that have been transmitted by this Supplicant."
    REFERENCE
        "9.5.2, EAPOL Logoff frames transmitted"
    ::= { dot1xSuppStatsEntry 4 }

dot1xSuppEapolRespIdFramesTx OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of EAP Resp/Id frames
        that have been transmitted by this Supplicant."
    REFERENCE
        "9.5.2, EAP Resp/Id frames transmitted"
    ::= { dot1xSuppStatsEntry 5 }

dot1xSuppEapolRespFramesTx OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of valid EAP Response frames
        (other than Resp/Id frames)
        that have been transmitted by this Supplicant."
    REFERENCE
        "9.5.2, EAP Resp frames transmitted"
    ::= { dot1xSuppStatsEntry 6 }

dot1xSuppEapolReqIdFramesRx OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of EAP Req/Id frames
        that have been received by this Supplicant."
    REFERENCE
        "9.5.2, EAP Req/Id frames received"
    ::= { dot1xSuppStatsEntry 7 }

dot1xSuppEapolReqFramesRx OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of EAP Request frames (other than Rq/Id
        frames) that have been received by this Supplicant."
    REFERENCE
        "9.5.2, EAP Req frames received"
    ::= { dot1xSuppStatsEntry 8 }

dot1xSuppInvalidEapolFramesRx OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of EAPOL frames that have been
        received by this Supplicant in which the
        frame type is not recognized."
    REFERENCE
        "9.5.2, Invalid EAPOL frames received"
    ::= { dot1xSuppStatsEntry 9 }

dot1xSuppEapLengthErrorFramesRx OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of EAPOL frames that have been
        received by this Supplicant in which the Packet
        Body Length field (7.5.5) is invalid."
    REFERENCE
        "9.5.2, EAP length error frames received"
    ::= { dot1xSuppStatsEntry 10 }

dot1xSuppLastEapolFrameVersion OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The protocol version number carried in the
        most recently received EAPOL frame."
    REFERENCE
        "9.5.2, Last EAPOL frame version"
    ::= { dot1xSuppStatsEntry 11 }

dot1xSuppLastEapolFrameSource OBJECT-TYPE
    SYNTAX      MacAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The source MAC address carried in the
        most recently received EAPOL frame."
    REFERENCE
        "9.5.2, Last EAPOL frame source"
    ::= { dot1xSuppStatsEntry 12 }

-- ---------------------------------------------------------- --
-- IEEE 802.1X MIB - Conformance Information
-- ---------------------------------------------------------- --

dot1xPaeConformance OBJECT IDENTIFIER ::= { ieee8021paeMIB 2 }

dot1xPaeGroups OBJECT IDENTIFIER ::= { dot1xPaeConformance 1 }

dot1xPaeCompliances OBJECT IDENTIFIER
    ::= { dot1xPaeConformance 2 }

-- ---------------------------------------------------------- --
-- units of conformance
-- ---------------------------------------------------------- --

dot1xPaeSystemGroup OBJECT-GROUP
    OBJECTS {
        dot1xPaeSystemAuthControl,
        dot1xPaePortProtocolVersion,
        dot1xPaePortCapabilities,
        dot1xPaePortInitialize
    }
    STATUS      current
    DESCRIPTION
        "A collection of objects providing system information
        about, and control over, a PAE."
    ::= { dot1xPaeGroups 1 }

dot1xPaeAuthConfigGroup OBJECT-GROUP
    OBJECTS {
        dot1xAuthPaeState,
        dot1xAuthBackendAuthState,
        dot1xAuthAdminControlledDirections,
        dot1xAuthOperControlledDirections,
        dot1xAuthAuthControlledPortStatus,
        dot1xAuthAuthControlledPortControl,
        dot1xAuthQuietPeriod,
        dot1xAuthTxPeriod,
        dot1xAuthSuppTimeout,
        dot1xAuthServerTimeout,
        dot1xAuthMaxReq,
        dot1xAuthReAuthPeriod,
        dot1xAuthReAuthEnabled,
        dot1xAuthKeyTxEnabled
    }
    STATUS      current
    DESCRIPTION
        "A collection of objects providing configuration
        information about an Authenticator PAE."
    ::= { dot1xPaeGroups 2 }

dot1xPaeAuthStatsGroup OBJECT-GROUP
    OBJECTS {
        dot1xAuthEapolFramesRx,
        dot1xAuthEapolFramesTx,
        dot1xAuthEapolStartFramesRx,
        dot1xAuthEapolLogoffFramesRx,
        dot1xAuthEapolRespIdFramesRx,
        dot1xAuthEapolRespFramesRx,
        dot1xAuthEapolReqIdFramesTx,
        dot1xAuthEapolReqFramesTx,
        dot1xAuthInvalidEapolFramesRx,
        dot1xAuthEapLengthErrorFramesRx,
        dot1xAuthLastEapolFrameVersion,
        dot1xAuthLastEapolFrameSource
    }
    STATUS      current
    DESCRIPTION
        "A collection of objects providing statistics about an
        Authenticator PAE."
    ::= { dot1xPaeGroups 3 }

dot1xPaeAuthDiagGroup OBJECT-GROUP
    OBJECTS {
        dot1xAuthEntersConnecting,
        dot1xAuthEapLogoffsWhileConnecting,
        dot1xAuthEntersAuthenticating,
        dot1xAuthAuthSuccessWhileAuthenticating,
        dot1xAuthAuthTimeoutsWhileAuthenticating,
        dot1xAuthAuthFailWhileAuthenticating,
        dot1xAuthAuthReauthsWhileAuthenticating,
        dot1xAuthAuthEapStartsWhileAuthenticating,
        dot1xAuthAuthEapLogoffWhileAuthenticating,
        dot1xAuthAuthReauthsWhileAuthenticated,
        dot1xAuthAuthEapStartsWhileAuthenticated,
        dot1xAuthAuthEapLogoffWhileAuthenticated,
        dot1xAuthBackendResponses,
        dot1xAuthBackendAccessChallenges,
        dot1xAuthBackendOtherRequestsToSupplicant,
        dot1xAuthBackendNonNakResponsesFromSupplicant,
        dot1xAuthBackendAuthSuccesses,
        dot1xAuthBackendAuthFails
    }
    STATUS      current
    DESCRIPTION
        "A collection of objects providing diagnostic statistics
        about an Authenticator PAE."
    ::= { dot1xPaeGroups 4 }

dot1xPaeAuthSessionStatsGroup OBJECT-GROUP
    OBJECTS {
        dot1xAuthSessionOctetsRx,
        dot1xAuthSessionOctetsTx,
        dot1xAuthSessionFramesRx,
        dot1xAuthSessionFramesTx,
        dot1xAuthSessionId,
        dot1xAuthSessionAuthenticMethod,
        dot1xAuthSessionTime,
        dot1xAuthSessionTerminateCause
    }
    STATUS      current
    DESCRIPTION
        "A collection of objects providing statistics about the
        current, or last session for an Authenticator PAE."
    ::= { dot1xPaeGroups 5 }

dot1xPaeSuppConfigGroup OBJECT-GROUP
    OBJECTS {
        dot1xSuppPaeState,
        dot1xSuppHeldPeriod,
        dot1xSuppAuthPeriod,
        dot1xSuppStartPeriod,
        dot1xSuppMaxStart
    }
    STATUS      current
    DESCRIPTION
        "A collection of objects providing configuration
        information about a Supplicant PAE."
    ::= { dot1xPaeGroups 6 }

dot1xPaeSuppStatsGroup OBJECT-GROUP
    OBJECTS {
        dot1xSuppEapolFramesRx,
        dot1xSuppEapolFramesTx,
        dot1xSuppEapolStartFramesTx,
        dot1xSuppEapolLogoffFramesTx,
        dot1xSuppEapolRespIdFramesTx,
        dot1xSuppEapolRespFramesTx,
        dot1xSuppEapolReqIdFramesRx,
        dot1xSuppEapolReqFramesRx,
        dot1xSuppInvalidEapolFramesRx,
        dot1xSuppEapLengthErrorFramesRx,
        dot1xSuppLastEapolFrameVersion,
        dot1xSuppLastEapolFrameSource
    }
    STATUS      current
    DESCRIPTION
        "A collection of objects providing statistics about a
        Supplicant PAE."
    ::= { dot1xPaeGroups 7 }

-- ---------------------------------------------------------- --
-- compliance statements
-- ---------------------------------------------------------- --

dot1xPaeCompliance MODULE-COMPLIANCE
    STATUS  current
    DESCRIPTION
        "The compliance statement for device support of
        Port Access Control."

    MODULE
        MANDATORY-GROUPS {
            dot1xPaeSystemGroup
        }

        GROUP   dot1xPaeAuthConfigGroup
        DESCRIPTION
            "This group is mandatory for systems that support
            the Authenticator functions of the PAE."

        OBJECT  dot1xAuthAdminControlledDirections
        SYNTAX  INTEGER {
                    both(0)
                }
        MIN-ACCESS read-only
        DESCRIPTION
            "Support for in(1) is optional."

        OBJECT  dot1xAuthOperControlledDirections
        SYNTAX  INTEGER {
                    both(0)
                }
        DESCRIPTION
            "Support for in(1) is optional."

        OBJECT dot1xAuthKeyTxEnabled
        MIN-ACCESS read-only
        DESCRIPTION
          "An Authenticator PAE that does not support
          EAPOL-Key frames may implement this object as
          read-only, returning a value of FALSE."

        GROUP   dot1xPaeAuthStatsGroup
        DESCRIPTION
            "This group is mandatory for systems that support
            the Authenticator functions of the PAE."

        GROUP   dot1xPaeAuthDiagGroup
        DESCRIPTION
            "This group is optional for systems that support
            the Authenticator functions of the PAE."

        GROUP   dot1xPaeAuthSessionStatsGroup
        DESCRIPTION
            "This group is optional for systems that support
            the Authenticator functions of the PAE."

        GROUP   dot1xPaeSuppConfigGroup
        DESCRIPTION
            "This group is mandatory for systems that support
            the Supplicant functions of the PAE."

        GROUP   dot1xPaeSuppStatsGroup
        DESCRIPTION
            "This group is mandatory for systems that support
            the Supplicant functions of the PAE."

    ::= { dot1xPaeCompliances 1 }

END

