md5 checksums for Maui files.
e25a713be0d2940e4c07bceb44f8afb0  01MB240_470_013
d59d19e18bae685fa860ab659972f7f8  01MB240_470_013.sh
8a6b36cde71d6b9a79815823ecbf616b  drv470_013_MauiBringup8MB.img

chksum for Maui files
 8 bit checksum 27DEFA41 01MB240_470_013
16 bit checksum 35EBA567 01MB240_470_013
 8 bit checksum 6879FCD5 01MB240_470_013.sh
16 bit checksum 6F1219E5 01MB240_470_013.sh
 8 bit checksum 54CC8304 drv470_013_MauiBringup8MB.img
16 bit checksum 8E894026 drv470_013_MauiBringup8MB.img

Important Notes:------------------------------------------------------
- Only a combined firmware image containing both host FW and the BMC FW in now provided.
- DO NOT PERFORM A update_flash -c IF YOUR BLADE IS IN A LANGDON.  This is not supported.
- 01MB240_470_013 is used for inband updates from the OS.  The .img files are for flash burners.
The drv470_013 driver includes the following:
------------------------------------
Level fixlevel Release v2r40lf.phyp
Name         Austin Defect  Username                  Abstract
-----------  -------------  ------------------------  ----------------------------------------------------------------
P9B22703     541954         Mark Manges               LIC - model JS21 manufacturing default configuration not establ
P9B23620     544139         Van Lee                   JS21: Root cause and fix for the original BMC flash update prob
P9B23738     n/a            Van Lee                   JS21: BCM initialization per recent errata (split completion, e
P9B23796     n/a            Van Lee                   JS21: Maui Core FIR SCOM settings
P9B24033     n/a            Van Lee                   JS21: Implement Reset procedure for AMD8111 USB2.0 controller p
P9B24073     n/a            Van Lee                   JS21: Need to create a minimum VPD for the sp-PACA structure fo
P9B24095     n/a            Daniel R Harms            PHYPL: Delivering PF060330
P9B24790     n/a            Daniel R Harms            PHYPL: Delivering PF060410


- drv470_013 Latest PFW - Built on 04/10/2006 which contains the following:
Level PF060330 Release pfw_js21_1
Name    Username   Abstract
------	--------   -------------------------------------------------
535373 vsinghal    San Jacinto shows up with wrong physical location                   
537465 bharring    GA8: Buffers to PHYP cant span page                                 
541136 changh      system hangs upon first memory DLPAR add                            
541756 changh      network boot SLES10 Beta1, initrd memory corrupted                  
542739 smayes      BAT firmware is failing ibm,get-config-addr-info                    
543762 changh      SQFIELD - ATTN light, SRCBA210000 on AIX partition                  
543816 changh      BUP: GA8 PFW - DEFAULT CATCH on IPL                                 


Level PF060405 Release pfw_js21_1
Name    Username   Abstract
------	--------   -------------------------------------------------
542573  vsinghal   PFW:Confirm no VLAN because default network alias 
544672  changh     Improve VSCSI/VLAN performance in OF              


Level PF060407 Release pfw_js21_1
Name    Username   Abstract
------	--------   -------------------------------------------------
536491  changh     HV2++:  IPLtest fails at CA00E891                              
545743  causten    HOT: 0613C_53H CD install encounters UNKNOWN BOOTDEV on hina03 


Level PF060410 Release pfw_js21_1
Name    Username   Abstract
------	--------   -------------------------------------------------
546577  lindeman   PFW-Maui: Limit MMRBC to 512b and max-outstanding to 1 


Zip file contents:
-------------------------------------------------------------
01MB240_470_013    (22 MB)   Use only if drv393 with inband support is already flashed on your system.

The PHYP Lite 470_013 driver is the released 470_013 v2r40lf.phyp driver located at
/converge/v2r40lf.phyp/bld/gen/fixes/24l47_014/disruptive/
and is only meant for bringup Maui/Hanas.
