*********************************************

LSI Logic MegaRAID Sles 10 Driver Release 

*********************************************

Release Date: 02/15/2007
===================

Supported Controllers
==================

MegaRAID SAS 84016E
MegaRAID SAS 8704ELP
MegaRAID SAS 8708ELP
MegaRAID SAS 8888ELP
MegaRAID SAS 8408E
MegaRAID SAS 8480E
MegaRAID SAS 8308ELP
MegaRAID SAS 8344ELP
MegaRAID SAS 8304ELP
MegaRAID SAS 8300XLP


Component:
=========
SAS MegaRAID Driver Sles 10 all
Release Date: 02/15/2007


Version Numbers:	DUDs		RPM
===============		=====		====	
Current Version		03.07		03.07
Pervious Version	Not Applicable


Bug Fixes and Enhancements
==========================
LSID100063512 (CO)   Need driver to return same geometry information 
LSID100058872 (CO)   Add RHEL 3 U7, U8, and RHEL 4 U4 on Linux SAS 
LSID100058440 (DFCT) Driver can't flash to Cache of BBU. 
LSID100056648 (DFCT) IOs running on 1068 RAID with 1078 RAID present causes IO programs became sluggish and stop responding. 
LSID100058146 (DFCT) Linux RPM driver has failed on SLES 10 gold. 
LSID100057482 (DFCT) SLES 10 freezes after RAID FW re-engaged through debugger 
LSID100055601 (DFCT) DKMS update has failed on AMD system but works on Intel system. 


Known Restrictions: 
===================

1.	NONE


Known Bugs: 
===========

1.	NONE


Installation Notes: 
===============
DUDs:
megaraid_sas-v00.00.03.07-1-sles10-ga-all.img
	SLES10 GA i686
	SLES10 GA x86_64

DKMS RPM:
---------
megaraid_sas-v00.00.03.07-1.noarch.rpm
	All of the above
