CMOSMap 2.0.1, BC, 26, 26, BIOS, 10h, a3h, Port72

CompressedSetupDataSegment 9b64h
MainMenu 43b3h
CMOSName CMOS_DisketteA, change, 010h, 004h, 004h, 004h
CMOSName CMOS_DisketteB, change, 010h, 000h, 004h, 000h
CMOSName CMOS_BMCPwrExec, reboot, 01bh, 000h, 001h, 000h
CMOSName CMOS_CRTRequired, reboot, 01bh, 001h, 001h, 000h
CMOSName CMOS_KbdRequired, reboot, 01bh, 002h, 001h, 000h
CMOSName CMOS_UsbLegacy, reboot, 01bh, 003h, 001h, 000h
CMOSName CMOS_AlternateBootDevice4, reboot, 01dh, 000h, 004h, 008h
CMOSName CMOS_AlternateBootDevice3, reboot, 01dh, 004h, 004h, 00ch
CMOSName CMOS_AlternateBootDevice2, reboot, 01eh, 000h, 004h, 000h
CMOSName CMOS_AlternateBootDevice1, reboot, 01eh, 004h, 004h, 006h
CMOSName CMOS_NumLock, reboot, 02bh, 000h, 001h, 001h
CMOSName CMOS_PS2Mouse, change, 02bh, 001h, 001h, 001h
CMOSName CMOS_UserPwdChange, reboot, 02bh, 002h, 001h, 000h
CMOSName CMOS_ServerMode, reboot, 02bh, 004h, 001h, 000h
CMOSName CMOS_FloppyRequired, reboot, 02bh, 006h, 001h, 000h
CMOSName CMOS_PostBootFailRequired, reboot, 02bh, 007h, 001h, 000h
CMOSName CMOS_iSCSIEnabled, reboot, 035h, 002h, 001h, 000h
CMOSName CMOS_ENET2_PLANAR_ENABLE, critical, 039h, 001h, 001h, 000h
CMOSName CMOS_ENET1_PLANAR_ENABLE, critical, 039h, 000h, 001h, 000h
CMOSName CMOS_DCSlot1_ENABLE, reboot, 039h, 002h, 001h, 000h
CMOSName CMOS_ExpressA0, reboot, 039h, 007h, 001h, 000h
CMOSName CMOS_ExpressA1, reboot, 03ch, 004h, 001h, 000h
CMOSName CMOS_ExpressB0, reboot, 03ch, 005h, 001h, 000h
CMOSName CMOS_MemoryConfig, change, 03ch, 006h, 002h, 000h
CMOSName CMOS_MemoryRow0Disable, change, 049h, 000h, 004h, 000h
CMOSName CMOS_MemoryRow1Disable, change, 049h, 004h, 004h, 000h
CMOSName CMOS_MemoryRow2Disable, change, 04ah, 000h, 004h, 000h
CMOSName CMOS_MemoryRow3Disable, change, 04ah, 004h, 004h, 000h
CMOSName CMOS_MemoryRow4Disable, change, 04bh, 000h, 004h, 000h
CMOSName CMOS_MemoryRow5Disable, change, 04bh, 004h, 004h, 000h
CMOSName CMOS_StopOnError, reboot, 04ch, 000h, 002h, 001h
CMOSName CMOS_MemoryRow6Disable, change, 04ch, 002h, 004h, 000h
CMOSName CMOS_MemoryRow7Disable, change, 04dh, 000h, 004h, 000h
CMOSName CMOS_BMCWatchdog, reboot, 069h, 007h, 001h, 000h
CMOSName CMOS_BMCPOSTWDTimeout, reboot, 06ch, 000h, 008h, 005h
CMOSName CMOS_BMCSerialConfig, reboot, 06dh, 000h, 002h, 002h
CMOSName CMOS_DisketteController, change, 073h, 006h, 001h, 000h
CMOSName CMOS_INT_19H, reboot, 076h, 000h, 001h, 001h
CMOSName CMOS_DisableC1E, reboot, 076h, 003h, 001h, 000h
CMOSName CMOS_VIDEO_PLANAR_ENABLE, nochange, 077h, 001h, 001h, 000h
CMOSName CMOS_DCSlot2_ENABLE, reboot, 077h, 002h, 001h, 000h
CMOSName CMOS_DCSlot3_ENABLE, reboot, 077h, 003h, 001h, 000h
CMOSName CMOS_SerialA, change, 077h, 004h, 003h, 001h
CMOSName CMOS_SerialB, change, 077h, 007h, 003h, 000h
CMOSName CMOS_IDEControllerPrimary, change, 078h, 006h, 001h, 001h
CMOSName CMOS_IDEControllerSecondary, change, 078h, 007h, 001h, 000h
CMOSName CMOS_IDERaid, change, 079h, 000h, 001h, 000h
CMOSName CMOS_OnDemand, reboot, 079h, 002h, 008h, 0ffh
CMOSName CMOS_ForcePR, change, 07ah, 002h, 002h, 000h
CMOSName CMOS_TM2Vid, change, 07ah, 004h, 008h, 000h
CMOSName CMOS_TM2Ratio, change, 07bh, 004h, 008h, 0ffh
CMOSName CMOS_ProcPrfrmStates, reboot, 07fh, 000h, 001h, 000h
CMOSName CMOS_ENET_PXE_ENABLE, reboot, 085h, 005h, 002h, 001h
CMOSName CMOS_PXE_NICSelect_Enable, reboot, 085h, 007h, 001h, 000h
CMOSName CMOS_SP_PXE_ENABLE, reboot, 086h, 001h, 001h, 000h
CMOSName CMOS_PciPIRQAValue, change, 087h, 006h, 004h, 000h
CMOSName CMOS_PciPIRQBValue, change, 088h, 003h, 004h, 000h
CMOSName CMOS_PciPIRQCValue, change, 089h, 000h, 004h, 000h
CMOSName CMOS_PciPIRQDValue, change, 089h, 005h, 004h, 000h
CMOSName CMOS_PciPIRQEValue, change, 08ah, 002h, 004h, 000h
CMOSName CMOS_PciPIRQFValue, change, 08ah, 007h, 004h, 000h
CMOSName CMOS_PciPIRQGValue, change, 08bh, 004h, 004h, 000h
CMOSName CMOS_PciPIRQHValue, change, 08ch, 001h, 004h, 000h
CMOSName CMOS_PCIMLT1, reboot, 08ch, 006h, 008h, 040h
CMOSName CMOS_ReportUserDisabledPCIDevices, reboot, 08dh, 006h, 001h, 000h
CMOSName CMOS_PCIBootPriority, change, 08dh, 007h, 008h, 000h
CMOSName CM_VIRUS_DETECT, change, 08fh, 006h, 001h, 000h
CMOSName CMOS_WakeOnLAN, reboot, 092h, 002h, 001h, 001h
CMOSName CMOS_RemoteConsoleEnable, reboot, 092h, 003h, 001h, 000h
CMOSName CMOS_RemoteConsoleComPort, reboot, 092h, 004h, 003h, 000h
CMOSName CMOS_RemoteConsoleBaud, reboot, 092h, 007h, 003h, 001h
CMOSName CMOS_RemoteConsoleDataBits, reboot, 093h, 002h, 003h, 003h
CMOSName CMOS_RemoteConsoleParity, reboot, 093h, 005h, 003h, 000h
CMOSName CMOS_RemoteConsoleStopBits, reboot, 094h, 000h, 003h, 000h
CMOSName CMOS_RemoteConsoleEmulation, reboot, 094h, 003h, 001h, 000h
CMOSName CMOS_RemoteConsoleKybdEmul, reboot, 094h, 004h, 001h, 000h
CMOSName CMOS_RemoteConsoleBootEnable, reboot, 094h, 005h, 001h, 000h
CMOSName CMOS_RemoteConsoleFlowCtrl, reboot, 094h, 006h, 001h, 000h
CMOSName CMOS_HookedInt8forAdaptec, reboot, 094h, 007h, 001h, 000h
CMOSName CMOS_QuietBoot, reboot, 095h, 000h, 001h, 000h
CMOSName CMOS_UsbDisk, reboot, 0a0h, 000h, 001h, 001h
CMOSName CMOS_UsbBootDiskPersist, reboot, 0a3h, 000h, 008h, 000h
CMOSName CMOS_ROMControlSlot1, reboot, 086h, 004h, 001h, 000h
CMOSName CMOS_ROMControlSlot2, reboot, 086h, 005h, 001h, 000h
CMOSName CMOS_ROMControlSlot3, reboot, 086h, 006h, 001h, 000h
CMOSName CMOS_ROMControlSlot4, reboot, 086h, 007h, 001h, 000h
CMOSName CMOS_ROMControlSlot5, reboot, 087h, 000h, 001h, 000h
CMOSName CMOS_ROMControlSlot6, reboot, 087h, 001h, 001h, 000h
CMOSName CMOS_ROMControlSlot7, reboot, 087h, 002h, 001h, 000h
CMOSName CMOS_ROMControlSlot8, reboot, 087h, 003h, 001h, 000h
CMOSName CMOS_ROMControlSlot9, reboot, 087h, 004h, 001h, 000h
CMOSName CMOS_ROMControlSlot10, reboot, 087h, 005h, 001h, 000h
CMOSChecksum 010h, 02dh, 02fh, 02eh
CMOSChecksum 07fh, 07fh, 03bh, 03ah
BMCSetting BMC_PrimaryBootDevice1, "First Primary Boot Device", critical, 184, 009:208.081.000.055.008.016|007#006, 010:208.081.000.055.008.016.001|003 {
        CMOSChoice "Floppy Drive", 0,
        CMOSChoice "iSCSI", 4,
        CMOSChoice "iSCSI Critical", 5,
        CMOSChoice "Network", 6,
        CMOSChoice "HDD0", 8,
        CMOSChoice "HDD1", 9,
        CMOSChoice "HDD2", 10,
        CMOSChoice "HDD3", 11,
        CMOSChoice "CD-ROM", 12,
        CMOSHelp "Help for First Primary Boot Device" {
                "The system uses a startup sequence to determine which",
                "device will be the startup device. The startup device",
                "is the diskette drive, hard disk, or network adapter",
                "which will be used to load the operating system. This",
                "field specifies the first device for which a system",
                "start will be attempted. If the start from this device",
                "fails, the system will be attempt to start from the",
                "second startup device."
        }
}
BMCSetting BMC_PrimaryBootDevice2, "Second Primary Boot Device", critical, 184, 009:208.081.000.056.008.016|007#006, 010:208.081.000.056.008.016.001|003 {
        CMOSChoice "Floppy Drive", 0,
        CMOSChoice "iSCSI", 4,
        CMOSChoice "iSCSI Critical", 5,
        CMOSChoice "Network", 6,
        CMOSChoice "HDD0", 8,
        CMOSChoice "HDD1", 9,
        CMOSChoice "HDD2", 10,
        CMOSChoice "HDD3", 11,
        CMOSChoice "CD-ROM", 12,
        CMOSHelp "Help for Second Primary Boot Device" {
                "The system uses a startup sequence to determine which",
                "device will be the startup device. The startup device",
                "is the diskette drive, hard disk, or network adapter",
                "which will be used to load the operating system. This",
                "field specifies the second device for which a system",
                "start will be attempted. If the start from this device",
                "fails, the system will be attempt to start from the",
                "third startup device."
        }
}
BMCSetting BMC_PrimaryBootDevice3, "Third Primary Boot Device", critical, 184, 009:208.081.000.057.008.016|007#006, 010:208.081.000.057.008.016.001|003 {
        CMOSChoice "Floppy Drive", 0,
        CMOSChoice "iSCSI", 4,
        CMOSChoice "iSCSI Critical", 5,
        CMOSChoice "Network", 6,
        CMOSChoice "HDD0", 8,
        CMOSChoice "HDD1", 9,
        CMOSChoice "HDD2", 10,
        CMOSChoice "HDD3", 11,
        CMOSChoice "CD-ROM", 12,
        CMOSHelp "Help for Third Primary Boot Device" {
                "The system uses a startup sequence to determine which",
                "device will be the startup device. The startup device",
                "is the diskette drive, hard disk, or network adapter",
                "which will be used to load the operating system. This",
                "field specifies the third device for which a system",
                "start will be attempted. If the start from this device",
                "fails, the system will be attempt to start from the",
                "fourth startup device."
        }
}
BMCSetting BMC_PrimaryBootDevice4, "Fourth Primary Boot Device", critical, 184, 009:208.081.000.058.008.016|007#006, 010:208.081.000.058.008.016.001|003 {
        CMOSChoice "Floppy Drive", 0,
        CMOSChoice "iSCSI", 4,
        CMOSChoice "iSCSI Critical", 5,
        CMOSChoice "Network", 6,
        CMOSChoice "HDD0", 8,
        CMOSChoice "HDD1", 9,
        CMOSChoice "HDD2", 10,
        CMOSChoice "HDD3", 11,
        CMOSChoice "CD-ROM", 12,
        CMOSHelp "Help for Fourth Primary Boot Device" {
                "The system uses a startup sequence to determine which",
                "device will be the startup device. The startup device",
                "is the diskette drive, hard disk, or network adapter",
                "which will be used to load the operating system. This",
                "field specifies the fourth device for which a system",
                "start will be attempted. If the start from this device",
                "fails, the system will halt with an error message."
        }
}

