  CONFIGURATION EDITOR
  BRIDGING

# Control Bridging By Protocol

IP

IPX

Manager via LLC

NetBIOS

Other Frame Types

SNA/LLC2

IP

  If ON, IP frames will be bridged through the unit. To select the method by which these frames are bridged, or to enable IP bridging, click on the IP button.

NetBIOS

  If ON, NetBIOS frames will be bridged through this unit. To select the method by which these frames are bridged, or to enable NetBIOS bridging, click on the NetBIOS button.

Manager via LLC

  Bridging for this protocol is either turned ON or OFF. Click on the Manager via LLC button to toggle the setting.
  If you want LLC2 frames generated by the management program to be bridged through this unit (i.e., you are managing downstream units via LLC2 through this unit), this feature must be set to ON.

IPX

  If ON, IPX frames will be bridged through this unit. To select the method by which these frames are bridged, or to enable IPX bridging, click on the IPX button.

SNA/LLC2

  If ON, SNA/LLC2 frames will be bridged through this unit. To select the method by which these frames are bridged, or to enable SNA/LLC2 bridging, click on the SNA/LLC2 button.

Other Frame Types

  If ON, frame types other than those listed above will be bridged through this unit. To select the method by which these frames are bridged, or to enable bridging of other frame types, click on the Other Frame Types button.