  CONFIGURATION EDITOR
  UNIT LEVEL PARAMETERS
  LAN

# Access Ports

Dial Backup

Frame Relay

Primary / Secondary Bisync RJE

Terminal / Host Async

Terminal / Host Bisync

Terminal / Host ISO Async

Terminal / Host SDLC

X.25

  Click inside an access port drop-down list to define the port type. Valid port types are:

Frame Relay (FRADs only)

  Frame relay ports enable you to connect the unit to a frame relay switch. These WAN ports should be configured on the lowest numbered ports.
  By default, the lowest numbered port is identified as your WAN port. Consecutive frame relay ports are identified by their respective port number. For instance, from an NMS session, you could enter ncl vie wan to view the configuration for port one. If you wanted to view the configuration for port two, however, you must type ncl vie 2.

X.25

  This option provides transparent terminal-to-IBM-Host connectivity across X.25 packet-switched networks.

Dial Backup (FRADs only)

  A dial backup port adds system reliability to any frame relay networking environment involving other frame relay devices.

Terminal / Host SDLC

  Terminal or Host connectivity is available for SDLC devices.

Terminal / Host Bisync

  Terminal or Host connectivity is available for Bisync devices.

Terminal / Host Async

  Terminal or Host connectivity is available for Async devices.

Terminal / Host ISO Async

  Terminal or Host connectivity is available for ISO Async devices.

Primary / Secondary Bisync RJE

  Primary or Secondary connectivity is available for Bisync RJE devices.

LAN

  The LAN port, if required, can be configured for Token Ring or Ethernet. If the unit does not use its LAN port, this field can be set to none.