# Unit Detail

# Unit Monitoring

# Displaying Short Term Statistics (Current)

#### Displaying Short Term Statistics

#### Done

#### Stop/Start Update

#### Displaying Short Term Statistics (Current)

  The FRAP and T-FRAP monitor and collect Short Term statistics on Frame Relay traffic passing across each DLCI. Packet traffic is monitored and statistical counts taken for Layer 2 throughput, Layer 3 application protocol-based, socket-level IP protocols,and other protocols defined by supported filters. Current Short Term statistics reflect the receive and transmit counts being collected during the current interval. To display the absolute running totals of all DLCIs, refer to Displaying Short Term Statistics
  To display the Short Term statistics (in tabular form) on an individual DLCI:
  1 Make sure that the unit Detail window's DLCIs tab has been clicked.
  2 Position the mouse arrow over the DLCI entry, listed in the Unit Detail window's DLCIs tab, whose Short Term current statistics you wish to view, and click the right
  mouse button.
  3 Select Short Term Statistics from the list of pull-down menu options.
  4 Select, from the list of pull-down menu options, the category of Short Term DLCI statistics you wish to view, and click the left mouse button.
  Note: The window values displayed in parentheses represents the difference (delta) between values obtained during the previous polling interval and the current interval.
  The buttons located at the bottom of each Short Term DLCI statistics window are described in the following paragraphs.
  Stop/Start - Clicking this button stops and starts the statistics polling action.
  Update - Clicking this button will update (refresh) the information contained in the Short Term DLCI statistics window.
  Done - Clicking this button will close the Short Term DLCI statistics window.