  CONFIGURATION EDITOR
  MAPPINGS

# Auto LLC Mappings

Alternate Destination Name

Alternate DLCI

Broadcast Test Frames on All DLCIs

Destination Name

Enable Auto LLC

Frame Relay Transmission Priority

Parallel DLCI

Place Call on Frame Relay Port

Primary DLCI

  Two basic topologies are supported by this feature:
  1. Ethernet LAN originated call, through frame relay, to a LAN-attached FEP
  The branch Ethernet unit is configured to establish dynamic PU sessions to an SNA Host through a Host-attached Token Ring.
  2. Ethernet LAN originated call to a frame relay-attached FEP
  The branch Ethernet unit is configured to establish dynamic session with an SNA Host through a frame relay BAN or BNN connection.

Enable Auto LLC

  Select this option if you intend to use the Auto LLC feature.
  Range: Enabled or Disabled

Broadcast Test Frames on All DLCIs

  Enable this feature if you want the unit to broadcast test frames over all available DLCIs. If you want to use a specific DLCI, then disable this feature.
  Range: Enabled or Disabled

Place Call on Frame Relay Port

  This is the port through which the unit can access the destination host.
  Range: 1 -- 8

Frame Relay Transmission Priority

  This field defines the priority for transmissions over the specified frame relay port.
  Range: Default, Low, Medium, High, or Urgent

Destination Name

  This button enables you to select the destination host from a list of names. If your destination host does not appear in the list, you may add it using the Destination Editor.
  Range: Any host in the destination list

Primary DLCI

  This parameter defines the primary DLCI on which the call will be placed.
  If Broadcast Test Frames on all DLCIs is disabled, you must define this parameter.
  Range: 16 -- 1023

Parallel DLCI

  This optional parameter defines the DLCI that should be used if the primary DLCI becomes inactive.
  Range: 16 -- 1023

Alternate Destination Name

  This button enables you to select the alternate destination host that should be contacted if the primary destination host becomes unreachable. If your destination host does not appear in the list, you may add it using the Destination Editor.
  Range: Any host in the destination list

Alternate DLCI

  This parameter defines the DLCI that should be used if the primary and parallel DLCIs become inactive.
  Range: 16 -- 1023