  CONFIGURATION EDITOR

# ISDN Configuration

Back in Service Time Out

Called Party Number

Connect Retry Delay

Connection Timeout

IBM LID

Local Service Profile ID

Number of Attempts

Number Plan ID

Out of Service Time Out

Service Type

Type of Number

  Some of the following parameters are only available for Frame Relay connections.

Local Service Profile ID

  This field enables you to enter the SPID, a zero-terminated ASCII string.
  Range: Up to 20 characters

Service Type

  Click on this field to select the appropriate service type.
  Range: Any service available from the list

Called Party Number

  Enter the number of the party that is answering the call.
  Note: This number must match what the central office has configured for the answering side.
  Range: Up to 20 characters

Type of Number

  Enter the type of number that is used by the answering side.
  Range: 0 -- 9

Number Plan ID

  Enter the number plan ID that is configured for the answering side.
  Range: 0 -- 9

Connection Parameters

  Select whether the unit is going to Answer or Originate the call.
  Range: Answer or Originate

IBM LID

  This feature enables you to configure the connection for the IBM LID protocol.

Connection Timeout

  This value defines the amount of time the unit waits before considering the connection as failed.
  Range: 0 -- 255 seconds

Number of Attempts

  This value defines the number of redials the unit attempts before considering the connection as failed.
  Range: 0 -- 255 attempts

Connect Retry Delay

  This value defines the the amount of time the unit waits before trying the call again after a failure.
  Range: 0 -- 255 seconds

Out of Service Time Out

  This value defines the timeout value for the Out of Service condition.
  Range: 0 -- 99 seconds

Back in Service Time Out

  This value defines the timeout value for the Back in Service condition.
  Range: 0 -- 99 seconds