#

# CONFIGURATION EDITOR

# IP ROUTING

# IP QOS

Destination IP Address

Destination IP Mask

Priority QOS

Protocol

Source IP Address

Source IP Mask

Source Port

  Click on the Insert button to ass an entry above the cursor's current position.

Protocol

  This field defines the source and destination port to be a TCP or UDP port. If this field does not apply, select N/A for Not Applicable.
  Range: N/A, TCP, or UDP

Source IP Address

  This field defines the source IP Address. If left blank, this parameter is ignored in the comparison process.
  Range: Four numbers (0-255) separated by a period.

Source IP Mask

  This field defines the network mask for the source. The value may depict an actual source host address, network address, subnet address, or all source addresses.
  Range: Four numbers (0-255) separated by a period.

Source Port

  This field defines the source TCP/UDP port number.
  Range: Any valid port number.

Destination IP Address

  This field defines the destination IP Address. If left blank, this parameter is ignored in the comparison process.
  Range: Four numbers (0-255) separated by a period.

Destination IP Mask

  This field defines the network mask for the destination. The value may depict an actual destination host address, network address, subnet address, or all destination addresses.
  Range: Four numbers (0-255) separated by a period.

Priority QOS

  This pull-down list enables you to select High, Medium, Low, or Urgent priority for the given specifications.
  Range: U, H, M, L