#

# EDITOR HOME

# NETWORK PORT

# S-FRAP Network Port

#### Application Type

#### Circuit Identifier

#### Cut-Thru Timeout

#### Operation Mode

#### Tx Timing

#### Application Type

  Identifies the type of carrier line service provided on the attached network line.
  Range: Frame Relay (HDLC) or Dedicated (CBO)

#### Cut-Thru Timeout (min)

  Defines the timer value used to automatically terminate the cut-through state and restore the unit to the configured operating mode. This timer has no effect if the switch on the unit's front panel, is set to the Off position (cut-through state)
  Range: 0 ~ 1440 seconds

#### Circuit Identifier

  Defines the network circuit identifier of the carrier service provider.
  Range: 0 ~ 30 alpha-numeric characters

#### Tx Timing

  Defines the serial transmit timing mode.
  Range: Loop-1 ~ The clock returned from the DTE (TT/TCE) is used to sample transmit data. Loop-2 ~ The clock supplied by the DCE device (ST/TC) is used to sample transmit data.

#### Operation Mode

  Defines the unit's mode of operation.
  Range: Tap ~ Enables the unit to passively monitor network data traffic between the DTE and DCE devices for statistical collection and quality of Service (QOS) purposes. While in this mode, the unit cannot alter or inject data directly into the network, and can only be managed via its Maintenance serial interface port. In band ~ Represents normal operating mode. All Frame Relay traffic passes through monitoring and probe circuits, gathers in local memory, then is forwarded to its destination.