# Unit Detail

# Unit Monitoring

# Displaying Network Status Information

#### Done

#### Mode

#### Port

#### Signal Status

#### Statistics

#### Status Information

#### Update

#### Displaying Network Status Information

  The Network Port Status window provides the user with the activity status of the Network port as well as the status of the various controls signals which pass through this interface.
  To open the Network Port Status window:
  1 Position the mouse arrow over the Unit Detail window's graphical representation of the Network port, and click the right mouse button. This action will cause a pull-down menu, similar to the following, to be displayed.
  2 Select Status Information... from the list of pull-down menu options and click the left mouse button.
  Note: The Network Port Status window can also be opened by double clicking the graphical representation of the Network port displayed in the Unit Detail window.
  This action will cause a Network Port Status window similar to the following to be displayed. The fields and buttons contained within the Network Port Status window are described in the following paragraphs.
  Port - Identifies the interface port (NET).
  Mode - Identifies the current status of the interface port (e.g., No connection, Active, or Test).
  Status Information - A textual description of the Network port's current status (e.g., TI Frame Sync Okay, Sync Okay, Port is in test mode).
  Signal Status - These values will always display as N/A (not applicable) because these signals are not found on the network interface.
  Update - Clicking this button will update (refresh) the status of Network control signals.
  Statistics... - Clicking this button will open the Network Port Statistics window. For additional information about the window, refer to "Displaying Network Port Statistics.
  Done - Clicking this button will close the Network Port Status window.