  CONFIGURATION EDITOR
  IPX ROUTING

# Transmit / Receive RIP For IPX Routing

  Click on the Add button to add an override.

Port

  Click inside this field to select another port from the list.
  Range: 1 -- 8

DLCI

  Click inside this field to specify a DLCI for the frame relay port. If a LAN port is defined, this field is ignored.
  Range: 16 -- 1023

Transmit/Receive RIP

  Click inside this field to select the appropriate override for the specified interface.
  Range: Yes or No