  CONFIGURATION EDITOR
  BRIDGING
  BRIDGING CONTROL BY PROTOCOL

# Bridging Control By Protocol Other Frame Types

Bridging Method

  This field enables you to specify which method to use for the protocol.
  Range: None, Transparent/Source Route, or Forward Unconditionally to Virtual Port

Forward Unconditionally to Virtual Port Below

  If this option is selected, you can specify the port and DLCI over which this traffic will flow.
  Range: Ports: 1 --8, DLCIs: 17 --1023