  CONFIGURATION EDITOR
  IPX ROUTING

# Network Numbers For IPX Routing

DLCI

IPX WAN Enable

Network Number

Port

Port

  This field identifies the configured LAN and frame relay ports.
  Range: LAN, or ports 1 -- 8

DLCI

  When configuring a frame relay port's network number, you must specify the appropriate DLCI number. When coupled with a network assignment of 00000000 (unnumbered RIP), this DLCI number creates a virtual port over which IPX traffic travels.
  If you have more than one DLCI assigned to a frame relay port, click on the Add button to include it in the routing table.
  Range: 16 -- 1023

Network Number

  This field defines the network number that corresponds with the destination. Assign this number based on the port type:
  LAN ports must have a network number that matches the Novell server residing the same LAN. If the LAN has no server attached, you must create a network number that is unique throughout the network.
  Frame relay ports must include a provider-assigned DLCI and a network number of 00000000 (unnumbered RIP).
  Range: 8 hexadecimal numbers

IPX WAN Enable

  This field enables you to specify whether or not IPX WAN negotiation will occur on this virtual port.
  Range: Enable or Disable