  Customize

# Customizing Miscellaneous

Bootp Server Enabled

Log Alarms to File

Setting Up The Bootp Feature

Use Alternate Adapter

Use NAU Names

  These parameters enable you to activate or deactivate global program features.

Log Alarms to File

  Enable this feature if you want alarms and traps logged to a file. A new file is created for each day of the week under the AlarmLog sub directory.These alarm logs are not related to the ones accumulated in the alarm buffer for on-line viewing.
  Range: Enabled or Disabled

Use NAU Names

  Enable this feature if you want the NMS pop-up menu to use NAU names. This feature also causes PU NAU names to appear in the Unit Detail window under the PU tab.
  Range: Enabled or Disabled

Use Alternate Adapter

  Enable this feature if you want the management program to use the alternate LAN adapter installed in the workstation.
  Range: Enabled or Disabled

Bootp Server Enabled

  Enable this feature if you want the management workstation to act as a Bootp server. This enables you to configure factory-fresh units via IP routing without having to configure an IP address on the unit via a direct connection.
  Range: Enabled or Disabled

Setting up the Bootp Feature