  CONFIGURATION EDITOR

# Mappings

  This screen enables you to configure mappings for the unit, and displays the number of mappings that are currently configured.

Auto LLC

  This feature enables the unit to automatically configure and use terminated sessions.

LAN PUs

  If Down Stream PUs (DSPUs) communicate through the LAN or WAN, you must map them as logical PUs.

X.25 Pass-Through

  This feature enables the unit to support X.25 PADs over frame relay.

QLLC Conversion

  This feature enables you to define X.25 devices on the LAN or WAN.