# CONFIGURATION EDITOR

# IP ROUTING

# RIP V2 Summary

Starting IP Address

  This field defines the starting IP Address to include in the summarization packet.
  Range: Four numbers (0-255) seperated by a period.

Ending IP Address

  This field defines the ending IP Address to include in the summarization packet.
  Range: Four numbers (0-255) seperated by a period.

Network Mask

  This field defines the network mask to use for the summarization packet.
  Range: Four numbers (0-255) seperated by a period.