# Network Requirements

LAN Adapter Requirements

  Your workstation requires a LAN adapter for either an Ethernet or Token Ring network connection.
  Although you may use other compatible adapter cards, the following cards are recommended:
  ~ 3Com EtherLink III 3C509 and 3C509-Tp adapters
  ~ SMC Elite 16 series Ethernet adapters
  ~ IBM Token Ring adapters

LLC2

  LLC2 management is not supported. Connect by (LLC2) address, however, is supported under Windows 95 only. For more information, please see LLC support.

IP/SNMP

  This management program comes with WinSNMP files that enable the program to run with many other vendors' IP stacks. The installation script copies the WinSNMP files to the SYNCMAN executable (BIN) directory.
  If your PC's memory contains another WinSNMP.DLL, the program cannot load its WinSNMP files.
  You must configure a default gateway address on the management workstation. The default gateway is the LAN IP address assigned to the router through which the program manages other units.