  CONFIGURATION EDITOR

# LAN IPX Frame Format

  The LAN IPX frame format must match the one configured on the Novell server and clients connected to the same LAN as the unit you are configuring.
  The Novell network interface accepts a link driver FRAME command that identifies the frame format. The following table identifies the frame format parameter used to configure the unit, along with the corresponding Novell identifier used in the NET.CFG file.

LAN Type | FRAD | Novell
Ethernet | IEEE 802.2 (LLC) | Ethernet_802.2
Ethernet | Version 2 (DIX) | Ethernet_II
Ethernet | 802.3 Raw Format | Ethernet_802.3
Ethernet | SNAP Encapsulation | Ethernet_SNAP
Token Ring | IEEE 802.2 (LLC) | Token-Ring
Token Ring | SNAP Encapsulation | Token-Ring_SNAP

  From the Format for Routing and RIP/SAP dialog, select one of the following options:
  Range: IEEE 802.2 (LLC), SNAP Encapsulation, Version 2 (DIX), or 802.3 Raw Format