  CONFIGURATION EDITOR
  IPX ROUTING

# Static Routes For IPX Routing

DLCI

Forwarding Router Network Number

Forwarding Router Node Address

Network Number

Port

  You may define static routes when the network is not using RIP broadcasts or the router at the other end is using a routing protocol other than RIP. You may specify these values for selected PVCs or the LAN port.
  To add an entry, click on the Add button.
  To delete an entry, select the entry you want to delete, then click on the Delete button.

Port

  This field identifies the port through which IPX traffic is forwarded. This port must be a LAN or frame relay port.
  Range: 1 -- 8, or LAN

DLCI

  The DLCI number must match the one assigned by your frame relay provider. If you are connecting two FRADs back-to-back, use DLCI number 32 for both ends.
  Range: 16 -- 1023

Network Number

  This number must reflect the network number assigned to the specified port and/or DLCI. All frame relay ports use network number 00000000 (unnumbered RIP).
  Range: 8 hexadecimal numbers

Forwarding Router Network Number

  This field defines the network number assigned to the forwarding router. All frame relay ports use network number 00000000 (unnumbered RIP).
  Range: 8 hexadecimal numbers

Forwarding Router Node Address

  This field defines the MAC address of the forwarding router.
  Range: 12 hexadecimal numbers