#

# EDITOR HOME

# DTE PORT

# S-FRAP 3.0 DTE/DCE Ports

#### Port

  This field displays configured ports and cannot be changed

#### Interface Type

  Defines the type of interface used.
  Range: EIA-530, RS-449, V.35, or X.21

#### Rx Clock Mode

  To-DCE Rx Clock Mode setting is ignored by the software

#### Tx Clock Mode

  To-DTE Tx Clock Mode setting is ignored by the software

#### To-DCE Reporting of RTS

  To-DCE Reporting of RTS Mode setting is ignored by the software

#### Reporting of RTS or Control Lead

  RTS is initiated by the software if the Interface Type is V.35 because the signal is reported as "RTS" on the To-DTE port.
  Control Lead is initiated by the software if the Interface Type is V.21 because the signal is reported as "Control Lead" on the To-DTE port.
  Menu choices are available to the user to determine whether this option should be monitored or ignored.
  Range: Monitored or Ignored