  CONFIGURATION EDITOR

# NetView PUs

Connect Type

Destination

Dial Backup

Enable

Map to Parallel Port

Map to Primary Port

Parallel DLCI

Primary DLCI

XID

  Up to two NetView PUs may be defined.

Enable

  Check this option if you want to enable the primary or alternate PU.
  Range: Enabled or Disabled

XID

  Enter the XID of the NetView PU.
  Range: 8 hexadecimal characters

Destination

  Select the NetView PU's destination from the list of names. If the destination does not appear in the list, you may add it through the Destination Editor.
  Range: Any name in the list.

Map to Primary Port

  Select the primary port through which the unit communicates with the NetView host.
  Range: 1 -- 8 or LAN

Primary DLCI

  If the NetView PU communicates with the host device through the WAN, and is using a specific DLCI, enter the number in this field.
  Range: 16 -- 1023

Map to Parallel Port

  If applicable, select the secondary port through which the unit communicates with the NetView host.
  Range: 1 -- 8 or LAN

Parallel DLCI

  If the NetView PU communicates with the host device through the WAN, and is using a secondary DLCI, enter the number in this field.
  Range: 16 -- 1023

Connect Type

  Set the connection type to originate or answer.
  Range: Answer

Dial Backup

  Click on this button to define the dial backup specifics for the NetView PU.