  CONFIGURATION EDITOR\
  IPX ROUTING

# RIP/SAP Timers For IPX Routing

Port

RIP Aging Timer

RIP Update Timer

SAP Aging Timer

SAP Update Timer

  The default values in this table reflect the standard RIP and SAP timer values defined by the IPX routing specifications. Do not change these values without considering the impact it may have on your network.

Port

  This field identifies the LAN and frame relay ports configured on the unit.
  Range: LAN or ports 1 -- 8

RIP Update Timer

  This parameter defines the frequency at which the unit sends RIP packets over the specified port.
  Range: 0 -- 180 seconds

RIP Aging Timer

  This parameter defines the frequency at which the unit removes learned RIP entries from its table if a corresponding RIP update or broadcast is not received within the defined time limit.
  Range: 40 -- 540 seconds

SAP Update Timer

  This parameter defines the frequency at which the unit sends SAP packets over the specified port.
  Range: 0 -- 180 seconds

SAP Aging Timer

  This parameter defines the frequency at which the unit removes learned SAP entries if a corresponding SAP update or broadcast is not received within the defined time limit.
  Range: 40 -- 720 seconds