  CONFIGURATION EDITOR
  BRIDGING
  BRIDGING CONTROL BY PROTOCOL

# Bridging Control By Protocol IPX

  If IPX packets are bridged, RIP and SAP packets may not be necessary.

Bridging Method

  This field enables you to specify which method to use for the protocol.
  Range: None, Transparent/Source Route, or Forward Unconditionally to Virtual Port, WAN1 or WAN2

Forward Unconditionally to Virtual Port Below

  If this option is selected, you can specify the port and DLCI over which this traffic will flow.
  Range: Ports: 1 --8, DLCIs: 17 --1023, WAN1 or WAN2

RIP/SAP Transmission Control

  You can fine tune RIP and SAP transmissions to prevent the network from becoming too congested with unnecessary RIPs and SAPs.