# InSight

  This software is an optional application that enables you to monitor FRAP and T-FRAP traffic statistics via a graphical interface.
  Polling begins when this application is launched. Polling continues at the user-defined intervals. The delta values, on which the statistics are built, will not be accurate until the completion of the second poll cycle. When the application is closed, polling will cease. Polling will be interrupted if contact with the unit is lost. Once contact with the unit resumes, polling will continue.
  Note: This application does not guarantee polling interval consistency. For an interval of ten seconds, data collected from one poll interval may represent eight seconds worth of collected traffic data while the next poll may represent twelve seconds. This application initiates each poll on the interval, however, it will not normalize or smooth the delta values to compensate for uneven poll intervals. To ease inconsistencies, InSight collects the SysTime value during each poll cycle, then uses the SysTime delta value to calculate the ‘xxx per second’ values.
  Three polling intervals occur for the following statistics:
  • VNIP Delay
  • Protocol Delay
  • Other
  VNIP Delay statistics are collected at a relatively low frequency to ensure that the VNIP delay poll is a fraction of the unit’s VNIP transmission frequency. This frequency is obtained from the configured MIB variable on the unit.
  Protocol Delay polls and Other statistic polls are performed at user-defined intervals defined in the INI file.
  For more information, please see:

### Congestion

### InSight Features

### Launching InSight

### Long-Term Statistics

### Polling Information

### Protocol Detail

### Protocols

### Service Quality

### Utilization

###