#

# EDITOR HELP

# NETWORK PORT

# T-FRAP 3.0 Network Port

#### Circuit Identifier

#### Clock Source

#### Density

#### Framing

#### Interface

#### Line Build out

#### Line Coding

#### Network Mode

#### Performance Buffer

#### Clock Source

  Identifies the source of the network timing clock. The clock source may be obtained from the network line, internal clock crystal, or DTE

#### Network Mode

  Identifies the type of carrier line service provided on the attached network line.
  Range: Frame Relay (HDLC) or Dedicated (CBO)

#### Interface

####

  Range: DSX-1 OR CSU

#### Performance Buffer

  Range: 0 ~ 512.

#### Circuit Identifier

  Defines the network circuit identifier of the carrier service provider.
  Range: 0 ~ 30 alpha-numeric characters

#### Framing

  Range: D4, ESF-54016, or ESF-ANSI

#### Line Coding

  Range: AMI or B8ZS

#### Density

  Range: 1:8, 1:16, or 1:64

####

#### Line Build out

  Range: 0dB, 7.5dB, or 15dB

####