# Customize LLC2

  Broadcast Test Timeout
  Broadcast Type
  LLC Enabled
  Local Test Timeout
  Send Local Test
  Single Route, All Return
  Single Route, Single Return
  T1

  You must define these parameters if you intend to manage units via LLC2.
  LLC Enabled
  Enable this feature if you intend to manage units via LLC2
  Default: Enabled
  Range: Enabled or Disabled
  Send Local Test
  Enable this feature if there are units on the local ring. If disabled, the program will not attempt to locate local units.
  Default: Disabled
  Range: Enabled or Disabled
  Local Test Timeout
  This field defines the number of seconds the management workstation must wait before expecting a response to a local test frame.
  Default: 8 seconds
  Range: 1 -- 20 seconds
  Broadcast Type
  The broadcast type determines how the management workstation finds the best possible route as follows:
  Default: All Routes
  Range: All Routes
  Causes the management workstation to transmit signals to a remote unit over all possible broadcast routes. The remote unit then responds with a non-broadcast (source-routed) frame.
  Single Route, All Return
  Causes the management workstation to transmit signals to a remote unit over a single route. The remote unit then responds with an all-routes broadcast. The route listed in the first response is the route used for the session.
  Single Route, Single Return
  Causes the management workstation to transmit signals to a remote unit over a single route. The remote unit then responds with a non-broadcast (source-routed) frame.
  Broadcast Test Timeout
  This field defines the number of seconds the management workstation must wait before expecting a response from a broadcast test frame.
  Default: 8 seconds
  Range: 1 -- 20 seconds
  T1
  This field helps tune performance by setting the number of seconds the management workstation waits for an LLC2 response before entering a recover-retry sequence.
  Default: 1 second
  Range: 1 -- 10 seconds