  CONFIGURATION EDITOR
  MISCELLANEOUS PARAMETERS

# IP Redirection Without RIP

Enable IP Redirection

Number of Attempts

PING Interval

Response Timer

  If you enable this feature, make certain you configure RIP broadcasts to transmit only in the IP Routing dialog.
  The primary default gateway should be defined on the port through which the primary router is reached.
  The secondary default gateway should be defined on the port through which the secondary router is reached.
  For instance, if the primary default router is reached through the FRAD's LAN port, you need to define the router's LAN IP address in the FRAD's LAN port Default Gateway dialog, as Primary.
  If the secondary default router is reached through the FRAD's WAN port, you need to define the router's WAN IP address in the FRAD's WAN port Default Gateway dialog, as Secondary.
  You cannot have more than one primary or secondary default gateway defined.

Enable IP Redirection

  Enable this feature if you want the FRAD to use the defined secondary default gateway if the primary default gateway fails to respond to a PING. This feature will only work if you have the FRAD configured to only transmit RIP packets.

Response Timer

  This is the amount of time the unit waits for a response to a PING. If a PING response is not received before this time expires, a failed PING response is declared.
  Range: 1 -- 9999 milliseconds

Number of Attempts

  This is the number of consecutive failed PING responses that must occur before the primary router is declared down. Once the primary router is declared down, the secondary router is initiated.
  Range: 1 -- 99

PING Interval

  This is the amount of time between consecutive PING packets sent to the primary router.
  Range: 1 -- 3600 seconds