  CONFIGURATION EDITOR
  MISCELLANEOUS PARAMETERS

# ARP Format Over Frame Relay

Port

  This field reflects the configured frame relay ports.

ARP Format

  If you chose Auto, the unit sends Inverse ARP and Routed ARP for a routed environment, and all three bridged ARP formats for a bridged environment.
  In a normal routed environment, only Routed ARP should be sent.
  In a normal bridged environment, only the appropriate bridged format should be sent.
  Inverse ARP is always sent when a DLCI is activated in both routed and bridged environments.
  Range: Auto, Inverse, Routed, 802.5 Token Ring bridged, Version-2 Ethernet II bridged, 802.3 bridged, or None