  CONFIGURATION EDITOR
  LAN PORT

# Ethernet Port

Default Gateways

Frame Format

IP Frame Format

IP Parameters

MAC Address

NAU Name

NAU Name

  The Network Accessible Unit (NAU) name is optional. It enables you to assign a name to the port. Each NAU name must be unique to the unit.
  Range: Up to 8 characters (A-Z, 0-9, @, #, or $)

Frame Format

  This option must reflect the frame format used on the LAN.
  Some units enable you to set this parameter via a hardware switch.
  Range: 802.3

MAC Address

  This parameter defines the LAN port's MAC address. You may use the burned-in address, however, it is not recommended if the unit is configured to answer calls.
  Configuring your own MAC address enables you to swap the unit in the event of a failure without having to reconfigure downstream devices with the new destination MAC address.
  Range: 400000000001 -- 7FFFFFFFFFFF

IP Frame Format

  The frame format for IP management traffic may be different than that used for LLC2 traffic. This option defines the format to use for IP management frames.
  Range: Version 2 or IEEE 802.3

IP Parameters

  If you are using SNMP or IP management, you must configure the IP parameters for each required interface.

Default Gateways

  This feature enables you to define one or more default gateway.