  Customize

# Customize LLC2

Select a topic for further information:

Broadcast Test Timeout

Broadcast Type

LLC Enabled

LLC Support

Local Test Timeout

Send Local Test

Single Route, All Return

Single Route, Single Return

T1

LLC Support

  This management program does not support LLC management. However, on Windows 95 platforms, it continues to support the LLC Connect-by-address application. Connect by Address can be used to contact Access products that cannot currently be reached via IP. The purpose of this facility is to allow you to correct or set the IP address so the unit can be managed via IP.
  Note: The Probe family of products do not support LLC.

LLC Enabled

  Enable this feature if you intend to manage units via LLC2.
  Range: Enabled or Disabled

Send Local Test

  Enable this feature if there are units on the local ring. If disabled, the program will not attempt to locate local units.
  Range: Enabled or Disabled

Local Test Timeout

  This field defines the number of seconds the management workstation must wait before expecting a response to a local test frame
  Range: 1 -- 20 seconds

Broadcast Type

  Causes the management workstation to transmit signals to a remote unit over all possible broadcast routes. The remote unit then responds with a non-broadcast (source-routed) frame. The broadcast type determines how the management workstation finds the best possible route as follows:
  Range: All Routes

Single Route, All Return

  Causes the management workstation to transmit signals to a remote unit over a single route. The remote unit then responds with an all-routes broadcast. The route listed in the first response is the route used for the session.

Single Route, Single Return

  Causes the management workstation to transmit signals to a remote unit over a single route. The remote unit then responds with a non-broadcast (source-routed) frame.

Broadcast Test Timeout

  This field defines the number of seconds the management workstation must wait before expecting a response from a broadcast test frame.
  Range: 1 -- 20 seconds

T1

  This field helps tune performance by setting the number of seconds the management workstation waits for an LLC2 response before entering a recover-retry sequence.
  Range: 1 -- 10 seconds