# Status Colors

White

  The unit is not being monitored

Green (Normal)

  The unit has been contacted, its ports are enabled, and its PUs are active (in session)

Mustard(Marginal)

  Line quality is marginal Line is in the "Ready to Re-Home" state. When a dial backup trigger event occurs, the session is automatically switched to the dial-backup connection. Once the trigger event clears, the "Ready to Re-Home" state is initiated, indicating that it is safe to home the backup port.

Yellow (Minor)

  The unit has not responded to the last poll (Out of contact~short), a port or PU has failed

Dark Red (Major)

  A PU is not in session (inactive)

Red (Critical)

  The unit has not responded to repeated session initiation attempts from the management console Out of contact~long)

Gray (Unknown)

  The unit or PU has never responded to a poll from the management console.

Blue (Disabled)

  The port or PU is disabled by the operator

Magenta (Informational)

  A configured NetView PU is not in session A dump file exists on the unit The software version in the unit's configuration does not match the software version currently loaded on the device. The unit's Configuration ID, in the database, does not match the CID of the currently-loaded configuration. To correct this problem, enter the configuration editor and reinstall the configuration onto the unit.