  CONFIGURATION EDITOR
  BRIDGING

# Bridged SNA/LLC2 Traffic Priorities

Default Priority

  If you intend to use one priority for most of the sessions, you may set this field to that priority. The priority you select becomes the default for each session you add in the Per-Session Priority Overrides List.
  Range: Low, Medium, High, or Urgent

Per-Session Priority Overrides

  Click on the Add button to define an SNA/LLC2 session priority.
  Each session relies on a MAC and SAP pair to establish a connection between the source and destination device.
  MAC Address 1 and SAP 1 represent one end of the connection, while MAC Address 2 and SAP 2 represent the other end of the connection.
  If the default priority for a session is not acceptable, select another priority from the override's priority list.
  Range: MAC Address:
  Token Ring: 000000000001 -- 7FFFFFFFFFFF
  Ethernet: 020000000000 -- FFFFFFFFFFFF
  SAP: 04 -- F8 in increments of 4
  Priority: Low, Medium, High, or Urgent