# Unit Detail

# Unit Monitoring

# Displaying Status Information

#### DLCI

#### DLCI Status

#### Done

#### Port

#### Port Status

#### Statistics

#### Status Information

#### Displaying Status Information

  The DLCI Status window, associated with an individual DLCI, provides the user with the connection status of the DLCI.
  To open a DLCI Status window:
  1 Make sure that the Unit Detail window's DLCIs tab has been clicked.
  2 Position the mouse arrow over the DLCI entry, listed in the Unit Detail window's DLCIs tab, whose status you wish to view, and click the right mouse button.
  3 Select Status Information...from the list of pull-down menu options.
  This action will cause a window, corresponding to your DLCI selection, to be displayed.
  The fields and buttons contained within each DLCI Status window are described in the following paragraphs.
  Port - Identifies the interface port (DTE) or (NET) off from which the DLCI is seen.
  DLCI- Identifies the number of the DLCI whose status you are viewing.
  DLCI Status - Identifies the current status of the DLCI (e.g., Active or Inactive).
  Status Information - A textual description of the DLCI's current status (e.g., The DLCI is active).
  Statistics... - Clicking this button will open the DLCI Statistics window of the DLCI whose status is currently being viewed. For additional information about this window, refer to "Displaying Throughput Statistics
  Port Status... - Clicking this button will open the Port Statistics window which corresponds to the interface (DTE or Network) off from which the DLCI is seen. For additional information about this window, refer to "Displaying DTE Status Information," page B-4 and "Displaying Network Status Information
  Done - Clicking this button will close the DLCI Status window.