  CONFIGURATION EDITOR
  IPX ROUTING

# Transmit / Receive SAPs For IPX Routing

  These values override any configured IPX SAP filters by virtual port.
  To add an entry to this list, click on the Add button. The IPX SAP Transmit/Receive Override edit window will display.
  To delete an existing entry, click inside any field within the row you want to delete, then click on the Delete button.
  To edit an existing entry, click inside any field within the row you want to edit, then click on the Modify button.