  CONFIGURATION EDITOR
  BURST CONTROL

# Burst Control Virtual-Port Specific Overrides

  To add an entry, click on the Add button.
  To delete an entry, select the entry you want to delete, then click on the Delete button.

Committed Burst Size

DLCI

Excess Burst Size

Port

Port

  Click on this field to select the port for which you want to define an override.
  Range: 1 -- 8

DLCI

  Enter the DLCI for the selected port.
  Range: 16 -- 1023

Committed Burst Size

  This value defines the maximum number of bits, during time interval (Tc), the network agrees to accept under normal conditions. This value depends upon the Measurement Period (Tc) and the line speed. It must match the configured value (Bc) for the network, and must not be greater than the configured line speed.
  Range: 1 -- 2048 Kbps

Excess Burst Size

  This value defines the maximum number of uncommitted bits, during time interval (Tc), the network accepts above the committed burst size (Bc). It cannot be greater than the configured line speed.
  Range: 0 -- 2048 Kbps