# Overview

  This management software enables you to configure, monitor, and manage supported units connected to the LAN or WAN.
  The management workstation can connect to its supported units across the Local Area Network (LAN) or Wide Area Network (WAN).
  Managed units are located via the Media Access Control (MAC) address or Internal Protocol (IP) address. By default, Conversion devices have a MAC address assigned to their LAN port, and Frame Relay access devices have a MAC address assigned to their internal ring.