#

# EDITOR HOME

# DTE PORT

# FRAP 3.0 DTE Port

#### Clocking Mode

#### DCD, DSR, and CTS Signal Generator

#### Timing

#### Clocking Mode

  This field defines the DTE clocking mode. Most applications do not require inverting the DTE clock, but occasionally, shifting the DTE clock 180 degrees will solve out-of-phase timing problems on the DTE link.
  Range: Normal or Inverted

#### Timing

  Timing may be looped internally from the unit (Loop 2), or externally from the DTE device (Loop 1). If a problem with DTE timing occurs or if you are uncertain which to use, configure the unit for Loop-2 timing.
  Range: Loop-1 or Loop-2

#### DCD, DSR, and CTS Signal Generator

  This field defines the source for the DCD, DSR, or CTS signal on the line.
  Range: The following is a list of available ranges:
  1. Always On
  2. Always Off
  3. Follow Carrier
  4. Off During Testing
  5. Follow RTS
  6. Follow Carrier & RTS