  CONFIGURATION EDITOR
  IPX ROUTING

# IPX SAP Transmit/Receive Override

Port

  This is the port for which you want to define an override. Click inside this field to select a port from the list.
  Range: LAN or 1 -- 8

DLCI

  This DLCI number must match the one assigned to the virtual port. If you are connecting two FRADs back-to-back, use DLCI number 32.
  Range: 16 -- 1023

Transmit/Receive SAP Packets

  This field defines whether or not the unit will transmit SAP packets and/or process received RIP packets.
  Range: Transmit, Receive, Both, or Neither

Servers

  This option box enables you to specify the method by which the selected virtual port interfaces with a Novell server.
  To control service from a specific network address, number, or both network address and number, click the appropriate radio button and enter the necessary values in a series of 0s or Fs.