  CONFIGURATION EDITOR
  FILTERING

# Source MAC Address Filtering

  Note: Depending upon your product type, this dialog may vary. This help context covers all possible configuration parameters. If your dialog does not contain certain parameters, they don't apply to the product you are configuring.

Filter Out Frames with Source MAC Address

  Click on the Add button, then enter the MAC address of the source device whose packets you want the unit to filter.
  Range: Any MAC address on the network
  This field accepts wild cards, so you can specify a range of MAC addresses. For example:
  404????????? filters all addresses beginning with 404.
  404?????951 filters all addresses beginning with 404 and ending with 951.
  ???579?????? filters all addresses with 579 in the fourth, fifth, and sixth position.