# Unit Detail

# Unit Monitoring

# Displaying DTE Port Statistic

#### Displaying DTE Port Statistics

#### DTE Port Statistics

#### Port Statistics

#### Displaying DTE Port Statistics

  The DTE Port Statistics window provides the user with physical Layer 2 Throughput statistics collected on the DTE interface.
  To open the DTE Port Statistics window:
  1. Position the mouse arrow over the Unit Detail window's graphical representation of the DTE port, and click the right mouse button.
  2. Select Port Statistics... from the list of pull-down menu options and click the left mouse button.
  Note: The DTE statistics window can also be opened from the DTE Port Status window. After opening the status window click on the Statistics... button. For information about the DTE Port Status window, refer to "Displaying DTE Status Information The fields and buttons contained within the DTE Port Statistics window are described in the following paragraphs. The value displayed in parentheses represents the difference (delta) between values obtained during the previous polling interval and the current interval.
  The number in the upper right-hand corner is a countdown for the remaining seconds before the next poll cycle begins.
  Port Statistics - Identifies Layer 2 Throughout statistics collected on High-level Data Link Control (HDLC) frames passing through the DTE interface port. These statistics are described in Table B-1.
  DTE Port Statistics
  In Octets ~ The number of octets (bytes) which have been received on the DTE interface.
  Out Octets ~ The number of octets (bytes) which have been transmitted on the DTE interface.
  In Frames ~ The number of frames which have been received on the DTE interface.
  Out Frames ~ The number of frames which have been transmitted on the DTE interface.
  In CRC Errors ~ The number of frames which have been received on the DTE interface that contain Cyclic Redundancy Check (CRC) errors. The unit can be configured to either discard or pass through CRC errored frames..
  In Aborts ~ The number of frames which have been received on the DTE interface that have been marked with an abort sequence (indicates that the frames were incomplete).contain Cyclic Redundancy Check (CRC) errors. The unit can be configured to either discard or pass through CRC errored frames..
  Stop/Start - Clicking this button stops and starts the statistics polling action.
  Update - Clicking this button will update (refresh) the counts of each DTE interface statistic.
  Done - Clicking this button will close the DTE Port Statistics window.