  CONFIGURATION EDITOR
  BURST CONTROL

# Burst Control Values For Configured Ports

Port

  All configured frame relay ports are automatically displayed.

Committed Burst Size

  This value defines the maximum number of bits, during time interval (Tc), the network agrees to accept under normal conditions. This value depends upon the Measurement Period (Tc) and the line speed. It must match the configured value (Bc) for the network, and must not be greater than the configured line speed.
  Range: 1 -- 2048 Kbps

Excess Burst Size

  This value defines the maximum number of uncommitted bits, during time interval (Tc), the network accepts above the committed burst size (Bc). It cannot be greater than the configured line speed.
  Range: 0 -- 2048 Kbps