  Customize

# Customize Session Tuning

  These parameters define how many sessions can be managed at a given time. These values may only be altered for LLC2 sessions.
  Note: The sum of the following values must be equal to or less than 240, or the LAN adapter will have problems connecting to the network.

Maximum Number of Monitor Sessions

  This value defines the maximum number of units that can be monitored at a given time.
  Range: 1 -- 200 sessions

Maximum Number of Configuration Sessions

  This value defines the maximum number of configuration sessions that can occur at a given time.
  Range: 1 -- 20 sessions

Maximum Number of NMS Sessions

  This value defines the maximum number of NMS sessions that can occur at a given time.
  Range: 1 -- 20 sessions