  CONFIGURATION EDITOR
  IP REDIRECTION WITHOUT RIP

# IP Routing Summary

  If you have several nodes on several networks, broadcasting each node address over the network can impact performance.
  When enabled, the summary feature only broadcasts the network class address associated with the broadcasting router.

Values for Configured LAN and Frame Relay Ports

  If the summary is set to NO, RIP will broadcast subnet information as it is defined in the routing table.
  Range: Yes or No