  CONFIGURATION EDITOR

# SNMP

Access

Enable Traps

Manager IP Address

Name

Use SNMP

  Note: Up to two SNMP managers may be defined.

Use SNMP

  Select the feature if you intend to use SNMP management.
  Range: Enabled or Disabled

Name

  A community is the relationship between an SNMP agent and one or more SNMP managers. A community name identifies this agent-to-manager relationship and is included in each SNMP request and response.
  The agent and manager's community name must be identical or transactions will not occur.
  Range: 40 alphanumeric characters

Manager IP Address

  This field reflects the IP address of the SNMP manager.
  The SNMP manager identified by this address receives unsolicited alarms if traps are enabled. If you have enabled traps, you must define this address.
  Range: 4 numbers (0--255) separated by three periods

Enable Traps

  Enable this option if you want traps sent to the manager identified by the manager IP address.
  Range: Enabled or Disabled

Access

  This parameter defines the access level the community members have within the community.
  Range: None, Read/Write, Read Only, or Super User
  Read/Write enables the user to modify MIB variables.
  Super User enables the user to modify MIB variables and community parameters.